{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["20191223_基ポリマー（プラスチック）（整理番号付与）"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"20191223_基ポリマー（プラスチック）（整理番号付与）","index":0,"n_rows":1278,"n_cols":16,"rows_kept":1278,"cut":false,"hidden":false,"merged":[[1269,5,1270,5],[861,5,862,5],[964,5,965,5],[1084,5,1085,5],[1089,5,1090,5],[1084,13,1085,13],[1089,13,1090,13],[861,7,862,7],[964,7,965,7],[1084,7,1085,7],[1089,7,1090,7],[1261,5,1262,5],[1084,14,1085,14],[523,15,524,15],[964,15,965,15],[1084,15,1085,15],[718,14,719,14],[723,14,724,14],[1261,14,1262,14],[1269,14,1270,14],[1269,7,1270,7],[1261,7,1262,7],[1261,8,1261,12],[1269,8,1269,12],[1269,15,1270,15],[536,15,537,15],[700,15,701,15],[710,15,711,15],[718,15,719,15],[733,15,734,15],[826,15,827,15],[861,15,862,15],[1261,13,1262,13],[1269,13,1270,13],[723,7,724,7],[728,7,729,7],[475,15,476,15],[354,15,355,15],[380,15,381,15],[397,15,398,15],[402,15,403,15],[407,15,408,15],[435,15,436,15],[1089,15,1090,15],[1261,15,1262,15],[482,15,483,15],[493,15,494,15],[499,15,500,15],[505,15,506,15],[512,15,513,15],[518,15,519,15],[531,15,532,15],[723,15,724,15],[728,15,729,15],[290,15,291,15],[295,15,296,15],[303,15,304,15],[308,15,309,15],[444,15,445,15],[449,15,450,15],[454,15,455,15],[463,15,464,15],[469,15,470,15],[454,14,455,14],[463,14,464,14],[6,15,7,15],[21,15,22,15],[28,15,29,15],[37,15,38,15],[42,15,43,15],[48,15,49,15],[53,15,54,15],[73,15,74,15],[78,15,79,15],[60,15,61,15],[68,15,69,15],[313,15,314,15],[324,15,325,15],[329,15,330,15],[337,15,338,15],[121,15,122,15],[128,15,129,15],[133,15,134,15],[83,15,84,15],[90,15,91,15],[103,15,104,15],[114,15,115,15],[469,13,470,13],[475,13,476,13],[138,15,139,15],[143,15,144,15],[469,14,470,14],[475,14,476,14],[160,14,161,14],[171,14,172,14],[190,14,191,14],[201,14,202,14],[215,13,216,13],[249,13,250,13],[343,15,344,15],[348,15,349,15],[249,14,250,14],[160,15,161,15],[171,15,172,15],[190,15,191,15],[201,15,202,15],[215,15,216,15],[249,15,250,15],[303,14,304,14],[308,14,309,14],[313,14,314,14],[114,14,115,14],[121,14,122,14],[128,14,129,14],[215,14,216,14],[121,13,122,13],[128,13,129,13],[6,14,7,14],[21,14,22,14],[28,14,29,14],[37,14,38,14],[42,14,43,14],[48,14,49,14],[53,14,54,14],[60,14,61,14],[68,14,69,14],[73,14,74,14],[78,14,79,14],[83,14,84,14],[90,14,91,14],[103,14,104,14],[380,14,381,14],[290,14,291,14],[295,14,296,14],[397,14,398,14],[402,14,403,14],[407,14,408,14],[449,13,450,13],[449,14,450,14],[324,14,325,14],[329,14,330,14],[337,14,338,14],[343,14,344,14],[348,14,349,14],[354,14,355,14],[329,13,330,13],[337,13,338,13],[343,13,344,13],[407,13,408,13],[435,13,436,13],[435,14,436,14],[444,14,445,14],[324,13,325,13],[733,7,734,7],[133,14,134,14],[138,14,139,14],[143,14,144,14],[454,13,455,13],[463,13,464,13],[133,13,134,13],[138,13,139,13],[531,7,532,7],[536,7,537,7],[700,7,701,7],[710,7,711,7],[718,7,719,7],[499,13,500,13],[505,13,506,13],[512,13,513,13],[348,13,349,13],[354,13,355,13],[380,13,381,13],[397,13,398,13],[402,13,403,13],[444,13,445,13],[435,7,436,7],[523,7,524,7],[826,7,827,7],[444,7,445,7],[449,7,450,7],[454,7,455,7],[295,7,296,7],[303,7,304,7],[308,7,309,7],[313,7,314,7],[42,13,43,13],[48,13,49,13],[53,13,54,13],[60,13,61,13],[68,13,69,13],[201,13,202,13],[143,13,144,13],[160,13,161,13],[171,13,172,13],[190,13,191,13],[512,7,513,7],[518,7,519,7],[354,7,355,7],[380,7,381,7],[397,7,398,7],[402,7,403,7],[463,7,464,7],[469,7,470,7],[475,7,476,7],[482,7,483,7],[493,7,494,7],[499,7,500,7],[505,7,506,7],[249,7,250,7],[283,7,284,7],[290,7,291,7],[324,7,325,7],[329,7,330,7],[337,7,338,7],[343,7,344,7],[348,7,349,7],[407,7,408,7],[90,13,91,13],[103,13,104,13],[114,13,115,13],[290,13,291,13],[295,13,296,13],[303,13,304,13],[308,13,309,13],[313,13,314,13],[402,8,402,12],[313,8,313,12],[324,8,324,12],[103,3,104,3],[114,3,115,3],[121,3,122,3],[128,3,129,3],[103,8,103,12],[114,8,114,12],[121,8,121,12],[128,8,128,12],[133,8,133,12],[171,8,171,12],[90,5,91,5],[103,5,104,5],[114,5,115,5],[114,7,115,7],[121,7,122,7],[128,7,129,7],[133,7,134,7],[138,7,139,7],[723,5,724,5],[728,5,729,5],[733,5,734,5],[826,5,827,5],[469,5,470,5],[475,5,476,5],[482,5,483,5],[493,5,494,5],[499,5,500,5],[710,5,711,5],[536,5,537,5],[700,5,701,5],[531,5,532,5],[505,5,506,5],[512,5,513,5],[518,5,519,5],[523,5,524,5],[397,3,398,3],[402,3,403,3],[407,3,408,3],[329,3,330,3],[337,3,338,3],[343,3,344,3],[444,8,444,12],[354,8,354,12],[718,5,719,5],[449,5,450,5],[454,5,455,5],[463,5,464,5],[329,5,330,5],[380,5,381,5],[337,5,338,5],[343,5,344,5],[449,8,449,12],[454,8,454,12],[463,8,463,12],[469,8,469,12],[475,8,475,12],[380,8,380,12],[397,8,397,12],[407,8,407,12],[397,5,398,5],[402,5,403,5],[407,5,408,5],[435,5,436,5],[444,5,445,5],[348,5,349,5],[354,5,355,5],[215,8,215,12],[249,8,249,12],[283,8,283,12],[290,5,291,5],[295,5,296,5],[303,5,304,5],[308,5,309,5],[313,5,314,5],[324,5,325,5],[435,8,435,12],[171,5,172,5],[53,5,54,5],[215,7,216,7],[249,5,250,5],[283,5,284,5],[173,2,173,15],[180,2,180,15],[190,8,190,12],[201,8,201,12],[283,13,284,13],[215,3,216,3],[249,3,250,3],[283,3,284,3],[283,14,284,14],[283,15,284,15],[190,5,191,5],[201,5,202,5],[215,5,216,5],[143,7,144,7],[160,7,161,7],[171,7,172,7],[190,7,191,7],[201,7,202,7],[170,2,170,15],[964,3,965,3],[1084,3,1085,3],[1089,3,1090,3],[1261,3,1262,3],[1269,3,1270,3],[21,5,22,5],[28,5,29,5],[37,5,38,5],[42,5,43,5],[48,5,49,5],[718,3,719,3],[723,3,724,3],[728,3,729,3],[733,3,734,3],[826,3,827,3],[861,3,862,3],[518,3,519,3],[523,3,524,3],[531,3,532,3],[536,3,537,3],[700,3,701,3],[710,3,711,3],[475,3,476,3],[482,3,483,3],[482,2,483,2],[493,2,494,2],[499,2,500,2],[700,2,701,2],[710,2,711,2],[518,2,519,2],[444,3,445,3],[449,3,450,3],[454,3,455,3],[463,3,464,3],[469,3,470,3],[190,3,191,3],[201,3,202,3],[493,3,494,3],[499,3,500,3],[505,3,506,3],[512,3,513,3],[435,3,436,3],[60,3,61,3],[68,3,69,3],[73,3,74,3],[78,3,79,3],[83,3,84,3],[90,3,91,3],[143,3,144,3],[160,3,161,3],[295,3,296,3],[303,3,304,3],[308,3,309,3],[313,3,314,3],[324,3,325,3],[290,3,291,3],[348,3,349,3],[354,3,355,3],[380,3,381,3],[1261,2,1262,2],[1089,1,1090,2],[512,2,513,2],[348,2,349,2],[354,2,355,2],[380,2,381,2],[397,2,398,2],[402,2,403,2],[407,2,408,2],[435,2,436,2],[444,2,445,2],[449,2,450,2],[505,2,506,2],[1091,1,1091,2],[1092,1,1092,3],[1159,1,1159,3],[1183,1,1183,5],[1221,1,1225,1],[718,2,719,2],[723,2,724,2],[454,2,455,2],[463,2,464,2],[469,2,470,2],[475,2,476,2],[728,2,729,2],[523,2,524,2],[531,2,532,2],[536,2,537,2],[678,2,697,2],[290,2,291,2],[295,2,296,2],[303,2,304,2],[42,2,43,2],[48,2,49,2],[53,2,54,2],[60,2,61,2],[68,2,69,2],[73,2,74,2],[143,2,144,2],[160,2,161,2],[171,2,172,2],[190,2,191,2],[201,2,202,2],[215,2,216,2],[249,2,250,2],[283,2,284,2],[103,2,104,2],[114,2,115,2],[728,14,729,14],[718,8,718,12],[723,8,723,12],[1269,2,1270,2],[733,14,734,14],[826,14,827,14],[861,14,862,14],[964,14,965,14],[1084,8,1084,12],[1089,8,1089,12],[1089,14,1090,14],[828,8,828,14],[847,8,847,14],[861,8,861,12],[929,8,929,14],[964,8,964,12],[966,8,966,14],[861,13,862,13],[964,13,965,13],[733,2,734,2],[826,2,827,2],[861,2,862,2],[964,2,965,2],[1084,2,1085,2],[718,13,719,13],[723,13,724,13],[523,8,523,12],[531,8,531,12],[536,8,536,12],[728,8,728,12],[733,8,733,12],[826,8,826,12],[728,13,729,13],[733,13,734,13],[826,13,827,13],[700,8,700,12],[710,8,710,12],[523,13,524,13],[531,14,532,14],[536,14,537,14],[700,14,701,14],[710,14,711,14],[482,8,482,12],[493,8,493,12],[499,8,499,12],[505,8,505,12],[512,8,512,12],[518,8,518,12],[531,13,532,13],[536,13,537,13],[700,13,701,13],[710,13,711,13],[493,13,494,13],[482,14,483,14],[493,14,494,14],[499,14,500,14],[512,14,513,14],[505,14,506,14],[482,13,483,13],[518,14,519,14],[523,14,524,14],[518,13,519,13],[329,8,329,12],[337,8,337,12],[343,8,343,12],[348,8,348,12],[290,8,290,12],[295,8,295,12],[303,8,303,12],[308,8,308,12],[308,2,309,2],[343,2,344,2],[313,2,314,2],[324,2,325,2],[329,2,330,2],[337,2,338,2],[159,2,159,15],[160,8,160,12],[171,3,172,3],[83,8,83,12],[90,8,90,12],[160,5,161,5],[42,7,43,7],[48,7,49,7],[53,7,54,7],[60,7,61,7],[68,7,69,7],[73,7,74,7],[78,7,79,7],[48,8,48,12],[53,8,53,12],[60,8,60,12],[68,8,68,12],[73,8,73,12],[78,8,78,12],[60,5,61,5],[68,5,69,5],[73,5,74,5],[42,3,43,3],[48,3,49,3],[3,8,3,15],[0,1,0,15],[133,3,134,3],[138,3,139,3],[133,5,134,5],[138,5,139,5],[1,2,1,11],[2,2,2,11],[6,2,7,2],[21,2,22,2],[28,2,29,2],[37,2,38,2],[78,2,79,2],[83,2,84,2],[90,2,91,2],[138,8,138,12],[21,3,22,3],[28,3,29,3],[37,3,38,3],[53,3,54,3],[121,2,122,2],[128,2,129,2],[133,2,134,2],[138,2,139,2],[143,5,144,5],[42,8,42,12],[21,7,22,7],[28,7,29,7],[37,7,38,7],[6,13,7,13],[21,13,22,13],[28,13,29,13],[37,13,38,13],[6,8,6,12],[21,8,21,12],[28,8,28,12],[37,8,37,12],[78,5,79,5],[83,5,84,5],[83,7,84,7],[90,7,91,7],[103,7,104,7],[143,8,143,12],[121,5,122,5],[128,5,129,5],[73,13,74,13],[78,13,79,13],[83,13,84,13],[133,0,134,0],[6,0,7,0],[21,0,22,0],[28,0,29,0],[42,0,43,0],[37,0,38,0],[48,0,49,0],[53,0,54,0],[60,0,61,0],[68,0,69,0],[73,0,74,0],[78,0,79,0],[83,0,84,0],[90,0,91,0],[103,0,104,0],[114,0,115,0],[121,0,122,0],[128,0,129,0],[329,0,330,0],[337,0,338,0],[343,0,344,0],[138,0,139,0],[143,0,144,0],[160,0,161,0],[171,0,172,0],[190,0,191,0],[201,0,202,0],[215,0,216,0],[290,0,291,0],[295,0,296,0],[303,0,304,0],[308,0,309,0],[313,0,314,0],[324,0,325,0],[249,0,250,0],[283,0,284,0],[499,0,500,0],[505,0,506,0],[512,0,513,0],[348,0,349,0],[354,0,355,0],[380,0,381,0],[397,0,398,0],[402,0,403,0],[407,0,408,0],[435,0,436,0],[444,0,445,0],[449,0,450,0],[1261,0,1262,0],[1269,0,1270,0],[3,3,3,7],[518,0,519,0],[523,0,524,0],[531,0,532,0],[536,0,537,0],[700,0,701,0],[710,0,711,0],[718,0,719,0],[733,0,734,0],[826,0,827,0],[861,0,862,0],[964,0,965,0],[1084,0,1085,0],[1089,0,1090,0],[723,0,724,0],[728,0,729,0],[454,0,455,0],[463,0,464,0],[469,0,470,0],[475,0,476,0],[482,0,483,0],[493,0,494,0]]}
[null,"※2019年12月23日時点"]
[null,null,"別表第１　第１表案（基ポリマー）（１）基ポリマー（プラスチック）"]
[]
[null,null,null,"a　表中使用可能食品の欄は、次に定めるとおりとする。\n① 「○」は、使用可能であることを示す。\n② 「－」は、使用不可であることを示す。\nb　表中使用可能最高温度の欄は、次に定めるとおりとする。\n① 「Ⅰ」は、70℃以下で使用可能であることを示す。\n② 「Ⅱ」は、100℃以下で使用可能であることを示す。\n③ 「Ⅲ」は、100℃超で使用可能であることを示す。\n\n特記事項欄における「＃」の記号等は記載されていない。\n（「＃」は食品安全基本法第１１条第１項第３項に該当するものであることを示す予定）",null,null,null,null,"※　今後、物質名称の追加・変更、物質の統合、CAS登録番号の追加・変更、記載順の変更等、\n　　整備を行う予定である。\n\n※　2019年８月９日時点のポジティブリスト案からの変更箇所が着色されて表示されている。"]
[]
[null,null,"１．ポリエチレン（PE）"]
["整理番号",null,"No","使用可能ポリマー","和名20200120","英名","英名20200120","CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[985,null,1,"エチレン単独重合体",null,"Ethylene, homopolymer",null,"9002-88-4","○","○","○","○","○","Ⅲ",5]
[982,null,2,"エチレン・１－アルケン共重合体",null,"Copolymers of ethylene and 1-alken",null,"9010-79-1\n25087-34-7\n25213-02-9\n25213-96-1\n25895-47-0\n26221-73-8\n25895-46-9\n60785-11-7\n28829-58-5\n等","○","○","○","○","○","Ⅲ",5]
[991,null,3,"エチレン単独重合体・無水マレイン酸グラフト化物",null,"Ethylene, homopolymer and 2,5-furandione, graft",null,"9006-26-2\n106343-08-2","〇","〇","○","〇","〇","Ⅲ",2]
[990,null,4,"エチレン・１－アルケン共重合体・無水マレイン酸グラフト化物",null,"1-Alkene, polymer with ethylene and 2,5-furandione, graft　　　　　　　　　　　　　　　　　　　　　　　　　　",null,"31069-12-2\n63625-36-5\n86286-09-1\n85244-45-7\n108388-93-8\n等","〇","〇","○","〇","〇","Ⅲ",2]
[989,null,5,"エチレン単独重合体・マレイン酸モノエチルエステルグラフト化物",null,"Ethylene homopolymer, maleic anhydride monoethyl ester grafted",null,"59975-36-9","○","○","ー","○","○","Ⅲ",2]
[986,null,6,"エチレン単独重合体・スチレングラフト化物",null,"Benzen, ethenyl-, polymer with ethene, graft",null,"106826-12-4","○","○","○","○","○","Ⅲ",2]
[988,null,7,"エチレン単独重合体・エテニルトリメトキシシラングラフト化物及びその架橋体",null,"Ethenyltrimethoxysilane-grafted polyethylene",null,"35312-82-4\n107257-99-8　","〇","〇","○","〇","〇","Ⅲ",2,"エテニルトリメトキシシラン（CAS登録番号2768-02-7）はポリマー構成成分に対して２重量％未満。"]
[987,null,8,"エチレン・１－アルケン共重合体・エテニルトリメトキシシラン\nグラフト化物及びその架橋体",null,"Ethenyltrimethoxysilane-grafted ethylene 1-alken  copolymer",null,"107240-66-4\n113883-62-8\n108388-96-1\n107709-77-3","〇","〇","○","〇","〇","Ⅲ",2,"エテニルトリメトキシシラン（CAS登録番号2768-02-7）はポリマー構成成分に対して２重量％未満。\n１－アルケンはプロピレン（CAS登録番号115-07-1）、１－ブテン（CAS登録番号106-98-9）、１－ヘキセン（CAS登録番号592-41-6）、１－オクテン（CAS登録番号111-66-0）のうち１種類使用可能。"]
[984,null,9,"エチレン・スチレン共重合体（ポリスチレングラフト重合体を含む）","エチレン・スチレン共重合体（ポリスチレンでグラフト化された重合体を含む）","Benzene, ethenyl-, polymer with ethene",null,"0025068-12-6","〇","〇","○","〇","〇","III",2,"エチレンはポリマー構成成分に対して50重量%以上。"]
[983,null,10,"エチレン・プロピレン・5－エチリデン－2－ノルボルネン共重合体","2-エチリデン-5-ノルボルネン・エチレン・プロピレン共重合体","Ethene, terpolymer with 1-​propene and 5-Ethylidene-2-norbornene",null,"0025038-36-2","○","ー","ー","○","○","III",2]
[992,null,11,"エチレン単独重合体・メタクリル酸グリシジルグラフト化物","メタクリル酸 グリシジルでグラフト化されたエチレン単独重合体","Ethylene homopolymer, Glycidyl methacrylate, grafted",null,"0026061-90-5","ー","ー","ー","ー","○","Ⅰ",5]
[]
[null,null,"２．エチレン・酢酸ビニル共重合体（EVA）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[84,null,1,"エチレン・酢酸ビニル共重合体",null,"Ethene, polymer with ethenyl acetate",null,"24937-78-8","〇","〇","〇","〇","〇","III",2]
[85,null,2,"エチレン・酢酸ビニル共重合体・無水マレイン酸グラフト化物",null,"Ethene, copolymer with vinyl acetate, maleic anhydride grafted ",null,"28064-24-6","○","○","ー","○","○","III",2]
[83,null,3,"エチレン・酢酸ビニル・一酸化炭素共重合体",null,"Ethene, terpolymer with vinyl acetate and carbon monoxide ",null,"26337-35-9","○","○","ー","○","○","III",2]
[]
[null,null,"３．エチレン・ビニルアルコール共重合体（EVOH）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[96,null,1,"エチレン・酢酸ビニル共重合体完全ケン化物／エチレン・酢酸ビニル共重合体部分ケン化物\n（エチレン・ビニルアルコール共重合体／エチレン・酢酸ビニル・ビニルアルコール共重合体）",null,"Completely hydrolyzed copolymer of ethylene and vinyl acetate/\nPartially hydrolyzed polymer of ethylene and vinyl acetate",null,"25067-34-9\n26221-27-2","〇","〇","〇","〇","〇","Ⅲ",3]
[97,null,2,"エチレン・酢酸ビニル・３，４－ジアセトキシ－１－ブテン共重合体完全ケン化物／\nエチレン・酢酸ビニル・３，４－ジアセトキシ－１－ブテン共重合体部分ケン化物\n（エチレン・ビニルアルコール・３，４－ジアセトキシ－１－ブテン共重合体／エチレン・ビニルアルコール・酢酸ビニル・３，４－ジアセトキシ－１－ブテン共重合体）",null,"Completely hydrolyzed polymer of ethylene, vinyl acetate and 3,4-diacetoxy-1-butene／\nPartially hydrolyzed polymer of ethylene, vinyl acetate and 3,4-diacetoxy-1-butene",null,"917249-65-1","○","○","○","○","○","III",3,"ビニルアルコールはポリマー構成成分に対して50重量％以上。\nエチレンの共重合範囲は38mol％以下。\n３，４－ジアセトキシ－１－ブテンの共重合量は3.3mol％以下。"]
[98,null,3,"２－メチレンー１，３－プロパンジオール・エチレン・酢酸ビニル共重合体完全ケン化物／２－メチレンー１，３－プロパンジオール・エチレン・酢酸ビニル共重合体部分ケン化物\n（２－メチレンー１，３－プロパンジオール・エチレン・ビニルアルコール共重合体／２－メチレンー１，３－プロパンジオール・エチレン・酢酸ビニル・ビニルアルコール共重合体）",null,"Completely hydrolyzed polymer of 2-Methylene-1,3-propanediol, ethylene and vinyl acetate／\nPartially hydrolyzed polymer of 2-Methylene-1,3-propanediol, ethylene and vinyl acetate",null,"1485481-35-3","〇","〇","〇","〇","〇","Ⅲ",3,"ビニルアルコールはポリマー構成成分に対して50重量％以上。"]
[99,null,4,"ビニルトリメトキシシラン変性エチレン・酢酸ビニル共重合体完全ケン化物／ビニルトリメトキシシラン変性エチレン・酢酸ビニル共重合体部分ケン化物\n（ビニルトリメトキシシラン変性エチレン・ビニルアルコール共重合体／ビニルトリメトキシシラン変性エチレン・酢酸ビニル・ビニルアルコール共重合体）",null,"Completely hydrolyzed polymer of　Vinyltrimethoxysilane modified ethylene and vinyl acetate／\nPartially hydrolyzed polymer of　Vinyltrimethoxysilane modified ethylene and vinyl acetate",null,"26221-27-2","〇","〇","○","〇","〇","Ⅲ",3,"ビニルアルコールはポリマー構成成分に対して50重量％以上。"]
[95,null,5,"1,2-エポキシプロパン変性エチレン・酢酸ビニル共重合体完全ケン化物／1,2-エポキシプロパン変性エチレン・酢酸ビニル共重合体部分ケン化物\n（1,2-エポキシプロパン変性エチレン・ビニルアルコール共重合体／1,2-エポキシプロパン変性エチレン・酢酸ビニル・ビニルアルコール共重合体）",null,"Completely hydrolyzed polymer of 1,2-epoxypropane modified ethylene and vinyl acetate／\nPartially hydrolyzed polymer of 1,2-epoxypropane modified ethylene and vinyl acetate",null,"482589-30-0","〇","〇","〇","〇","〇","Ⅲ",3,"ビニルアルコールはポリマー構成成分に対して50重量％以上。"]
[]
[null,null,"４．エチレン・アクリル酸共重合体（EAA）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[23,null,1,"エチレン・アクリル酸共重合体",null,"Polymer of acrylic acid / ethylene",null,"9010-77-9","〇","〇","〇","〇","〇","Ⅲ",2]
[]
[null,null,"５．エチレン・アクリル酸メチル共重合体（EMA）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[36,null,1,"エチレン・アクリル酸メチル共重合体",null,"2-Propenoic acid, methyl ester, polymer with ethene",null,"25103-74-6","〇","〇","〇","〇","〇","Ⅲ",2]
[37,null,2,"エチレン・アクリル酸メチル共重合体・無水マレイン酸グラフト化物",null,"Ethene, copolymer with Methyl 2-propenoate maleic anhydride grafted",null,"88450-35-5","○","○","ー","○","○","Ⅲ",2]
[]
[null,null,"６．エチレン・アクリル酸メチル・無水マレイン酸共重合体"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[42,null,1,"エチレン・アクリル酸メチル・無水マレイン酸共重合体",null,"Ethylene･methyl acrylate･maleic anhydride copolymer",null,"88450-35-5","〇","〇","〇","〇","〇","III",2]
[]
[null,null,"７．エチレン・アクリル酸エチル共重合体（EEA）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[16,null,1,"エチレン・アクリル酸エチル共重合体",null,"2-Propenoicacid, ethylester, polymer with ethene",null,"9010-86-0","〇","〇","〇","〇","〇","Ⅲ",2]
[17,null,2,"エチレン・アクリル酸エチル・無水マレイン酸共重合体","アクリル酸 エチル・エチレン・無水マレイン酸共重合体","Ethylene･ethyl acrylate･maleic anhydride terpolymer",null,"?4117114-6","〇","〇","〇","〇","〇","Ⅲ",2,"アクリル酸エチルはポリマー構成成分に対して10重量％未満"]
[18,null,3,"エチレン・アクリル酸エチル・無水マレイン酸共重合体","アクリル酸 エチル・エチレン・無水マレイン酸共重合体","Ethylene･ethyl acrylate･maleic anhydride terpolymer",null,"?4117114-6","〇","〇","〇","〇","〇","Ⅱ",2,"アクリル酸エチルはポリマー構成成分に対して10重量％以上"]
[]
[null,null,"８．エチレン・アクリル酸ブチル共重合体（EBA）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[29,null,1,"エチレン・アクリル酸ブチル共重合体",null,"Ethene copolymer with buthyl acrylate",null,"25750-84-9","○","○","ー","○","○","Ⅲ",2]
[28,null,2,"エチレン・アクリル酸ブチル・一酸化炭素共重合体",null,"Ethene,  terpolymer with butyl acrylate and carbon monoxide \n",null,"61843-70-7","○","○","ー","○","○","Ⅲ",2]
[31,null,3,"エチレン・アクリル酸ブチル・メタクリル酸共重合体",null,"Ethene, terpolymer with butyl acrylate and metacryl acid",null,"37433-35-5","○","○","ー","○","○","Ⅲ",2]
[30,null,4,"エチレン・アクリル酸ブチル・無水マレイン酸共重合体","アクリル酸 ブチル・エチレン・無水マレイン酸共重合体","Ethylene･butyl acrylate･maleic anhydride terpolymer",null,"0064652-60-4","〇","〇","〇","〇","〇","Ⅲ",2,"アクリル酸ブチルはポリマー構成成分に対して10重量%未満"]
[]
[null,null,"９．エチレン・メタクリル酸共重合体（EMAA）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[104,null,1,"エチレン・メタクリル酸共重合体",null,"Ethene, polymer with 2-Propenoic acid 2-methyl-",null,"25053-53-6","〇","〇","〇","〇","〇","III",2]
[]
[null,null,"１０．エチレン・メタクリル酸メチル共重合体（EMMA）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[114,null,1,"エチレン・メタクリル酸メチル共重合体",null,"Ethene, polymer with 2-Propenoic acid 2-methyl-, methyl ester",null,"25101-13-7 ","〇","〇","〇","〇","〇","III",2]
[]
[null,null,"１１．エチレン・メタクリル酸・イソブチルアクリレート共重合体（EMAAIBA）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[11,null,1,"エチレン・メタクリル酸・イソブチルアクリレート共重合体",null,"Polymer of ethylene, methacrylic acid, isobutyl acrylate",null,"37433-35-5","〇","〇","〇","〇","〇","III",2]
[]
[null,null,"１２．アイオノマー樹脂（ION）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[5,null,1,"エチレン・アクリル酸共重合体無機塩（Na, K, Zn）","アクリル酸・エチレン共重合体のナトリウム、カリウム、亜鉛塩","Ethene, copolymer with acrylic acid​ with salt (Na, K, Zn) ",null,"0027515-34-0\n0025750-82-7","〇","〇","ー","〇","〇","Ⅲ",3]
[6,null,2,"エチレン・メタクリル酸共重合体無機塩（Na, Mg, Zn, K）",null,"Ethylene, methacrylic acid coplymer with salts (Na, Mg, Zn, K)",null,"25608-26-8 75062-18-9 28516-43-0 26376-80-7","〇","〇","〇","〇","〇","Ⅲ",3]
[4,null,3,"エチレン・メタクリル酸・イソブチルアクリレート共重合体無機塩（Na, Mg, Zn, K）",null,"Ethylene, methacrylic acid, isobutyl acrylate coplymer with salts (Na, Mg, Zn, K)",null,"61615-65-4 96927-32-1 61843-71-8 93228-27-4","〇","〇","〇","〇","〇","Ⅲ",3]
[]
[null,null,"１３．ポリプロピレン（PP)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1219,null,1,"プロピレン単独重合体",null,"Propylene, homopolymer",null,"9003-07-0","○","○","○","○","○","Ⅲ",6]
[1216,null,2,"プロピレン・エチレン共重合体",null,"Coplymer of propylene and ethylene",null,"9010-79-1","○","○","○","○","○","Ⅲ",6]
[1214,null,3,"プロピレン・１－アルケン共重合体",null,"Coplymer of propylene and 1-alkene",null,"29160-13-2","○","○","○","○","○","Ⅲ",6]
[1213,null,4,"プロピレン・エチレン・１－アルケン共重合体",null,"Coplymer of propylene, ethylene and 1-alkene",null,"25895-47-0","○","○","○","○","○","Ⅲ",6]
[1221,null,5,"プロピレン単独重合体・無水マレイン酸グラフト化物",null,"Propylene homopolymer, maleic anhydride grafted",null,"25722-45-6","○","○","○","○","○","Ⅲ",6]
[1215,null,6,"プロピレン単独重合体・イソプレングラフト化物",null,"Propylene, homopolymer, isoprene grafted",null,"9003-07-0","〇","〇","〇","〇","〇","III",6,"イソプレン（CAS登録番号78-79-5）はポリマー構成成分に対して1.0重量％以下。\n101℃以上での使用は30分以内。"]
[1217,null,7,"プロピレン・エチレン共重合体・エテニルトリメトキシシラン\nグラフト化物及びその架橋体",null,"Ethenyltrimethoxysilane-grafted ethylene propylene  copolymer",null,"107240-66-4","〇","〇","〇","〇","〇","Ⅲ",2,"プロピレン・エチレン共重合体のプロピレンはポリマー構成成分に対して５０重量％以上。\nエテニルトリメトキシシラン（CAS登録番号2768-02-7）はポリマー構成成分に対して２重量％未満。"]
[1218,null,8,"プロピレン単独重合体・エテニルトリメトキシシラングラフト化物及びその架橋体",null,"Ethenyltrimethoxysilane-grafted polypropylene",null,"107240-65-3　","〇","〇","〇","〇","〇","Ⅲ",2,"エテニルトリメトキシシラン（CAS登録番号2768-02-7）はポリマー構成成分に対して２重量％未満。"]
[1220,null,9,"プロピレン・エチレン共重合体・無水マレイン酸グラフト化物","無水マレイン酸でグラフト化されたエチレン・プロピレン共重合体","2,5-Furandione, polymer with ethene and 1-propene",null,"0031069-12-2","○","○","○","○","○","　Ⅲ",2]
[]
[null,null,"１４．ポリビニールアルコール（PVA）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1152,null,1,"酢酸ビニル単独重合体完全ケン化物\n（ビニルアルコール単独重合体）","完全加水分解処理された酢酸 ビニル単独重合体","Completely hydrolyzed polyvinyl acetate",null,"0009002-89-5","○","○","○","○","○","II",3,"区分４の樹脂と混合（５％以下）する場合は使用可能温度はⅢ。\nポリスチレン又は区分２，３，４いずれかの樹脂と混合する場合は、混合する樹脂の使用制限を適用可能。"]
[1153,null,2,"酢酸ビニル単独重合体部分ケン化物\n（ビニルアルコール・酢酸ビニル共重合体）","部分加水分解処理された酢酸 ビニル単独重合体","Partially hydrolyzed polyvinyl acetate",null,"0025213-24-5","○","○","○","○","○","II",3,"区分４の樹脂と混合（５％以下）する場合は使用可能温度はⅢ。\nポリスチレン又は区分２，３，４いずれかの樹脂と混合する場合は、混合する樹脂の使用制限を適用可能。"]
[1149,null,3,"酢酸ビニル・３，４－ジアセトキシ－１－ブテン共重合体完全ケン化物／酢酸ビニル・３，４－ジアセトキシ－１－ブテン共重合体部分ケン化物\n（ビニルアルコール・３，４－ジアセトキシ－１－ブテン共重合体／ビニルアルコール・酢酸ビニル・３，４－ジアセトキシ－１－ブテン共重合体）",null,"Completely hydrolyzed copolymer of vinyl acetate and 3,4-diacetoxy-1-butene/\nPartially hydrolyzed copolymer of vinyl acetate and 3,4-diacetoxy-1-butene",null,"917249-64-0","ー","○","ー","ー","ー","Ⅲ",3,"ビニルアルコールはポリマー構成成分に対して50重量%以上。\n３，４－ジアセトキシ-1-ブテンの共重合量は8mol%以下。"]
[1150,null,4,"酢酸ビニル・ジアセトンアクリルアミド共重合体完全ケン化物／酢酸ビニル・ジアセトンアクリルアミド共重合体部分ケン化物\n（ビニルアルコール・ジアセトンアクリルアミド共重合体／\nビニルアルコール・酢酸ビニル・ジアセトンアクリルアミド共重合体）",null,"Completely hydrolyzed copolymer of vinyl acetate and diacetone acrylamide/\nPartially hydrolyzed copolymer of vinyl acetate and diacetone acrylamide",null,"259679-38-4","ー","ー","ー","ー","ー","Ⅰ",3,"食品非接触層に限る。\nAw0.7以下の食品に限る。\nビニルアルコール：80～99mol％\n酢酸ビニル：0～12mol％\nジアセトンアクリルアミド：1～8mol％"]
[1148,null,5,"酢酸ビニル・イタコン酸共重合体部分ケン化物及びそのナトリウム塩（ビニルアルコール・酢酸ビニル・イタコン酸共重合体及びそのナトリウム塩）",null,"Partially hydrolyzed copolymer of Vinyl acetate and Itaconic acid, sodium salts",null,"122625-12-1","○","○","○","○","○","Ⅰ",3]
[1151,null,6,"加水分解処理された酢酸ビニル・N-ビニルフォルムアミド共重合体","加水分解処理された酢酸ビニル・N-ビニル-ホルムアミド共重合体","Acetic acid ethenyl ester, polymer with N-ethenylformamide, hydrolyzed",null,"0163879-68-3","ー","ー","ー","ー","ー","Ⅰ",3,"食品非接触層に限る。"]
[1154,null,7,"酢酸ビニル重合体ケン化物・ホルムアルデヒド変性物","ホルムアルデヒド修飾及び完全加水分解処理された酢酸 ビニル単独重合体","Formalized polyvinyl alcohol",null,"0063148-64-1","○","○","○","○","○","Ⅰ",3]
[]
[null,null,"１５．ポリメチルペンテン（PMP)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1246,null,1,"４－メチル－１－ペンテン単独重合体",null,"4-methyl pentene-1 homopolymer",null,"25068-26-2","○","○","ー","○","○","Ⅲ",2]
[1244,null,2,"４－メチル－１－ペンテン・１－アルケン共重合体",null,"Copolymers of 4-methyl pentene-1 with one or more of 1-alkenes (C2-C18), ",null,"68413-03-6\n25155-83-3\n81229-87-0\n25119-95-3\n等","○","○","○","○","○","Ⅲ",2,"１－アルケンはC2～C18。\n１－アルケンは１種類以上使用可能。\n１－アルケンの含有量は、\nC2～C5:10モル%以下\nC6～C10:8モル%以下\nC12～C18:3モル%以下"]
[1245,null,3,"４－メチル－１－ペンテン・１－アルケン共重合体・無水マレイン酸グラフト重合体",null,"Maleic anhydride-modified Copolymers of 4-methyl pentene-1 with one or more of 1-alkenes (C2-C18), ",null,"1240978-82-8\n等\n","○","○","ー","○","○","Ⅲ",2,"１－アルケンはC2～C18。\n１－アルケンは１種類以上使用可能。\n１－アルケンの含有量は、\nC2～C5:10モル%以下\nC6～C10:8モル%以下\nC12～C18:3モル%以下\n無水マレイン酸はポリマー構成成分に対して10重量%以下"]
[]
[null,null,"１６．ポリブテン（PB)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1208,null,1,"１－ブテン単独重合体",null,"1-Butene, homopolymer",null,"9003-28-5","○","○","○","○","○","Ⅱ",2,"区分５、６の樹脂と混合する場合は使用可能温度はIII。"]
[1206,null,2,"１－ブテン・１－アルケン共重合体",null,"Copolymers of butene-1 with one or more of 1-alkene",null,"25087-34-7\n29160-13-2\n等","○","○","○","○","○","Ⅲ",2,"１－アルケンは１種類以上使用可能。\n１－アルケンは合計50 重量%未満。\nC11以上の１－アルケンにあってはポリマー構成成分に対して合計10 重量%以下。"]
[1207,null,3,"ポリイソブチレン単独重合体","イソブテン単独重合体","Polyisobutylene,homopolymer",null,"0009003-27-4","○","○","○","○","○","Ⅱ",2]
[]
[null,null,"１７．ブタジエン樹脂（BDR)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1177,null,1,"１，３－ブタジエン単独重合体（シンジオタクチック型）",null,"Polymer of Syndiotactic Buta-1,3-diene (consisting with over 70% of Vinyl Bonding content)",null,"9003-17-2","○","○","ー","○","○","Ⅰ",2,"１，２－結合70％以上。"]
[]
[null,null,"１８．エチレン・テトラシクロドデセン共重合体（E/TD）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[90,null,1,"エチレン・テトラシクロドデセン(テトラシクロ［４．４．０．１2,5．１7,10］ドデセン－３)共重合体",null,"Copolymers of ethylene and tetracyclododecene (tetracyclo[4.4.0.12,5.17,10]dodecene-3)",null,"26007-55-6","○","○","ー","○","○","Ⅲ",2,"テトラシクロドデセンはポリマー構成成分に対して10～50mol%の範囲"]
[]
[null,null,"１９．エチレン・2-ノルボルネン共重合体（E/NB）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[78,null,1,"エチレン・２－ノルボルネン共重合体",null,"Bicyclo[2.2.1]hept-2-ene, polymer with ethene",null,"26007-43-2","〇","ー","〇","〇","〇","Ⅲ",2,"２－ノルボルネンはポリマー構成成分に対して9～31、46～89重量%（３～12、20～70mol%）。"]
[]
[null,null,"２０．ポリスチレン（PS)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1119,null,1,"スチレン単独重合体",null,"Polystyrene",null,"9003-53-6","○","○","○","○","○","Ⅲ",2]
[1122,null,2,"スチレン単独重合体（シンジオタクチック構造を有するもの）",null,"Polystyrene(syndiotactic)",null,"9003-53-6\n28325-75-9","○","○","○","○","○","Ⅲ",2]
[1121,null,3,"スチレン単独重合体及び１，３－ブタジエン単独共重合体のスチレングラフト重合体の混合物",null,"Mixture of polybutadiene grafted with polystyrene and polystyrene",null,"9003-53-6\n9003-55-8\n106974-54-3","○","○","○","○","○","Ⅲ",2,"スチレンはポリマー構成成分に対して50重量%以上。\nスチレン・１，３－ブタジエンブロック共重合体と混合する場合は使用可能温度はⅢ。"]
[1120,null,4,"スチレン・１，３－ブタジエン共重合体のスチレングラフト重合体及びスチレン単独重合体の混合物",null,"Mixture of benzene, ethenyl-, polymer with 1,3-butadiene grafted with polystyrene and polystyrene",null,"9003-53-6\n9003-55-8","○","○","○","○","○","Ⅲ",2,"スチレンはポリマー構成成分に対して50重量%以上。\nスチレン・１，３－ブタジエンブロック共重合体と混合する場合は使用可能温度はⅢ。"]
[1117,null,5,"スチレン・エチレン共重合体(ポリスチレングラフト重合体を含む）","エチレン・スチレン共重合体（スチレン単独重合体でグラフト化されたものを含む）","Benzene, ethenyl-, polymer with ethene",null,"0025068-12-6","○","○","○","○","○","Ⅲ",2,"スチレンはポリマー構成成分に対して50重量%以上。"]
[1123,null,6,"スチレン・メタクリル酸共重合体",null,"2-Propenoic acid, 2-methyl-, polymer with ethenylbenzene",null,"9010-92-8","○","○","○","○","○","Ⅲ",2,"スチレンはポリマー構成成分に対して50重量%以上。\nメタクリル酸はポリマー構成成分に対して10重量%未満。"]
[1124,null,7,"スチレン・メタクリル酸共重合体",null,"2-Propenoic acid, 2-methyl-, polymer with ethenylbenzene",null,"9010-92-8","○","○","○","○","○","Ⅲ",3,"スチレンはポリマー構成成分に対して50重量%以上。\nメタクリル酸はポリマー構成成分に対して10重量%以上。"]
[1115,null,8,"スチレン・アクリル酸ブチル共重合体",null,"2-Propenoic acid, butyl ester, polymer with ethenylbenzene",null,"25767-47-9","○","○","○","○","○","III",2,"スチレンはポリマー構成成分に対して50重量%以上。"]
[1116,null,9,"スチレン・１，３－ブタジエン共重合体のスチレン・アクリル酸ブチルグラフト重合体及びスチレン・アクリル酸ブチル共重合体の混合物",null,"Mixture of  benzene, ethenyl-, polymer with 1,3-butadiene grafted with 2-propenoic acid,butyl ester,polymer with ethenylbenzene, and 2-propenoic acid,butyl ester,polymer with ethenyl benzene",null,"25767-47-9\n25838-20-4","○","○","ー","○","○","III",2,"スチレンはポリマー構成成分に対して50重量%以上。\nスチレン・１，３－ブタジエンブロック共重合体と混合する場合は使用可能温度はⅢ。"]
[1125,null,10,"スチレン・メタクリル酸・無水マレイン酸共重合体",null,"2-Propenoic acid, 2-methyl-, methyl ester, polymer with ethenylbenzene and 2,5-furandione",null,"26809-51-8","○","○","○","○","○","Ⅲ",2,"スチレンはポリマー構成成分に対して50重量%以上。"]
[1126,null,11,"スチレン・メタクリル酸メチル・メタクリル酸共重合体",null,"2-Propenoic acid 2-methyl-, polymer with ethenylbenzene and 2-propenoic acid, 2-methyl-,metyl ester",null,"25035-81-8","○","○","ー","○","○","Ⅲ",3,"スチレンはポリマー構成成分に対して50重量％以上。\nメタクリル酸及びメタクリル酸メチルの合計はポリマー構成成分に対して10wt%以上。"]
[1118,null,12,"スチレン-αメチルスチレン共重合樹脂","スチレン・α-メチルスチレン共重合体","Poly(Styrene -co-alpha-methylstyrene)",null,"0009011-11-4","○","○","○","○","○","Ⅲ",2]
[1127,null,13,"4-メチルスチレン・スチレン共重合物","スチレン・4-メチルスチレン共重合体","Copolymer of 4-methylstyrene and styrene",null,"0026655-84-5","○","○","ー","○","○","III",2,"スチレンはポリマー構成成分に対して50重量%以上。"]
[]
[null,null,"２１．スチレンブロック共重合体（SBC)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[559,null,1,"スチレン・１，３－ブタジエンブロック共重合体",null,"Benzene, ethenyl-, block polymer with 1,3-butadiene",null,"9003-55-8","○","○","○","○","○","Ⅱ",2,"使用可能温度Ⅲは、30分未満。\n区分２のメタクリル酸メチル・スチレン共重合体と混合（49％以下）する場合は使用可能温度はIII。"]
[555,null,2,"スチレン・１，３－ブタジエンブロック共重合体（水素化されたもの）",null,"Benzene, ethenyl-, block polymer with 1,3-butadiene, hydrogenated",null,"66070-58-4\n113569-15-6\n124578-11-6","〇","〇","○","〇","〇","Ⅲ",2,"油性及び脂肪性食品の使用は、他の樹脂と混合する場合に限る。"]
[554,null,3,"スチレン・イソプレンブロック共重合体（水素化されたもの）",null,"Benzene, ethenyl-, block polymer with 2-methyl-1,3-butadiene, hydrogenated",null,"68648-89-5","〇","ー","○","〇","〇","Ⅲ",2]
[553,null,4,"スチレン・イソプレン・１，３－ブタジエンブロック共重合体（水素化されたもの）",null,"Benzene, ethenyl-, polymer with 1,3-butadiene and 2-methyl-1,3-butadiene, hydrogenated, block",null,"132778-07-5","〇","ー","○","〇","〇","Ⅲ",2]
[556,null,5,"スチレン・ｐ－メチルスチレン・イソプレン・１，３－ブタジエンブロック共重合体（水素化されたもの）",null,"Benzene, 1-ethenyl-4-methyl, block polymer with 1,3-butadiene, ethenylbenzene and 2-methyl-1,3-butadiene, hydrogenated",null,"685518-46-1","〇","ー","○","〇","〇","Ⅱ",2]
[558,null,6,"スチレン・イソプレンブロック共重合体","スチレン単独重合体とイソプレン単独重合体のブロック共重合体","Benzene, ethenyl-, block polymer with 2-methyl-1,3-butadiene",null,"0025038-32-8","○","○","○","○","○","Ⅲ",2]
[557,null,7,"スチレン・イソブチレンブロック共重合体","スチレン単独重合体とイソブテン単独重合体のブロック共重合体","benzene, ethenyl-, block polymer with 2-methyl-1-propene",null,"0009011-12-5","○","○","○","○","○","Ⅲ",2]
[]
[null,null,"２２．スチレン・アクリロニトリル樹脂（SAN)及びアクリロニトリル・ブタジエン・スチレン樹脂（ABS）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[null,null,"（１）硬質相"]
[60,null,1,"スチレン・アクリロニトリル共重合体",null,"Polymer of acrylonitrile / styrene",null,"9003-54-7","○","○","○","○","○","Ⅱ",3,"スチレンは最終ポリマー構成成分に対して50重量%以上。"]
[63,null,2,"αーメチルスチレン・アクリロニトリル共重合体",null,"Polymer of acrylonitrile / isopropenylbenzene",null,"25747-74-4","○","○","ー","○","○","Ⅱ",3,"他の硬質相及び（２）の弾性体相との混合に限る。\nαｰメチルスチレンは最終ポリマー構成成分に対して50重量%以上。"]
[65,null,3,"スチレン・アクリロニトリル・メタクリル酸メチル共重合体",null,"Polymer of acrylonitrile / methyl methacrylate / styrene",null,"25213-88-1","○","○","○","○","○","Ⅱ",3,"（２）の弾性体相との混合に限る。\nアクリロニトリルは最終ポリマー構成成分に対して50重量%未満。"]
[61,null,4,"スチレン・アクリロニトリル・アクリル酸ブチル共重合体",null,"Polymer of acrylonitrile / butyl acrylate / styrene",null,"26299-47-8","○","○","○","○","○","Ⅱ",3,"スチレンは最終ポリマー構成成分に対して50重量%以上。"]
[62,null,5,"スチレン・アクリロニトリル・メタクリル酸メチル・アクリル酸ブチル共重合体",null,"Polymer of acrylonitrile / butyl acrylate / styrene/ methyl methacrylate",null,"25852-38-4","○","○","○","○","○","Ⅱ",3,"（２）の弾性体相との混合に限る。\nアクリロニトリルは最終ポリマー構成成分に対して50重量%未満。"]
[64,null,6,"スチレン・アクリロニトリル・Ｎ－フェニルマレイミド共重合体",null,"2-Propenenitrile, polymer with ethenylbenzene and 1-phenyl-1H-pyrrole-2,5-dione",null,"31621-07-5","○","○","ー","○","○","Ⅱ",3,"（２）の弾性体相との混合に限る。\nアクリロニトリルは最終ポリマー構成成分に対して50重量%未満。"]
[null,null,"（２）弾性体相 "]
[71,null,1,"１，３－ブタジエン単独重合体又はスチレン・１，３－ブタジエン共重合体のスチレン・アクリロニトリルグラフト共重合体",null,"Polymer of acrylonitrile / buta-1,3-diene / styrene",null,"9003-56-9","○","○","○","○","○","Ⅱ",3,"（１）の硬質相との混合に限る。\nスチレンはゴム成分を除いたポリマー構成成分に対して50重量%以上。"]
[72,null,2,"１，３－ブタジエン単独重合体のスチレン・アクリロニトリル・メタクリル酸メチルグラフト共重合体",null,"Methylmethacrylate-Acrylonitrile-Butadiene-Styrene Copolymer",null,"9010-94-0","○","○","○","○","○","Ⅱ",3,"（１）の硬質相との混合に限る。\nアクリロニトリルはゴム成分を除いたポリマー構成成分に対して50重量%未満。"]
[67,null,3,"スチレン・１，３－ブタジエン共重合体のスチレン・アクリロニトリル・メタクリル酸メチル・アクリル酸ブチルグラフト共重合体",null,"2-Propenoic acid, 2-methyl-, methyl ester, polymer with acryloitrile, 1,3-butadiene, butyl 2-propenoate and ethenylbenzene",null,"27308-83-4","○","○","○","○","○","Ⅱ",3,"（１）の硬質相との混合に限る。\nアクリロニトリルはゴム成分を除いたポリマー構成成分に対して50重量%未満。"]
[73,null,4,"スチレン・１，３－ブタジエン共重合体のスチレン・メタクリル酸メチルグラフト共重合体",null,"Polymer of buta-1,3-diene / methyl methacrylate / styrene",null,"25053-09-2","○","○","○","○","○","Ⅱ",3,"（１）の硬質相との混合に限る。"]
[68,null,5,"アクリル酸ブチル単独重合体のスチレン・アクリロニトリルグラフト共重合体",null,"Polymer of acrylonitrile / butyl acrylate / styrene",null,"26299-47-8","○","○","ー","○","○","Ⅱ",3,"（１）の硬質相との混合に限る。\nスチレンはゴム成分を除いたポリマー構成成分に対して50重量%未満。"]
[69,null,6,"アクリル酸ブチル・１，３－ブタジエン共重合体のスチレン・アクリロニトリルグラフト共重合体",null,"2-Propenoic acid, butyl ester, polymer with 1,3-butadiene, ethenylbenzene and 2-propenenitrile",null,"26657-42-1","○","○","ー","○","○","Ⅱ",3,"（１）の硬質相との混合に限る。\nスチレンはゴム成分を除いたポリマー構成成分に対して50重量%未満。"]
[70,null,7,"エチレン・プロピレン・ジシクロペンタジエン共重合体のスチレン・アクリロニトリルグラフト共重合体",null,"Polymer of acrylonitrile / ethene / prop-1-ene / styrene / tricyclo[5.2.1.0(2,6)]deca-3,8-diene",null,"30396-50-0","○","○","ー","○","○","Ⅱ",3,"（１）の硬質相との混合に限る。\nスチレンはゴム成分を除いたポリマー構成成分に対して50重量%未満。"]
[]
[null,null,"２３．メタクリル酸メチル・スチレン樹脂（MS)及びメタクリル酸メチル・ブタジエン・スチレン樹脂（MBS）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[null,null,"（１）硬質相"]
[566,null,1,"メタクリル酸メチル・スチレン共重合体",null,"Polymer of methyl methacrylate / styrene",null,"25034-86-0","○","○","○","○","○","Ⅲ",2,"メタクリル酸メチルは最終ポリマー構成成分に対して20重量%以上、50重量%未満、スチレンは最終ポリマー構成成分に対して20重量％以上、ただし両モノマーの合計は最終ポリマー構成成分に対して60重量％以上。"]
[567,null,2,"メタクリル酸メチル・スチレン共重合体",null,"Polymer of methyl methacrylate / styrene",null,"25034-86-0","○","○","○","○","○","Ⅲ",3,"メタクリル酸メチルは最終ポリマー構成成分に対して50重量%以上、スチレンは最終ポリマー構成成分に対して20重量％以上。"]
[565,null,3,"メタクリル酸メチル・スチレン・アクリル酸ブチル共重合体",null," 2　-Propenoic acid, 2-methyl-, methyl ester, polymer\n with butyl 2-propenoate and ethenylbenzene",null,"27136-15-8","○","○","○","○","○","Ⅱ",3,"メタクリル酸エステルおよびスチレンは、最終ポリマー構成成分に対して各20重量％以上、合計60重量％以上。"]
[null,null,"（２）弾性体相"]
[569,null,1,"スチレン・1,3-ブタジエン共重合体のスチレン・メタクリル酸メチル・アクリル酸ブチルグラフト共重合体",null,"2　-Propenoic acid, 2-methyl-, methyl ester, polymer with 1,3-butadiene, butyl 2-propenoate and ethenylbenzene",null,"25101-28-4","○","○","○","○","○","Ⅱ",3,"（１）の硬質相またはポリスチレンとの混合に限る。\n当該物質を30％以下の割合として「メタクリル酸メチル・スチレン共重合体」と混合する場合及び、当該物質を20％以下の割合として「スチレン単独重合体及び１，３－ブタジエン単独共重合体のスチレングラフト重合体の混合物」または「スチレン・メタクリル酸共重合体」（樹脂区分２）と混合する場合は、使用可能温度はIII。"]
[570,null,2,"1,3-ブタジエン単独重合体又はスチレン・1,3-ブタジエン共重合体のメタクリル酸メチル・アクリロニトリル・スチレングラフト共重合体",null,"2-Propenoic acid, 2-methyl-, methyl ester, polymer with 1,3-butadiene, ethenylbenzene and 2-propenenitrile",null,"9010-94-0","○","○","○","○","○","Ⅱ",3,"（１）の硬質相との混合に限る。"]
[]
[null,null,"２４．ポリメタクリル酸メチル（PMMA）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1239,null,1,"メタクリル酸メチル単独重合体",null,"Polymer of methyl methacrylate",null,"9011-14-7","○","○","○","○","○","Ⅱ",3,"区分４の樹脂と混合（５％以下）する場合は使用可能温度はⅢ。"]
[54,null,2,"トリメチロールプロパントリメタクリレート単独重合体",null,"2-Propenoic acid, 2-methyl-, 1,1'-[2-ethyl-2-[[(2-methyl-1-oxo-2-propen-1-yl)oxy]methyl]-1,3-propanediyl] ester, homopolymer",null,"26426-04-0","○","○","○","○","○","Ⅱ",1]
[1235,null,3,"メタクリル酸メチル・アクリル酸メチル共重合物",null,"Methylmethacrylate methylacrylate copolymer",null,"9011-87-4","〇","〇","〇","〇","〇","Ⅱ",3,"メタクリル酸メチルは、ポリマー構成成分に対して50重量％以上。"]
[1238,null,4,"メタクリル酸メチル・メタクリル酸ブチル・メタクリル酸共重合物","メタクリル酸・メタクリル酸 ブチル・メタクリル酸 メチル共重合体","2-Propenoic acid, 2-methyl-, polymer with butyl 2-methyl-2-propenoate and methyl 2-methyl-2-propenoate",null,"0028262-63-7","○","○","ー","○","○","Ⅱ",3,"メタクリル酸メチルはポリマー構成成分に対して50重量%以上、\nメタクリル酸はポリマー構成成分に対して5重量%以下。"]
[1234,null,5,"メタクリル酸メチル・アクリル酸ブチル共重合物","アクリル酸 ブチル・メタクリル酸 メチル共重合体","Methylmethacrylate butylacrylate copolymer",null,"0025852-37-3","○","○","○","○","○","Ⅲ",3,"メタクリル酸メチルは、ポリマー構成成分に対して50重量％以上。"]
[1232,null,6,"アクリル酸ブチル・メタクリル酸メチル・スチレン共重合物","アクリル酸 ブチル・スチレン・メタクリル酸 メチル共重合体"," Butyl acrylate-methyl methacrylate-styrene copolymer",null,"0027136-15-8","○","○","○","○","○","II",3,"メタクリル酸メチルは、ポリマー構成成分に対して50重量％以上。"]
[1231,null,7,"メタクリル酸メチルとアクリル酸メチルとアクリル酸ブチルとスチレンのコポリマー","アクリル酸 ブチル・アクリル酸 メチル・スチレン・メタクリル酸 メチル共重合体","Copolymers of methyl methacrylate and methyl acrylate and butylacrylate with styrene.",null,"0051998-22-2","○","○","○","○","○","II",3,"メタクリル酸メチルは、ポリマー構成成分に対して50重量％以上。"]
[1236,null,8,"メタクリル酸メチル・スチレン共重合物","スチレン・メタクリル酸 メチル共重合体"," \nMethyl methacrylate-styrene copolymer \n",null,"0025034-86-0 ","○","○","○","○","○","II",3,"メタクリル酸メチルは、ポリマー構成成分に対して50重量％以上。"]
[1237,null,9,"メタクリル酸メチル・メタクリル酸グリシジル共重合物","メタクリル酸 グリシジル・メタクリル酸 メチル共重合体","2-Propenoic acid, 2-methyl-, methyl ester, polymer with 2-oxiranylmethyl 2-methyl-2-propenoate",null,"0026141-88-8","○","○","ー","○","○","Ⅱ",3,"メタクリル酸グリシジルの含有量はポリマー構成成分に対して5重量%以下。"]
[1233,null,10,"メタクリル酸メチル・メタクリル酸ブチル・アクリル酸ブチル共重合体","アクリル酸 ブチル・メタクリル酸 ブチル・メタクリル酸 メチル共重合体","2-Propenoic acid, 2-methyl-, butyl ester, polymer with butyl 2-propenoate and methyl 2-methyl-2-propenoate",null,"0025322-99-0","○","○","○","○","○","II",3,"メタクリル酸メチルは、ポリマー構成成分に対して50重量％以上。"]
[]
[null,null,"２５．ポリアミド（PA）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[918,null,1,"ε－カプロラクタム単独重合体",null,"Poly[imino(1-oxohexane-1,6-diyl)]",null,"25038-54-4","○","○","○","○","○","Ⅲ",3]
[909,null,2,"11－アミノウンデカン酸単独重合体",null,"11-aminoundecanoic acid homopolymer",null,"25587-80-8","○","○","○","○","○","Ⅲ",3]
[928,null,3,"ω－ラウロラクタム単独重合体",null,"Azacyclotridecan-2-one, homopolymer\n（Lauryl lactam, homopolymer）",null,"25038-74-8\n24937-16-4","○","○","○","○","○","Ⅲ",3]
[912,null,4,"12－アミノドデカン酸単独重合体",null,"Dodecanoic acid, 12-amino-, homopolymer",null,"25768-33-6","○","○","○","○","○","Ⅲ",3]
[911,null,5,"ε－カプロラクタム・12－アミノドデカン酸共重合体",null,"Dodecanoic acid, 12-amino-, polymer with hexahydro-2H-azepin-2-one",null,"61878-98-6\n26098-55-5","○","○","○","○","○","Ⅲ",3]
[902,null,6,"ε－カプロラクタム・ヘキサメチレンジアミン・アジピン酸共重合体",null,"Hexanedioic acid, polymer with hexahydro-2H-azepin-2-one and 1,6-hexanediamine",null,"24993-04-2","○","○","○","○","○","Ⅲ",3,"ε－カプロラクタム（CAS登録番号105-60-2）はポリマー構成成分に対して50重量%以上。"]
[899,null,7,"ε－カプロラクタム・ヘキサメチレンジアミン・アジピン酸・12－アミノドデカン酸共重合体",null,"Hexanedioic acid, polymer with 12-aminododecanoic acid, hexahydro-2H-azepin-2-one and 1,6-hexanediamine",null,"40959-29-3","○","○","○","○","○","Ⅲ",3]
[919,null,8,"ε－カプロラクタム・ヘキサメチレンジアミン・テレフタル酸共重合体",null,"1,4-Benzenedicarboxylic acid, compd. with 1,6-hexanediamine, polymer with hexahydro-2H-azepin-2-one",null,"51025-80-0","○","○","○","○","○","Ⅲ",3]
[917,null,9,"ε－カプロラクタム・３－アミノメチル－３，５，５－トリメチルシクロヘキシルアミン・テレフタル酸共重合体",null,"1,4-Benzenedicarboxylic acid, polymer with\n5-amino-1,3,3’-trimethyl-cyclohexanemethanamine\nand hexahydro-2H-azepin-2-one",null,"1105025-82-8","○","○","○","○","○","Ⅲ",3,"テレフタル酸（CAS登録番号100-21-0）と３－アミノメチル－３，５，５－トリメチルシクロヘキシルアミン（CAS登録番号2855-13-2）の合計はポリマー構成成分に対して１重量％未満。"]
[910,null,10,"11－アミノウンデカン酸・ヘキサメチレンジアミン・テレフタル酸共重合体",null,"Polymer of 11-aminoundecanoic acid / (compound of hexane-1,6-diamine and terephthalic acid)",null,"247056-11-7","○","○","ー","○","○","Ⅲ",3,"１１－アミノウンデカン酸（CAS登録番号2432-99-7）はポリマー構成成分に対して50重量%以下。\n乳・乳製品の容器包装では、食品非接触層に限る。"]
[907,null,11,"ヘキサメチレンジアミン・アジピン酸共重合体",null,"Poly[imino(1,6-dioxohexane-1,6-diyl)iminohexane-1,6-diyl]",null,"32131-17-2","○","○","○","○","○","Ⅲ",3]
[916,null,12,"ヘキサメチレンジアミン・イソフタル酸共重合体",null,"Poly(hexamethylene isophthalamide)\n1,3-Benzenedicarboxylic acid, polymer with 1,6-hexanediamine",null,"25722-07-0","ー","ー","ー","ー","○","Ⅲ",3]
[901,null,13,"ヘキサメチレンジアミン・アジピン酸・イソフタル酸共重合体",null,"1,3-Benzenedicarboxylic acid, polymer with 1,6-hexanediamine and hexanedioic acid\nPolycondensate of adipic acid, hexane-1,6-diyldiamine and isophthalic acid",null,"26353-66-2","ー","ー","ー","ー","○","Ⅰ",3]
[915,null,14,"ヘキサメチレンジアミン・イソフタル酸・テレフタル酸共重合体",null,"1,3-Benzenedicarboxylic acid, polymer with 1,4-benzenedicarboxylic acid and 1,6-hexanediamine",null,"25750-23-6","○","○","○","○","○","Ⅲ",3]
[922,null,15,"ヘキサメチレンジアミン・セバシン酸共重合体",null,"Poly[imino-1,6-hexanediylimino(1,10-dioxo-1,10-decanediyl)]\n(Decanedioic acid, polymer with 1,6-hexanediamine)",null,"9011-52-3","○","○","○","○","○","Ⅲ",3]
[906,null,16,"テトラメチレンジアミン・アジピン酸共重合体",null,"Polymer of adipic acid / butane-1,4-diamine",null,"50327-77-0","○","○","○","○","○","Ⅰ",3]
[921,null,17,"テトラメチレンジアミン・セバシン酸共重合体",null,"Poly[iminobutane-1,4-diylimino(1,10-dioxodecane-1,10-diyl)]",null,"26247-06-3","○","○","○","○","○","Ⅲ",3]
[925,null,18,"テトラメチレンジアミン・ヘキサメチレンジアミン・テレフタル酸共重合体",null,"1,4-Benzenedicarboxylic acid, polymer with 1,4-butanediamine and 1,6-hexanediamine",null,"2155803-47-5","○","○","○","○","○","Ⅲ",3,"ジアミン成分に対してテトラメチレンジアミン（CAS登録番号110-60-1）は50 mol%以上。"]
[905,null,19,"テトラメチレンジアミン・ヘキサメチレンジアミン・アジピン酸・テレフタル酸共重合体",null,"Polycondensation products of adipic acid / butane-1,4-diyldiamine / hexane-1,6-diyldiamine / terephthalic acid ",null,"2155803-51-1","○","○","○","○","○","Ⅲ",3,"ジアミン成分に対してテトラメチレンジアミン（CAS登録番号110-60-1）は50 mol%以上。"]
[914,null,20,"テトラメチレンジアミン・ヘキサメチレンジアミン・イソフタル酸・テレフタル酸共重合体",null,"1,3-Benzenedicarboxylic acid, polymer with 1,4-benzenedicarboxylic acid, 1,4-butanediamine and 1,6-hexanediamine",null,"2201801-54-7","○","○","○","○","○","Ⅲ",3,"ジアミン成分に対してテトラメチレンジアミン（CAS登録番号110-60-1）は50 mol%以上。"]
[924,null,21,"ノナメチレンジアミン・２－メチルオクタン－１，８－ジアミン・テレフタル酸共重合体",null,"1,4-Benzenedicarboxylic acid, polymer with 2-methyl-1,8-octadiamine and 1,9-nonanediamine",null,"169284-22-4","○","○","○","○","○","Ⅲ",3,"乳幼児を対象とする食品(調製粉乳等)用器具・容器包装を除く。"]
[913,null,22,"ノナメチレンジアミン・２－メチルオクタン－１，８－ジアミン・テレフタル酸・安息⾹酸共重合体",null,"1,4-Benzenedicarboxylic acid, polymer with 2-methyl-1,8-octadiamine and 1,9-nonanediamine, reaction products with benzoic acid\n",null,"1310362-57-2","○","○","○","○","○","Ⅲ",3,"乳幼児を対象とする食品(調製粉乳等)用器具・容器包装を除く。"]
[903,null,23,"m－キシリレンジアミン・アジピン酸共重合体",null,"Hexanedioic acid polymer with 1,3-benzenedimethanamine",null,"25718-70-1","○","○","○","○","○","Ⅲ",3]
[900,null,24,"m－キシリレンジアミン・アジピン酸・イソフタル酸共重合体",null,"1,3-benzenedicarboxylic acid polymer with 1,3-benzenedimethanamine and hexanedioic acid",null,"28628-75-3","○","○","○","○","○","Ⅲ",3,"イソフタル酸（CAS登録番号121-91-5）はジカルボン酸成分に対して6 mol%以下。"]
[904,null,25,"m－キシリレンジアミン・アジピン酸・ビス（アミノプロピル）ポリ（エチレンオキサイド）共重合体",null,"Adipic acid polymer with 1,3-benzenedimethanamine and bis(aminopropyl)-poly(oxyethylene)",null,"59655-05-9","○","○","ー","○","○","Ⅲ",3,"ビス(アミノプロピル)ポリ(エチレンオキサイド）（CAS登録番号34901-14-9）はポリマー構成成分に対して10重量％以下。\n単独で使用する場合は厚み15μm以下。\n混合して使用する場合は厚み200μm以下。\n乳・乳製品の容器包装では、食品非接触層に限る。"]
[923,null,26,"４，４’－メチレンビス（シクロヘキサンアミン）・ドデカン酸共重合体",null,"Dodecanedioic acid, polymer with 4,4'-methylenebis[cyclohexanamine]",null,"25038-97-5","○","○","○","○","○","Ⅱ",3]
[908,null,27,"ヘキサン二酸、アザシクロトリデカン－２－オン と、α－ヒドロ－ ω－ヒドロキシ（オキシ－１，４－ブタンジオール）の共重合体","アジピン酸・ポリテトラメチレングリコール・ラウロラクタム共重合体","Hexanedioic acid, polymer with azacyclotridecan-2-one and .alpha.-hydro-.omega.-hydroxypoly(oxy-1,4-butanediyl)",null,"0077402-38-1","○","○","ー","○","○","III",3]
[927,null,28,"1, 3－ベンゼンアミン・1, 3, 5－ベンゼントリカルボン酸重縮合物","トリメシン酸トリクロライド・1, 3－ベンゼンアミン共重合体","Polymer of benzene-1,3,5-tricarbonyl trichloride/m-Phenylenediamine",null,"0083044-99-9","○","○","○","○","○","Ⅱ",3]
[926,null,29,"ピペラジン・1, 3, 5－ベンゼントリカルボン酸重縮合物","トリメシン酸トリクロライド・ピペラジン共重合体","Polymer of benzene-1,3,5-tricarbonyl trichloride/Piperazine",null,"0079122-60-4","○","○","○","○","○","Ⅱ",3]
[920,null,30,"テレフタル酸・ステアリン酸・1,10－デカンジアミン重縮合物","ステアリン酸・1,10-デカンジアミン・テレフタル酸共重合体","1,4-Benzenedicarboxylic acid, polymer with 1,10-decanediamine, stearic acid-terminated",null,"1638190-68-7","○","○","○","○","○","Ⅲ",3]
[]
[null,null,"２６．ポリエチレンテレフタレート（PET)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1021,null,1,"テレフタル酸ジメチル・エチレングリコール共重合体／  \nテレフタル酸・エチレングリコール共重合体  ",null,"1,4-Benzenedicarboxylic acid, dimethyl ester, polymer with1,2-ethanediol / \n1,4-Benzenedicarboxylic acid, polymer with1,2-ethanediol",null,"25038-59-9","○","○","○","○","○","Ⅲ",7]
[1005,null,2,"テレフタル酸ジメチル・イソフタル酸・エチレングリコール共重合体／  \nテレフタル酸・イソフタル酸・エチレングリコール共重合体",null,"1,3-Benzenedicarboxylic acid, polymer with 1,4-benzenedicarboxylic acid, dimethyl ester and 1,2-ethanediol /\n1,3-Benzenedicarboxylic acid, polymer with 1,4-benzenedicarboxylic acid and 1,2-ethanediol",null,"24938-04-3\n26006-30-4\n28934-16-9\n31342-83-3","○","○","○","○","○","Ⅲ",7,"無水トリメリット酸（CAS登録番号552-30-7）を酸成分に対して１mol％以下使用可能。ただし、乳等１群食品用容器包装では食品直接接触層に使用してはならない。"]
[1017,null,3,"テレフタル酸・セバシン酸・エチレングリコール共重合体  ",null,"1,4-Benzenedicarboxylic acid, polymer with decanedioic acid and 1,2-ethanediol",null,"25067-21-4","○","○","○","○","○","Ⅲ",7]
[1010,null,4,"テレフタル酸ジメチル・エチレングリコール・ジエチレングリコール共重合体／\nテレフタル酸・エチレングリコール・ジエチレングリコール共重合体",null,"1,4-Benzenedicarboxylic acid, demethyl ester, polymer with 1,2-ethanediol and 2,2'-oxybis[ethanol] /\n1,4-Benzenedicarboxylic acid, polymer with 1,2-ethanediol and 2,2'-oxybis[ethanol]",null,"25052-77-1","○","○","○","○","○","Ⅲ",7]
[1022,null,5,"テレフタル酸ジメチル・エチレングリコール・ネオペンチルグリコール共重合体／\nテレフタル酸・エチレングリコール・ネオペンチルグリコール共重合体",null,"1,4-Benzenedicarboxylic acid, dimethyl ester, polymer with 2,2-dimethyl-1,3-propanediol and 1,2-ethanediol /\n1,4-Benzenedicarboxylic acid, polymer with 2,2-dimethyl-1,3-propanediol and 1,2-ethanediol",null,"26780-49-4\n28604-35-5","○","○","○","○","○","Ⅲ",7,"乳等１群食品用容器包装では食品直接接触層に使用してはならない。"]
[999,null,6,"テレフタル酸ジメチル・イソフタル酸・エチレングリコール・ジエチレングリコール共重合体／\nテレフタル酸・イソフタル酸・エチレングリコール・ジエチレングリコール共重合体",null,"1,3-Benzenedicarboxylic acid, polymer with 1,4-benzenedicarboxylic acid, dimethyl ester, 1,2-ethanediol and 2,2'-oxybis(ethanol) /\n1,3-Benzenedicarboxylic acid, polymer with 1,4-benzenedicarboxylic acid, 1,2-ethanediol and 2,2'-oxybis(ethanol)",null,"27027-87-8\n69572-04-9","○","○","○","○","○","Ⅲ",7]
[1004,null,7,"テレフタル酸・イソフタル酸・エチレングリコール・１，４－ブタンジオール共重合体",null,"1,3-Benzenedicarboxylic acid, polymer with 1,4-benzenedicarboxylic acid, 1,4-butanediol and 1,2-ethanediol  ",null,"52257-23-5","○","○","○","○","○","Ⅲ",7]
[1002,null,8,"テレフタル酸・イソフタル酸・エチレングリコール・ネオペンチルグリコール共重合体",null,"1,3-Benzenedicarboxylic acid, polymer with 1,4-benzenedicarboxylic acid, 2,2-dimethyl-1,3-propanediol and 1,2-ethanedi",null,"27923-68-8","○","○","○","○","○","Ⅲ",7,"乳等１群食品用容器包装では食品直接接触層に使用してはならない。"]
[1011,null,9,"テレフタル酸ジメチル・エチレングリコール・ジエチレングリコール・ネオペンチルグリコール共重合体／\nテレフタル酸・エチレングリコール・ジエチレングリコール・ネオペンチルグリコール共重合体",null,"1,4-Benzenedicarboxylic acid, dimethyl ester, polymer with 2,2-dimethyl-1,3-propanediol, 1,2-ethanediol and 2,2'-oxybis[ethanol]  /\n1,4-Benzenedicarboxylic acid, polymer with 2,2-dimethyl-1,3-propanediol, 1,2-ethanediol and 2,2'-oxybis[ethanol]  ",null,"58792-58-8\n132354-80-4","○","○","○","○","○","Ⅲ",7,"乳等１群食品用容器包装では食品直接接触層に使用してはならない。"]
[1023,null,10,"テレフタル酸ジメチル・エチレングリコール・α－ヒドロ－ω－ヒドロキシポリ（オキシエチレン）ランダム共重合体／\nテレフタル酸・エチレングリコール・α－ヒドロ－ω－ヒドロキシポリ（オキシエチレン）ランダム共重合体",null,"1,4-Benzenedicarboxylic acid, dimethyl ester, polymer with1,2-ethanediol and alpha-hydro-omega-hydroxypoly(oxy-1,2-ethanediyl) / \n1,4-Benzenedicarboxylic acid, polymer with1,2-ethanediol and alpha-hydro-omega-hydroxypoly(oxy-1,2-ethanediyl)",null,"9016-88-0","○","○","○","○","○","Ⅲ",7,"ポリエチレングリコール（CAS登録番号25322-68-3）の使用量はポリマー構成成分に対して10重量％以下。\nポリエチレングリコール（CAS登録番号25322-68-3）の分子量：400～30000\n乳等１群食品用容器包装には使用してはならない。"]
[1012,null,11,"テレフタル酸ジメチル・１，４－シクロヘキサンジメタノール・エチレングリコール共重合体／\nテレフタル酸・１，４－シクロヘキサンンジメタノール・エチレングリコール共重合体","エチレングリコール・1,4-シクロヘキサンジメタノール・テレフタル酸またはテレフタル酸 ジメチル共重合体","1,4-benzenedicarboxylic acid, dimethyl ester, polymer with 1,4-cyclohexanedimethanol, and ethylene glycol / \n1,4-benzenedicarboxylic acid, polymer with 1,4-cyclohexanedimethanol, and ethylene glycol ",null,"0025640-14-6\n0025038-91-9","〇","〇","○","〇","〇","Ⅱ",7,"１，４－シクロヘキサンジメタノール（CAS登録番号105-08-8）はジオール成分の50mol%未満。\n酒類はアルコール濃度25％以下。\nアルコール濃度13%を越える場合、使用可能温度は70℃以下。"]
[1009,null,12,"テレフタル酸ジメチル・エチレングリコール・１，４－シクロヘキサンジメタノール・ジエチレングリコール共重合体／\nテレフタル酸・エチレングリコール・１，４－シクロヘキサンジメタノール・ジエチレングリコール共重合体","エチレングリコール・ジエチレングリコール・1,4-シクロヘキサンジメタノール・テレフタル酸またはテレフタル酸 ジメチル共重合体","1,4-Benzenedicarboxylic acid, dimethyl ester, polymer with 1,4-cyclohexanedimethanol, 1,2-ethanediol and 2,2'-oxybis[ethanol] /\n1,4-Benzenedicarboxylic acid, polymer with 1,4-cyclohexanedimethanol, 1,2-ethanediol and 2,2'-oxybis[ethanol]",null,"0148105-13-9\n0156209-91-5","－","〇","○","〇","〇","Ⅱ",7,"１，４－シクロヘキサンジメタノール（CAS登録番号105-08-8）及びジエチレングリコール（CAS登録番号107-21-1）の合計は、ジオール成分に対して35mol%以下。\nジエチレングリコール（CAS登録番号107-21-1）はジオール成分に対して12mol%以下。\n酒類はアルコール濃度15％以下。"]
[1019,null,13,"テレフタル酸・エチレングリコール・２，２－ビス［４－（２－ヒドロキシエトキシ）フェニル］プロパン共重合体",null,"1,4-Benzenedicarboxylic acid, polymer of ethylene glycol and 2,2'-[isopropylidenebis(4,1-phenyleneoxy)]diethanol",null,"25640-01-1","○","○","○","○","○","Ⅱ",7,"２，２－ビス［４－（２－ヒドロキシエトキシ）フェニル］プロパン（CAS登録番号901-44-0）はジオール成分に対して7.5mol%以下。\n乳等１群食品用容器包装には使用してはならない。"]
[1018,null,14,"テレフタル酸ジメチル・２，６－ナフタレンジカルボン酸ジメチル・エチレングリコール共重合体",null,"Dimethyl 1,4-benzenedicarboxylate and 1,2-ethanediol polymer\nwith 2,6-naphthalenedicarboxylic acid, dimethyl ester",null,"ー","○","○","○","○","○","Ⅲ",7,"２，６－ナフタレンジカルボン酸ジメチル（CAS登録番号840-65-3）は酸成分の50 mol%未満。\n乳等１群食品用容器包装では食品直接接触層に使用してはならない。"]
[1006,null,15,"テレフタル酸・イソフタル酸・不飽和脂肪酸(Ｃ18)二量体水素付加物・エチレングリコール共重合体／\nテレフタル酸ジメチル・イソフタル酸ジメチル・不飽和脂肪酸(Ｃ18)二量体水素付加物・エチレングリコール共重合体\n","イソフタル酸またはイソフタル酸 ジメチル・エチレングリコール・テレフタル酸またはテレフタル酸 ジメチル・二量化及び水素化処理された不飽和脂肪酸（C18）共重合体","Polycondensation products of ethylene glycol / isophthalic acid / terephthalic acid / [hydrogenated cyclic and acyclic dimer acid(mainly C=36) obtained as dimers of unsaturated fatty acid(C=18)]／\nPolycondensation products of ethylene glycol / dimethyl isophthalate / dimethyl terephthalate / [hydrogenated cyclic and acyclic dimer acid(mainly C=36) obtained as dimers of unsaturated fatty acid(C=18)]\n",null,"1997309-35-9\n2361307-67-5","○","○","○","○","○","Ⅲ",7,"不飽和脂肪酸（C18）二量体水素付加物（CAS登録番号68783-41-5）はポリマー構成成分に対しての3.5mol％以下。\n乳等１群食品用容器包装には使用してはならない。"]
[1014,null,16,"テレフタル酸ジメチル・エチレングリコール・スピログリコール共重合体／\nテレフタル酸・エチレングリコール・スピログリコール共重合体",null,"1,4-Benzenedicarboxylic acid, dimethyl ester, polymer with 1,2-ethanediol and β,β,β',β',-tetramethyl-2,4,8,10-tetraoxaspiro[5.5] undecane-3,9-diethanol / \n1,4-Benzenedicarboxylic acid, polymer with 1,2-ethanediol                                             and β,β,β',β',-tetramethyl-2,4,8,10-tetraoxaspiro[5.5]                                            undecane-3,9-diethanol",null,"59802-09-4\n102070-64-4","○","○","○","○","○","Ⅲ",7,"スピログリコール（CAS登録番号1455-42-1）はジオール成分に対して50mol%未満。"]
[1015,null,17,"テレフタル酸ジメチル・２，６－ナフタレンジカルボン酸ジメチル・エチレングリコール・スピログリコール共重合体／\nテレフタル酸・２，６－ナフタレンジカルボン酸・エチレングリコール・スピログリコール共重合体",null,"2,6-Naphthalenedicarboxylic acid, 2,6-dimethyl ester, polymer with 1,4-dimethyl 1,4-benzenedicarboxylate, 1,2-ethanediol and β,β,β',β'-tetramethyl-2,4,8,10-tetraoxaspiro[5.5]undecane-3,9-\ndiethanol / \n2,6-Naphthalenedicarboxylic acid,  polymer with 1,4-benzenedicarboxylate, 1,2-ethanediol and β,β,β',β'-tetramethyl-2,4,8,10-tetraoxaspiro[5.5]undecane-3,9-\ndiethanol",null,"380597-87-5","○","○","○","○","○","特記事項参照",7,"２，６－ナフタレンジカルボン酸（CAS登録番号1141-38-4）又は２，６－ナフタレンジカルボン酸ジメチル（CAS登録番号840-65-3）は酸成分に対して50mol%未満。スピログリコール（CAS登録番号1455-42-1）はジオール成分に対して50mol%未満。\n使用可能温度\n（a）２，６－ナフタレンジカルボン酸（CAS登録番号1141-38-4）又は２，６－ナフタレンジカルボン酸ジメチル（CAS登録番号840-65-3）が酸成分に対して25mol%未満の場合\n①スピログリコール（CAS登録番号1455-42-1）がジオール成分に対して25mol%未満のとき\n　油性及び脂肪性、酒類　Ⅱ\n　酸性、その他　Ⅲ\n②スピログリコール（CAS登録番号1455-42-1）がジオール成分に対して25mol%以上のとき\n　油性及び脂肪性　Ⅰ\n　酒類　Ⅱ\n　酸性、その他　Ⅲ\n（b）２，６－ナフタレンジカルボン酸（CAS登録番号1141-38-4）又は２，６－ナフタレンジカルボン酸ジメチル（CAS登録番号840-65-3）が酸成分に対して25mol%以上の場合　Ⅲ"]
[1003,null,18,"ベンゼン－１，２，４－トリカルボン酸・２，２－ジメチルプロパン－１，３－ジオール・エチレングリコール・２，２’－［（イソプロピリデン）ビス（４，１－フェニレンオキシ）］ジエタノール・テレフタル酸重合物\n／テレフタル酸・イソフタル酸・ビスフェノールＡ・エチレングリコール重縮合物","下記のブロック共重合体という意味か？（CASは上の共重合体のもの）\nエチレングリコール・2,2-ジメチル-1,3-プロパンジオール・テレフタル酸・トリメリット酸・ビスフェノールAとエチレングリコールのジエーテル共重合体\nイソフタル酸・エチレングリコール・テレフタル酸・ビスフェノールＡ共重合体","Polymer of benzene-1,2,4-tricarboxylic acid / 2,2-dimethylpropane-1,3-diol / ethylene glycol / 2,2'-[(isopropylidene)bis(4,1-phenyleneoxy)]diethanol / terephthalic acid",null,"0240481-82-7","○","○","○","○","○","Ⅰ",7]
[1008,null,19,"テレフタル酸・ε-カプロラクトン・エチレングリコール・１，４－ブタンジオール共重合体","エチレングリコール・カプロラクトン・テレフタル酸・1,4-ブタンジオール共重合体","1,4-Benzenedicarboxylic acid polymer with 2-oxepanone, \n1,2-ethanediol, and 1,4-butanediol",null,"0175719-44-5","〇","〇","〇","〇","〇","Ⅲ",7]
[1001,null,20,"テレフタル酸・イソフタル酸・エチレングリコール\n・ビスフェノールAエチレンオキサイド付加体共重合体","イソフタル酸・エチレングリコール・テレフタル酸・\nビスフェノールAとエチレングリコールのジエーテル共重合体","1,4-Benzenedicarboxylic acid polymer \nwith 1,3-Benzenedicarboxylic acid, 1,2-ethanediol,\nand 2,2-Bis[4-(2-hydroxyethoxy)phenyl]propane",null,"0041259-36-3","〇","〇","〇","〇","〇","Ⅲ",7]
["削除1",null,21,"テレフタル酸・２－（９’，１０’－ジヒドロ－９’－オキサ－１０’－オキサイド－１０’－ホスフアフエナントレン－１０’－イル）メチルコハク酸ビス（２－ヒドロキシエチル）・エチレングリコール共重合体","CAS間違い（0063562-48-1であれば28と同じ）","1,4-Benzenedicarboxylic acid polymer \nwith Bis(2-hydroxyethyl) (6H-dibenz[c,e][1,2]oxaphosphorin-6-ylmethyl)succinate P-oxide and 1,2-ethanediol",null,"0062562-34-5","〇","〇","〇","〇","〇","Ⅲ",7]
[997,null,22,"テレフタル酸ジメチル・アジピン酸・イソフタル酸・エチレングリコール共重合体/テレフタル酸・アジピン酸・イソフタル酸・エチレングリコール共重合体","アジピン酸・イソフタル酸・エチレングリコール・テレフタル酸またはテレフタル酸 ジメチル共重合体","1,3-Benzenedicarboxylic acid, polymer with 1,4-benzenedicarboxylic acid, dimethyl ester,hexanedioic acid and 1,2-ethanediol / 1,3-Benzenedicarboxylic acid, polymer with 1,4-benzenedicarboxylic\n   acid, hexanedioic acid and 1,2-ethanediol",null,"0028433-29-6","○","○","○","○","○","Ⅲ",7,"アジピン酸又はイソフタル酸が酸成分に対して50mol%未満"]
[1020,null,23,"テレフタル酸・エチレングリコール・１，４－ブタンジオール共重合体","エチレングリコール・テレフタル酸・1,4-ブタンジオール共重合体","1,4-Benzenedicarboxylic acid, polymer with 1,2-ethanediol, and 1,4-butanediol ",null,"－","○","○","○","○","○","Ⅲ",7]
[1024,null,24,"テレフタル酸・エチレングリコール・2-メチル-1,3-プロパンジオール共重合体  ","エチレングリコール・テレフタル酸・2-メチル-1,3-プロパンジオール共重合体  ","1,4-Benzenedicarboxylic acid, polymer with1,2-ethanediol, and 2-methyl-1,3-propanediol",null,"－","○","○","○","○","○","Ⅲ",7]
[1000,null,25,"テレフタル酸･イソフタル酸・１，４－シクロヘキシレンジメタノール・エチレングリコール共重合体","イソフタル酸・エチレングリコール・1,4-シクロヘキサンジメタノール・テレフタル酸共重合体","1,4-benzenedicarboxylic acid, polymer with 1,3-benzenedicarboxylic acid, 1,4-cyclohexanedimethanol, and 1,2-ethanediol  ",null,"－","○","○","○","○","○","Ⅲ",7]
[1025,null,26,"テレフタル酸・エチレングリコール・トリメチロールプロパン・不飽和脂肪酸（C18）2量体水素添加物・1,4-ブタンジオールブロック共重合体","エチレングリコール・テレフタル酸・トリメチロールプロパン・二量化及び水素化処理された不飽和脂肪酸（C18）・1,4-ブタンジオール共重合体","Fatty acids, C18-unsatd.,　dimmers,　hydrogenated polymers with 1,4-butanediol, ethylene glycol, terephthalic acid and trimethylolpropane,block",null,"1436849-13-6","○","○","○","○","○","Ⅲ",3]
[1016,null,27,"ポリエチレンテレフタレート―５―ナトリウム　スルホイソフタル酸コポリマー","エチレングリコール・5-スルホイソフタル酸 ジメチルのナトリウム塩・テレフタル酸ジメチル共重合体","Polymer of dimethyl terephthalate / ethylene glycol / sodium 3,5-bis(methoxycarbonyl)benzenesulfonate",null,"0027937-63-9","○","○","○","○","○","Ⅲ",3]
[1013,null,28,"テレフタル酸・２―(９，１０―ジヒドロ―９―オキサ―１０―オキサイド―１０―フォスファフェナンスレン―１０―イル)メチルコハク酸・エチレングリコール重縮合物","エチレングリコール・9,10-ジヒドロ-10-(2,3-ジカルボキシプロピル)-9-オキサ-10-ホスファフェナントレン-10-オキシド・テレフタル酸共重合体","Polymer of ethylene glycol / 2-[(6-oxo-6H-dibenzo[c,e][1,2lambda(5)]oxaphosphinin-6-yl)methyl]succinic acid / terephthalic acid",null,"0063562-48-1","○","○","○","○","○","Ⅲ",3]
[998,null,29,"テレフタル酸・1,4:3,6-ジアンヒドロソルビトール・1,4-シクロヘキサンジメタノール・エチレングリコール共重合体","イソソルビド・エチレングリコール・1,4-シクロヘキサンジメタノール・テレフタル酸共重合体","D-Glucitol, 1,4:3,6-dianhydro-, polymer with 1,4-benzenedicarboxylic acid, 1,4-cyclohexanedimethanol and 1,2-ethanediol",null,"1038843-64-9","○","○","○","○","○","特記事項参照",7,"1,4:3,6-ジアンヒドロソルビトール（CAS登録番号652-67-5）が構成成分の１～40mol%の場合、使用可能温度はⅡ。\n1,4:3,6-ジアンヒドロソルビトール（CAS登録番号652-67-5）が構成成分の41～60mol%の場合、使用可能温度はⅢ。"]
[1007,null,30,"テレフタル酸・1,4-シクロヘキサンジメタノール・エチレングリコール・ ４－（ヒドロキシメチル）シクロヘキサンカルボン酸［４－（ヒドロキシメチル）シクロヘキシル］メチル　エステル・ジエチレングリコール・４，４’－［オキシビス（メチレン）］ビス（シクロヘキサンメタノール）共重合体","エチレングリコール・4,4'-[オキシビス(メチレン)]ビス[シクロヘキサンメタノール]・ジエチレングリコール・1,4-シクロヘキサンジメタノール・テレフタル酸・4-​(ヒドロキシメチル)​-シクロヘキサンカルボン酸 [4-​(ヒドロキシメチル)シクロヘキシル​]メチル共重合体","1,4-Benzenedicarboxylic acid, polymer with 1,4-cyclohexanedimethanol, 1,2-ethanediol,[4-(hydroxymethyl) cyclohexyl]methyl 4-(hydroxymethyl)cyclohexanecarboxylate, 2,2'-oxybis[ethanol] and 4,4'-[oxybis(methylene)]bis[cyclohexanemethanol] ",null,"1632972-01-0","○","○","○","○","○","I",7]
[]
[null,null,"２７．ポリエチレンナフタレート（PEN)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1032,null,1,"２，６－ナフタレンジカルボン酸ジメチル・エチレングリコール共重合体／\n２，６－ナフタレンジカルボン酸・エチレングリコール共重合体",null,"2,6-naphthalenedicarboxylic acid, dimethyl ester polymer with 1,2-ethanediol / 2,6-naphthalenedicarboxylic acid, polymer with 1,2-ethanediol",null,"24968-11-4\n25853-85-4","○","○","○","○","○","III",3]
[1031,null,2,"２，６－ナフタレンジカルボン酸ジメチル・テレフタル酸ジメチル・エチレングリコール共重合体／\n２，６－ナフタレンジカルボン酸・テレフタル酸・エチレングリコール共重合体",null,"2,6-naphthalenedicarboxylic acid, dimethyl ester polymer with dimethyl 1,4-benzenedicarboxylate and 1,2-ethanediol / 2,6-naphthalenedicarboxylic acid, polymer with 1,4-benzenedicarboxylate and 1,2-ethanediol ",null,"26221-57-8","○","○","○","○","○","III",3,"テレフタル酸ジメチル（CAS登録番号120-61-6）又はテレフタル酸（CAS登録番号100-21-0）は酸成分に対しての50mol％以下。"]
[1030,null,3,"２，６－ナフタレンジカルボン酸ジメチル・テレフタル酸ジメチル・エチレングリコール・１，４－シクロヘキサンジメタノール共重合体／\n２，６－ナフタレンジカルボン酸・テレフタル酸・エチレングリコール・１，４－シクロヘキサンジメタノール共重合体","エチレングリコール・1,4-シクロヘキサンジメタノール・テレフタル酸またはテレフタル酸 ジメチル・2,6-ナフタレンジカルボン酸または2,6-ナフタレンジカルボン酸 ジメチル共重合体","2,6-naphthalenedicarboxylic acid, dimethyl ester polymer with dimethyl 1,4-benzenedicarboxylate, 1,2-ethanediol, 1,4-cyclohexanedimethanol/\n2,6-Naphthalenedicarboxylic acid, polymer with 1,4-benzenedicarboxylate, 1,2-ethanediol and 1,4-cyclohexanedimethanol",null,"0155337-45-4\n0161911-39-3","○","○","○","○","○","III",3,"テレフタル酸ジメチル（CAS登録番号120-61-6）又はテレフタル酸（CAS登録番号100-21-0）は酸成分に対しての15mol％。\n１，４－シクロヘキサンジメタノール（CAS登録番号105-08-8）はジオール成分に対して40mol%以下。"]
[]
[null,null,"２８．ポリエチレンフラノエート（PEF)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1037,null,1,"２，５－フランジカルボン酸・エチレングリコール共重合体",null,"2,5-Furandicarboxylic acid,polymer with 1,2-ethanediol",null,"28728-19-0","○","○","○","○","○","Ⅲ",3]
[]
[null,null,"２９．ポリシクロヘキシルジメチレンテレフタレート（PCT)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1105,null,1,"テレフタル酸ジメチル・１，４－シクロヘキサンジメタノール共重合体／\nテレフタル酸・１，４－シクロヘキサンジメタノール共重合体",null,"1,4-benzenedicarboxylic acid, dimethyl ester, polymer with 1,4-cyclohexanedimethanol / \n1,4-benzenedicarboxylic acid, polymer with 1,4-cyclohexanedimethanol ",null,"25135-20-0 25037-99-4","〇","〇","ー","〇","〇","Ⅱ",3,"酒類はアルコール濃度25％以下。\nアルコール濃度13%を越える場合、使用可能温度は70℃以下。"]
[1102,null,2,"テレフタル酸ジメチル・イソフタル酸ジメチル・１，４－シクロヘキサンジメタノール共重合体／\nテレフタル酸・イソフタル酸・1，４－シクロヘキサンジメタノール共重合体",null,"1,4-benzenedicarboxylic acid, dimethyl ester, polymer with 1,3-benzenedicarboxylic acid, dimethyl ester, 1,4-cyclohexanedimethanol / \n1,4-benzenedicarboxylic acid, polymer with 1,3-benzenedicarboxylic acid, 1,4-cyclohexanedimethanol ",null,"245106-28-9\n26124-27-6","〇","〇","ー","〇","〇","Ⅲ",3,"酒類はアルコール濃度15％以下。"]
[1103,null,3,"テレフタル酸ジメチル・１，４－シクロヘキサンジメタノール・エチレングリコール共重合体／\nテレフタル酸・１，４－シクロヘキサンジメタノール・エチレングリコール共重合体","エチレングリコール・1,4-シクロヘキサンジメタノール・テレフタル酸またはテレフタル酸 ジメチル共重合体","1,4-benzenedicarboxylic acid, dimethyl ester, polymer with 1,4-cyclohexanedimethanol, and ethylene glycol / \n1,4-benzenedicarboxylic acid, polymer with 1,4-cyclohexanedimethanol, and ethylene glycol ",null,"0025640-14-6\n0025038-91-9","〇","〇","ー","〇","〇","Ⅱ",3,"１，４－シクロヘキサンジメタノール（CAS登録番号105-08-8）はジオール成分の50mol%以上。\n酒類はアルコール濃度25％以下。\nアルコール濃度13%を越える場合、使用可能温度は70℃以下。"]
[1104,null,4,"テレフタル酸ジメチル・１，４－シクロヘキサンジメタノール・２，２，４，４－テトラメチルシクロブタン－１，３－ジオール共重合体","1,4-シクロヘキサンジメタノール・2,2,4,4-テトラメチル-1,3-シクロブタンジオール・テレフタル酸 ジメチル共重合体","Polymer of dimethyl terephthalate, 1,4-cyclohexanedimethanol, and 2,2,4,4-tetramethyl-1,3-cyclobutanediol ",null,"0261716-94-3","〇","〇","ー","〇","〇","Ⅱ",3,"２，２，４，４－テトラメチルー１，３－シクロブタンジオール（CAS登録番号3010-96-6）はジオール成分に対して40mol%以下。\n無水トリメット酸（CAS登録番号552-30-7）を分岐剤としてポリマー構成成分に対して0.5重量%以下で使用可能。"]
[]
[null,null,"３０．ポリシクロへキシレンジメチレンナフタレート（PCN）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1110,null,1,"２，６－ナフタレンジカルボン酸ジメチル・１，４－シクロヘキサンジメタノール・エチレングリコール・スピログリコール共重合体",null,"2,6-Naphthalenedicarboxylic acid, 2,6-dimethyl ester, polymer with 1,4-cyclohexanedimethanol, 1,2-ethanediol, 2,2’-oxybis［ethanol］　and β,β,β’,β’-tetramethyl-2,4,8,10- tetraoxaspiro［5.5］undecane-3,9-diethanol",null,"2146168-28-5","〇","〇","〇","〇","〇","Ⅲ",3,"ジオール成分に対して１，４－シクロヘキサンジメタノール（CAS登録番号105-08-8）は45～55mol%、エチレングリコール（CAS登録番号107-21-1）は5～20mol%、スピログリコール（CAS登録番号1455-42-1）は30～40mol%。"]
[]
[null,null,"３１．ポリトリメチレンテレフタレート（PTT）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1226,null,1,"テレフタル酸ジメチル・１，３－プロパンジオール共重合体／\nテレフタル酸・１，３－プロパンジオール共重合体",null,"1,4-benzenedicarboxylic acid, dimethyl ester, polymer with 1,3-propanediol / \n1,4-benzenedicarboxylic acid, polymer with 1,3-propanediol",null,"36619-23-5 26590-75-0","〇","〇","〇","〇","〇","Ⅱ",3]
[]
[null,null,"３２．ポリブチレンテレフタレート（PBT)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1201,null,1,"テレフタル酸ジメチル・１，４－ブタンジオール共重合体／\nテレフタル酸・１，４-ブタンジオール共重合体",null,"1,4-Benzenedicarboxylic acid, polymer with 1,4-butanediol",null,"26062-94-2\n24968-12-5\n30965-26-5","○","○","○","○","○","Ⅲ",1]
[1198,null,2,"テレフタル酸ジメチル・イソフタル酸・１，４－ブタンジオール共重合体",null,"1,3-Benzenedicarboxylic acid,  polymer with 1,4-Benzenedicarboxylic acid, 1,4-dimethyl ester, and 1,4-butanediol",null,"36008-14-7","○","○","○","○","○","Ⅲ",1]
[1200,null,3,"テレフタル酸ジメチル・１，４－ブタンジオール・α－ヒドロ－ω－ヒドロキシポリ（オキシブタン－１，４－ジイル）ブロック共重合体",null,"1,4-Benzenedicarboxylic acid, dimethyl ester, polymer with 1,4-butanediol and, alpha, -hydro-, omega, -hydroxypoly(oxy-1,4-butanediyl)",null,"9078-71-1","○","○","○","○","○","Ⅲ",1,"ガラス転移温度、ボールプレッシャー温度等のいずれかが150℃以上。"]
[1197,null,4,"テレフタル酸ジメチル・イソフタル酸ジメチル・１，４－ブタンジオール・α－ヒドロ－ω－ヒドロキシポリ（オキシブタン－１，４－ジイル）ブロック共重合体",null,"1,3-Benzenedicarboxylic acid, polymer with  dimethyl 1,4-benzenedicarboxylate, 1,4-butanediol and .alpha.-hydro-.omega.-hydroxypoly(oxy-1,4-butanediyl)",null,"37282-15-8","○","○","○","○","○","Ⅲ",1,"ガラス転移温度、ボールプレッシャー温度等のいずれかが150℃以上。"]
[1195,null,5,"テレフタル酸・アジピン酸・１，４－ブタンジオール共重合体","アジピン酸・テレフタル酸・1,4-ブタンジオール共重合体","\n1,4-Benzenedicarboxylic acid, polymer with 1,4-butanediol and hexanedioic acid",null,"0060961-73-1","○","○","○","○","○","Ⅱ",3,"ガラス転移温度、ボールプレッシャー温度等のいずれかが150℃未満。"]
[1199,null,6,"テレフタル酸・セバシン酸・１，４－ブタンジオール共重合体","セバシン酸・テレフタル酸・1,4-ブタンジオール共重合体","\n1,4-Benzenedicarboxylic acid, polymer with 1,4-butanediol and decanedioic acid",null,"0028205-74-5","○","○","○","○","○","Ⅱ",3]
[1196,null,7,"アジピン酸・ブタン－１，４－ジオール・テレフタル酸重合物","アジピン酸・テレフタル酸・1,4-ブタンジオール共重合体","1,4-Benzenedicarboxylic acid, polymer with 1,4-butanediol and hexanedioic acid",null,"0060961-73-1","○","○","○","○","○","III",1,"ガラス転移温度、ボールプレッシャー温度等のいずれかが150℃以上。"]
[]
[null,null,"３３．ポリブチレンナフタレート（PBN）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1190,null,1,"２，６－ナフタレンジカルボン酸ジメチル・１，４－ブタンジオール共重合体／\n２，６－ナフタレンジカルボン酸・１，４－ブタンジオール共重合体",null,"2,6-Naphthalendicarboxylic acid, dimethyl ester, polymer with 1,4-butanediol / 2,6-Naphthalendicarboxylic acid, polymer with 1,4-butanediol",null,"30424-90-9\n28779-82-0","○","○","○","○","○","III",3]
[]
[null,null,"３４．ポリブチルサクシネート（PBS)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1184,null,1,"コハク酸・１，４－ブタンジオール共重合体",null,"Polybutylene succinate",null,"25777-14-4","〇","〇","〇","〇","〇","Ⅱ",3]
[1182,null,2,"コハク酸・アジピン酸・１，４－ブタンジオール共重合体",null,"Polybutylene succinate adipate",null,"67423-06-7","〇","〇","〇","〇","〇","Ⅰ",3]
[1183,null,3,"コハク酸・テレフタル酸・１，４－ブタンジオール共重合体",null,"Polybutylene succinate terephthalate",null,"144123-61-5","〇","〇","〇","〇","〇","Ⅱ",3]
[1185,null,4,"コハク酸・２，５－フランジカルボン酸・１，４－ブタンジオール共重合体",null,"Polybutylene succinate furanoate",null,"1392804-03-3","〇","〇","〇","〇","〇","Ⅱ",3]
[]
[null,null,"３５．ポリ乳酸（PLA)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1137,null,1,"ラクチド単独重合体",null,"Polylactide",null,"9051-89-2","○","○","〇","○","○","Ⅱ　　　　",3,"D-乳酸（CAS登録番号10326-41-7）含有率が6%以下のもの。\n当該物質を49％以下の割合として「スチレン単独重合体及び１，３－ブタジエン単独共重合体のスチレングラフト重合体の混合物」と混合する場合は、使用可能温度IIIで使用可能。\nエチレングリコールジメタクリレートを0.3%までの範囲で添加して架橋したものも含む。"]
[1138,null,2,"ラクチド単独重合体",null,"Polylactide",null,"9051-89-2","○","○","〇","○","○","Ⅱ  ",3,"D-乳酸（CAS登録番号10326-41-7）含有率が6%を超え16％以下のもの。\n40℃を超え66℃以下での使用は2時間以内。\n66℃を超え100℃以下での使用は30分以内。\nエチレングリコールジメタクリレートを0.3%までの範囲で添加して架橋したものも含む。"]
[]
[null,null,"３６．ポリヒドロキシ酪酸（PHB)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1143,null,1,"３－ヒドロキシ酪酸・３－ヒドロキシヘキサン酸共重合体",null,"Poly[oxy(1-methyl-3-oxapropan-1,3-diyl)/oxy(3-oxa-1-propylpropan-1,3-diyl)]",null,"147398-31-0\n198007-37-3","○","○","○","○","○","Ⅱ",3,"３－ヒドロキシヘキサン酸（CAS登録番号10191-24-9）はポリマー構成成分に対して20mol％以下。\n植物油脂を原料として微生物が産生したポリマーを含む。"]
[]
[null,null,"３７．ポリグリコール酸（PGA)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1097,null,1,"グリコール酸単独重合体",null,"Poly(glycolic acid)",null,"26124-68-5\n26009-03-0","○","○","○","○","○","Ⅱ",3,"PETに対し最大2.5重量%混合し使用する場合、または、PET層もしくはPLA層で分離し食品に接触しないように使用する場合に限る。\nPETに対し最大2.5重量%混合し使用する場合、酒類はアルコール濃度15%以下に限る。"]
[1096,null,2,"グリコール酸・イソフタル酸・トリメチロールプロパン共重合体",null,"Poly(glycolic acid-co-isophthalic acid-co-trimethylolpropane)",null,"26124-68-5\n2231246-33-4","○","○","○","○","○","Ⅱ",3]
[]
[null,null,"３８．ポリ塩化ビニリデン（PVDC)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1060,null,1,"塩化ビニリデン単独重合体",null,"Ethene, 1,1-dichloro-, homopolymer",null,"9002-85-1","○","○","○","○","○","Ⅲ",4]
[1059,null,2,"塩化ビニリデン・塩化ビニル共重合体",null,"Ethene, 1,1-dichloro-, polymer with chloroethene",null,"9011-06-7","○","○","○","○","○","Ⅲ",4]
[1056,null,3,"塩化ビニリデン・塩化ビニル・アクリロニトリル共重合体",null,"Vinyl chloride-Vinylidene chloride-Acrylonitrile copolymer",null,"28411-60-1","○","○","○","○","○","Ⅲ",4]
[1042,null,4,"塩化ビニリデン・塩化ビニル・アクリロニトリル・メタクリル酸メチル・アクリル酸・イタコン酸共重合体",null,"Polymer of 1,1-dichloroethene / vinyl chloride / acyrylonitrile / methyl methacrylate / acrylic acid / itaconic acid",null,"794518-22-2","○","○","○","○","○","Ⅲ",4]
[1054,null,5,"塩化ビニリデン・塩化ビニル・アクリル酸メチル共重合体",null,"2-Propenoic acid, methyl ester, polymer with chloroethene and 1,1-dichloroethene",null,"28572-91-0","〇","〇","○","〇","〇","Ⅲ",4]
[1057,null,6,"塩化ビニリデン・アクリロニトリル共重合体",null,"2-Propenenitrile, polymer with 1,1-dichloroethene",null,"9010-76-8","〇","〇","○","〇","〇","Ⅲ",4]
[1051,null,7,"塩化ビニリデン・アクリロニトリル・アクリル酸メチル共重合体",null,"Polymer of acrylonitrile / 1,1-dichloroethene / methyl acrylate",null,"24968-80-7","○","○","○","○","○","Ⅲ",4]
[1044,null,8,"塩化ビニリデン・アクリロニトリル・アクリル酸メチル・アクリル酸２－ヒドロキシエチル共重合体",null,"2-Propenoic acid, 2-hydroxyethyl ester, polymer with 1,1-dichloroethene, methyl 2-propenoate and 2-propenenitrile",null,"245118-21-2","〇","〇","○","〇","〇","Ⅲ",4]
[1046,null,9,"塩化ビニリデン・アクリロニトリル・アクリル酸メチル・アクリル酸ヒドロキシエチル・メタクリロニトリル共重合体",null,"Polymer of acrylonitrile / 1,1-dichloroethene / 2-hydroxyethyl acrylate / methyl acrylate / methacrylonitrile",null,"277747-97-4","○","○","○","○","○","Ⅲ",4]
[1045,null,10,"塩化ビニリデン・アクリロニトリル・アクリル酸メチル・アクリル酸ヒドロキシエチル・メタクリル酸メチル共重合体",null,"Polymer of 1,1-dichloethene / acrylonitrile / methyl methacrylate /2-propenoic acid, 2-hydroxyethyl ester /methyl acrylate",null,"794518-17-5","○","○","○","○","○","Ⅲ",4]
[1047,null,11,"塩化ビニリデン・アクリロニトリル・メタクリル酸メチル・アクリル酸ヒドロキシエチル・メタクリロニトリル・メタクリル酸共重合体",null,"Polymer of 1,1-dichloethene / acrylonitrile / methyl methacrylate /2-propenoic acid, 2-hydroxyethyl ester /   methacrylonitrile / methacrylic acid",null,"794518-16-4","○","○","○","○","○","Ⅲ",4]
[1050,null,12,"塩化ビニリデン・アクリロニトリル・アクリル酸ブチル共重合体",null,"2-Propenoic acid, butyl ester, polymer with 1,1-dichloroethene and 2-propenenitrile",null,"26300-99-2","〇","〇","○","〇","〇","Ⅲ",4]
[1055,null,13,"塩化ビニリデン・アクリル酸メチル共重合体",null,"2-Propenoic acid, methyl ester, polymer with 1,1-dichloroethene",null,"25038-72-6","〇","〇","○","〇","〇","Ⅲ",4]
[1048,null,14,"塩化ビニリデン・アクリル酸メチル・アクリル酸ブチル共重合体",null,"2-Propenoic acid, butyl ester, polymer with 1,1-dichloroethene and methyl 2-propenoate",null,"25988-90-3","〇","〇","○","〇","〇","Ⅲ",4]
[1062,null,15,"塩化ビニリデン・メタクリロニトリル・メタクリル酸メチル共重合体",null,"2-Propenoic acid, 2-methyl-, methyl ester, polymer with 1,1-dichloroethene and 2-methyl-2-propenenitrile",null,"32335-23-2","〇","〇","○","〇","〇","Ⅲ",4]
[1043,null,16,"塩化ビニリデン・アクリロニトリル・アクリル酸エチル共重合体","アクリル酸 エチル・アクリロニトリル・塩化ビニリデン共重合体","2-Propenoic acid, ethyl ester, polymer with 1,1-dichloroethene and 2-propenenitrile",null,"0029295-71-4","○","○","○","○","○","Ⅲ",4]
[1049,null,17,"塩化ビニリデン・アクリル酸メチル・アクリル酸ブチル・メタクリル酸メチル共重合体","アクリル酸 ブチル・アクリル酸 メチル・塩化ビニリデン・メタクリル酸 メチル共重合体","2-Propenoic acid, 2-methyl-, methyl ester, polymer with 1,1-dichloroethene, 2-Propenoic acid, methyl ester and 2-Propenoic acid, butyl ester",null,"0277747-96-3","○","○","○","○","○","Ⅲ",4]
[1053,null,18,"塩化ビニリデン・アクリロニトリル・アクリル酸メチル・メタクリロニトリル共重合体","アクリル酸メチル・アクリロニトリル・塩化ビニリデン・メタクリロニトリル共重合体","Polymer of acrylonitrile / 1,1-dichloroethene / methyl acrylate / methacrylonitrile",null,"－","○","○","○","○","○","Ⅲ",4]
[1052,null,19,"塩化ビニリデン・アクリロニトリル・アクリル酸メチル・メタクリル酸メチル共重合体","アクリル酸 メチル・アクリロニトリル・塩化ビニリデン・メタクリル酸 メチル共重合体","Polymer of 1,1-dichloethene / acrylonitrile / methyl methacrylate / methyl acrylate",null,"－","○","○","○","○","○","Ⅲ",4]
[1058,null,20,"塩化ビニリデン・アクリロニトリル・メタクリル酸メチル・メタクリロニトリル・メタクリル酸共重合体","アクリロニトリル・塩化ビニリデン・メタクリル酸・メタクリル酸 メチル・メタクリロニトリル共重合体","Polymer of 1,1-dichloethene / acrylonitrile / methyl methacrylate / methacrylonitrile / methacrylic acid",null,"－","○","○","○","○","○","Ⅲ",4]
[1063,null,21,"塩化ビニリデン・メタクリロニトリル共重合体","塩化ビニリデン・メタクリロニトリル共重合体","2-methyl-2-propenenitrile, polymer with 1,1-dichloroethene",null,"0009010-80-4","〇","〇","○","〇","〇","Ⅲ",4]
[1061,null,22,"塩化ビニリデン・メタクリル酸メチル共重合体","塩化ビニリデン・メタクリル酸 メチル共重合体","2-Propenoic acid, 2-methyl-, methyl ester, polymer with 1,1-dichloroethene",null,"0025120-29-0","〇","〇","○","〇","〇","Ⅲ",4]
[]
[null,null,"３９．ポリ塩化ビニル（PVC)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1078,null,1,"塩化ビニル単独重合体",null,"Polyvinyl Chloride",null,"9002-86-2","○","○","○","○","○","Ⅲ",4]
[1079,null,2,"塩化ビニル単独重合体塩素化物",null,"Ethene, chloro-, homopolymer, chlorinated",null,"68648-82-8","〇","○","○","〇","〇","Ⅲ",4,"塩素はポリマー構成成分に対して69重量%以下。"]
[1075,null,3,"塩化ビニル・酢酸ビニル共重合体",null,"Acetic acid ethenyl ester, polymer with chloroethene",null,"9003-22-9","〇","○","○","〇","〇","Ⅲ",4]
[1076,null,4,"塩化ビニル・酢酸ビニル・フマル酸共重合体",null,"2-Butenedioic acid, (E)-, polymer with chloroethene and ethenyl acetate",null,"32650-26-3","〇","○","○","〇","〇","Ⅲ",4]
[1070,null,5,"塩化ビニル・酢酸ビニル・２－ヒドロキシプロピルアクリレート共重合体",null,"2-Propenoic acid, 2-hydroxypropyl ester, polymer with\nchloroethene and ethenyl acetate",null,"41618-91-1\n39317-41-4","〇","○","○","〇","〇","Ⅲ",4]
[1073,null,6,"塩化ビニル・エチレン共重合体",null,"Vinyl chloride-ethylene copolymer",null,"25037-78-9","○","○","○","○","○","Ⅲ",4]
[1074,null,7,"塩化ビニル・エチレン・酢酸ビニル共重合体",null,"Copolymer of ethylene,vinyl chloride and vinyl acetate",null,"25085-46-5","○","○","○","○","○","Ⅲ",4,"塩化ビニル（CAS登録番号75-01-4）はポリマー構成成分に対して50重量%以上。"]
[1071,null,8,"塩化ビニル・アクリル酸ブチル共重合体",null,"2-Propenoic acid, butyl ester, polymer with chloroethene",null,"25702-34-5","〇","○","○","〇","〇","Ⅲ",4]
[1080,null,9,"塩化ビニル・酢酸ビニル共重合体部分ケン化物\n（塩化ビニル・酢酸ビニル・ビニルアルコール共重合体）",null,"Partially hydrolyzed copolymer of vinyl chloride and vinyl acetate",null,"25086-48-0","〇","○","○","〇","〇","Ⅲ",4,"塩化ビニル（CAS登録番号75-01-4）はポリマー構成成分に対して50重量%以上。"]
[1068,null,10,"塩化ビニル・酢酸ビニル・アクリル酸共重合体","アクリル酸・塩化ビニル・酢酸 ビニル共重合体","Acrylic acid polymer with chloroethene and ethenyl acetate",null,"0029035-81-2","○","○","○","○","○","III",4]
[1072,null,11,"塩化ビニル・酢酸ビニル・イタコン酸共重合物","イタコン酸・塩化ビニル・酢酸 ビニル共重合体","Copolymer of vinyl chloride, vinyl acetate and itaconic acid",null,"0028086-69-3","○","○","○","○","○","III",4]
[1069,null,12,"塩化ビニル・２－ヒドロキシプロピルアクリレート共重合物","アクリル酸 2-ヒドロキシプロピル・塩化ビニル共重合体","2-Propenoic acid, 2-hydroxypropyl ester, polymer with chloroethene",null,"0053710-52-4","○","○","○","○","○","III",4]
[1077,null,13,"塩化ビニル・酢酸ビニル・ラウリン酸ビニル共重合物","塩化ビニル・酢酸 ビニル・ラウリン酸 ビニル共重合体","Copolymer of vinyl chloride, vinyl acetate and vinyl laurate",null,"0025155-88-8","○","○","○","○","○","III",4]
[]
[null,null,"４０．塩素化ポリエチレン"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[288,null,1,"エチレン単独重合体の塩素化物",null,"Chlorinated ethylene homopolymer",null,"64754-90-1","○","－","－","○","○","Ⅰ",2,"塩素はポリマー構成成分に対して65重量%以下\n区分４との混合（５％以下）では、使用可能食品は全食品、使用可能温度はⅢ"]
[]
[null,null,"４１．塩素化ポリプロピレン"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[293,null,1,"プロピレン単独重合体の塩素化物",null,"Chlorinated propylene homopolymer",null,"68442-33-1","○","○","○","○","○","Ⅰ",2,"塩素はポリマー構成成分に対して56%重量以下。"]
[]
[null,null,"４２．フッ素樹脂（FR）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[864,null,1,"テトラフルオロエチレン単独重合体（PTFE）",null,"Ethene, tetrafluoro-, homopolymer",null,"9002-84-0","○","○","○","○","○","Ⅲ",1]
[874,null,2,"テトラフルオロエチレン・ヘキサフルオロプロピレン共重合体（FEP）",null,"1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with tetrafluoroethene",null,"25067-11-2","○","○","○","○","○","Ⅲ",1]
[872,null,3,"１，１，２，２－テトラフルオロエテン・３，３，４，４，５，５，６，６，６－ノナフルオロー１－ヘキセン共重合体",null,"1-hexene,3,3,4,4,5,5,6,6,6-nonafluoro-, polymer with 1,1,2,2-tetrafluoroethene",null," 82606-24-4","○","○","○","○","○","Ⅲ",1]
[866,null,4,"テトラフルオロエチレン・パーフルオロメチルビニルエーテル共重合体（MFA）",null,"Ethene, 1,1,2,2-tetrafluoro-, polymer with 1,1,2-trifluoro-2-(trifluoromethoxy)ethene",null,"26425-79-6","○","○","○","○","○","Ⅲ",1]
[867,null,5,"テトラフルオロエチレン・パーフルオロメチルビニルエーテル・パーフルオロプロピルビニルエーテル共重合体",null,"Propane, 1,1,1,2,2,3,3-heptafluoro-3-[(1,2,2-trifluoroethenyl)oxy]-, polymer with 1,1,2,2-tetrafluoroethene and 1,1,2-trifluoro-2-(trifluoromethoxy)ethane",null,"165178-32-5 ","○","○","○","○","○","Ⅲ",1]
[870,null,6,"テトラフルオロエチレン・パーフルオロエチルビニルエーテル\n共重合体（TFE/C2VE）",null,"Pentafluoroethyl trifluorovinyl ether, polymer with tetrafluoroethylene",null,"31784-04-0","○","○","○","○","○","Ⅲ",1]
[871,null,7,"テトラフルオロエチレン・パーフルオロエチルビニルエーテル・ヘキサフルオロプロペン共重合体（TFE/HFP/C2VE）",null,"Copolymer of hexafluoropropylene, tetrafluoroethene\nand perfluoroethyl vinyl ether",null,"63654-40-0","○","○","○","○","○","Ⅲ",1]
[868,null,8,"テトラフルオロエチレン・パーフルオロプロピルビニルエーテル共重合体（PFA）",null,"Propane, 1,1,1,2,2,3,3-heptafluoro-3-[(trifluoroethenyl)oxy]-, polymer with tetrafluoroethene",null,"26655-00-5","○","○","○","○","○","Ⅲ",1]
[869,null,9,"テトラフルオロエチレン・パーフルオロプロピルビニルエーテル・５－ノルボルネン－２，３－ジカルボン酸無水物共重合体（PFA）",null,"Copolymer of perfluoroethene, 1,1,2-trifluoro-2-(1,1,2,2,3,3,3-heptafluoropropoxy) ethane, and 5-norbornene-2,3-dicarboxylic anhydride",null,"885121-25-5","○","○","○","○","○","Ⅲ",1]
[856,null,10,"テトラフルオロエチレン・エチレン共重合体（ETFE）",null,"Ethene,polymer with 1,1,2,2-tetrafluoroethene",null,"25038-71-5","○","○","○","○","○","Ⅲ",1]
[857,null,11,"エテン・３，３，４，４，５，５，６，６，６－ノナフルオロヘキサ－１－エン・ペルフルオロエテン共重合体（ETFE）",null,"1-Hexene, 3,3,4,4,5,5,6,6,6-nonafluoro-, polymer with ethene and 1,1,2,2-tetrafluoroethene",null,"68258-85-5","○","○","○","○","○","Ⅲ",1]
[859,null,12,"エテン・ペルフルオロエテン・３，３，４，４，４－ペンタフルオロブテン・３，４－ジヒドロ－３－メチレン－２，５－フランジオン共重合体（ETFE）",null,"3,3,4,4,4-pentafluoro butene, polymer with 3,4-Dihydro-3-methylene-2,5-furandione,   ethene , and 1,1,2,2-tetrafluoroethene",null,"583827-65-0","○","○","○","○","○","Ⅲ",1]
[855,null,13,"エテン・ペルフルオロエテン・ヘキサフルオロプロペン・３，３，４，４，５，５，６，６，６－ノナフルオロヘキサ－１－エン・３，４－ジヒドロ－３－メチレン－２，５－フランジオン共重合体",null,"Hexafluoropropene, polymer with 3,3,4,4,5,5,6,6,6-nonafluorohex-1-en, 3,4-Dihydro-3-methylene-2,5-furandione, ethene and 1,1,2,2-tetrafluoroethene",null,"676617-51-9","○","○","○","○","○","Ⅲ",1]
[865,null,14,"テトラフルオロエチレン・スルホニルビニルエーテルパーフルオルレート共重合体",null,"Ethene, 1,1,2,2-tetrafluoro-, polymer with 1,1,2,2-tetrafluoro-2-((1,2,2-trifluoroethenyl)oxy)ethanesulfonyl fluoride (The polymer is hydrolyzed and may optionally be further neutralized to its ammonium salt.)",null,"111173-25-2","○","○","ー","○","○","Ⅲ",1,"加水分解及びアンモニウム塩中和物を含む。"]
[875,null,15,"フッ化ビニリデン単独重合体（PVDF）",null,"Ethene, 1,1-difluoro-, homopolymer",null,"24937-79-9","○","○","○","○","○","Ⅲ",1]
[873,null,16,"フッ化ビニリデン・テトラフルオロエチレン共重合体（VDF/TFE）",null,"Ethene, 1,1,2,2-tetrafluoro-, polymer with 1,1-difluoroethene",null,"25684-76-8","○","○","○","○","○","Ⅲ",1]
[876,null,17,"フッ化ビニリデン・ヘキサフルオロプロピレン共重合体（VDF/HFP）",null,"1-Propene, 1,1,2,3,3,3-hexafluoro-, polymer with 1,1-difluoroethene",null,"9011-17-0","○","○","○","○","○","Ⅲ",1]
[863,null,18,"フッ化ビニリデン・クロロトリフルオロエチレン共重合体（VDF/CTFE）",null,"Chlorotrifluoroethene polymer with 1,1-difluoroethene",null,"9010-75-7","○","○","○","○","○","Ⅲ",1]
[877,null,19,"フッ化ビニル単独重合体（PVF）",null,"Ethene, fluoro-, homopolymer",null,"24981-14-4","○","○","ー","○","○","Ⅰ",1]
[860,null,20,"クロロトリフルオロエチレン単独重合体（PCTFE）",null,"Chlorotrifluoroethene- homopolymer",null,"9002-83-9","○","○","○","○","○","Ⅲ",1]
[861,null,21,"クロロトリフルオロエチレン・テトラフルオロエチレン共重合体（CTFE/TFE）",null,"Ethene, chlorotrifluoro-, polymer with tetrafluoroethene",null,"25038-89-5","○","○","○","○","○","Ⅲ",1]
[862,null,22,"クロロトリフルオロエチレン・フッ化ビニリデン・テトラフルオロエチレン共重合体（CTFE/VDF/TFE）",null,"Ethene, 1,1-difluoro-, polymer with chlorotrifluoroethene and tetrafluoroethene",null,"30421-59-1","○","○","○","○","○","Ⅲ",1]
[854,null,23,"クロロトリフルオロエチレン・エチレン共重合体（CTFE/E）",null,"Ethene, 1-chloro-1,2,2-trifluoro-, polymer with ethene",null,"25101-45-5","○","○","○","○","○","Ⅲ",1]
[858,null,24,"エテン・ペルフルオロエテン・3,3,4,4,4ペンタフルオロブテン共重合物","エチレン・テトラフルオロエチレン・3,3,4,4,4ペンタフルオロブテン共重合体","3,3,4,4,4-pentafluoro butene, polymer with ethene and Tetrafluoroethylene",null,"0460314-45-8","○","○","○","○","○","III",1]
[]
[null,null,"４３．ポリアセタール（POM)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[894,null,1,"ホルムアルデヒド単独重合体",null,"Formaldehyde homopolymer\n(Polyoxymethylene homopolymer) ",null,"9002-81-7\n25231-38-3\n30525-89-4","○","○","○","○","○","Ⅱ",1]
[890,null,2,"1，３，５－トリオキサン・エチレンオキサイド共重合体",null,"1,3,5-Trioxane, polymer with oxirane",null,"24969-25-3","○","○","○","○","○","Ⅱ",1,"エチレンオキサイド（CAS登録番号75-21-8）はポリマー構成成分に対して６重量%以下。"]
[892,null,3,"1，３，５－トリオキサン・1，３－ジオキソラン共重合体",null,"1,3,5-Trioxane, polymer with 1,3-dioxolane",null,"24969-26-4","○","○","○","○","○","Ⅱ",1,"1，３－ジオキソラン（CAS登録番号646-06-0）はポリマー構成成分に対して６重量%以下。"]
[893,null,4,"1，３，５－トリオキサン・1，３－ジオキソラン・１，４－ブタンジオールジグリシジルエーテル共重合体",null,"1,3,5-Trioxane, polymer with 2,2'-[1,4-butanediylbis(oxymethylene)]bis[oxirane] and 1,3-dioxolane",null,"41258-95-1","○","○","○","○","○","Ⅱ",1,"1，３－ジオキソラン（CAS登録番号646-06-0）及び１，４－ブタンジオールジグリシジルエーテル（CAS登録番号2425-79-8）はポリマー構成成分に対して合計で６重量%以下。"]
[891,null,5,"1，３，５－トリオキサン・ブタンジオールホルマール共重合体",null,"1,3-Dioxepane, polymer with 1,3,5-trioxane",null,"25214-85-1","○","○","○","○","○","Ⅱ",1,"ブタンジオールホルマール（CAS登録番号505-65-7）はポリマー構成成分に対して６重量%以下。"]
[]
[null,null,"４４．ポリエーテルエーテルケトン（PEEK)　"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[958,null,1,"４，４'－ジフルオロベンゾフェノン・ハイドロキノン共重合体",null,"Methanone, bis(4-fluorophenyl)-, polymer with 1,4-benzenediol",null,"29658-26-2\n31694-16-3","○","○","○","○","○","Ⅲ",1]
[]
[null,null,"４５．ポリエーテルケトン（PEK)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[963,null,1,"４，４'－ジフルオロベンゾフェノン・４，４'－ジヒドロキシベンゾフェノン共重合体",null,"Methanone, bis(4-fluorophenyl)-, polymer with bis(4-hydroxyphenyl)methanone",null,"27380-27-4 75467-54-8","○","○","○","○","ー","Ⅲ\n（酒類のみⅡ）",1]
[]
[null,null,"４６．ヒドロキシ安息香酸ポリエステル（HBP)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[835,null,1,"４，４’－ジヒドロキシビフェニル・４－ヒドロキシ安息香酸・テレフタル酸・イソフタル酸共重合体",null,"1,3-Benzenedicarboxylic acid, polymer with 1,4-benzenedicarboxylic acid, [1,1'-biphenyl]-4,4'-diol and 4-hydroxybenzoic acid",null,"60088-52-0","○","○","○","○","○","Ⅲ",1]
[836,null,"2","4,4-ビフェニルジオール・ヒドロキノン・p-ヒドロキシ安息香酸・2,6-ナフタレンカルボン酸・テレフタル酸重縮合物",null,"A copolymer of hydroquinone, terephthalic acid, 2,6-naphthalenedicarboxylic acid, 4- hydroxybenzoic acid, and optionally 4,4'-biphenol",null,"126710-21-2","〇","〇","〇","〇","〇","Ⅲ","1"]
[837,null,"3","４，４’－ジヒドロキシ－ジ－フェニル・４－ヒドロキシ安息香酸・ヒドロキシナフトエ酸・４’－ヒドロキシアセトアニリド・テレフタル酸重縮合物",null,"1,4-Benzenedicarboxylic acid polymer with [1,1'-biphenyl]-4,4'-diol, 4-hydroxy benzoic acid, 6-hydroxy-2-naphthalenecarboxylic acid and N-(4-hydroxyphenyl)acetamide",null,"147310-94-9","〇","〇","〇","〇","〇","Ⅱ","1","少なくとも55モル％のポリマー単位が6-ヒドロキシ-2-ナフトエ酸及び4-ヒドロキシ安息香酸との組み合わせで構成され、ポリマー単位の25モル％以下が4,4‘-ビフェノール、N-(4-ヒドロキシフェニル)アセトアミド及びテレフタル酸で構成される。"]
[838,null,"4","４，４’－ジヒドロキシ－ジ－フェニル・４－ヒドロキシ安息香酸・ヒドロキシナフトエ酸・テレフタル酸重縮合物",null,"1,4-Benzenedicarboxylic acid polymer with [1,1'-biphenyl]-4,4'-diol, 4-hydroxybenzoic acid and 6-hydroxy-2-naphthalenecarboxylic acid",null,"122122-87-6","〇","〇","〇","〇","〇","Ⅱ","1","少なくとも55モル％のポリマー単位が6-ヒドロキシ-2-ナフトエ酸及び4-ヒドロキシ安息香酸との組み合わせで構成され、ポリマー単位の25モル％以下が4,4‘-ビフェノール、及びテレフタル酸で構成される。"]
[839,null,"5","ｐ－ヒドロキシ安息香酸・６－ヒドロキシ－２－ナフトエ酸重縮合物",null,"Polymer(p-hydroxybenzoic acid/6-hydroxy-2-naphthoic acid)",null,"81843-52-9","〇","〇","〇","〇","〇","Ⅱ","1"]
[]
[null,null,"４７．ポリアミドイミド（PAI)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[934,null,1,"無水トリメリット酸クロライド・４，４’－メチレンビスベンゼンアミン共重合体",null,"Polymer of 4,4’-methylenebis[benzenamine] and 1,3-dihydro-1,3-dioxo-5-isobenzofurancarbonyl chloride",null,"31957-38-7","○","○","○","○","○","Ⅲ",1]
[933,null,2,"無水トリメリット酸・４，４’－ジフェニルメタンジイソシアネート共重合体",null,"5-Isobenzofurancarboxylic acid, 1,3-dihydro-1,3-dioxo-, polymer with 1,1'-methylenebis[4-isocyanatobenzene]",null,"25053-57-0","○","○","ー","○","○","Ⅲ",1]
[]
[null,null,"４８．ポリフェニレンエーテル（PPE)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1171,null,1,"２，６－ジメチルフェノール単独重合体",null,"Phenol, 2,6-dimethyl-, homopolymer",null,"25134-01-4","○","○","○","○","○","Ⅲ",1]
[1172,null,2,"２，６－ジメチルフェノール・２，３，６－トリメチルフェノール共重合体",null,"Copolymer of 2,6-xylenol and 2,3,6-trimethylphenol",null,"58295-79-7","○","○","○","○","○","Ⅲ",1]
[]
[null,null,"４９．ポリフェニレンサルファイド（PPS)",null,"ポリフェニルスルフィド（PPS）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1161,null,1,"１，４－ジクロロベンゼン・硫化ナトリウム共重合体",null,"Benzene, 1,4-dichloro-, polymer with sodium sulfide (Na2S)",null,"26125-40-6\n25212-74-2","○","○","○","○","○","Ⅲ",1,"酸素存在下の熱架橋反応生成物（酸化架橋型）を含む"]
[1160,null,2,"１，４－ジクロロベンゼン・１，２，４－トリクロロベンゼン・硫化ナトリウム共重合体",null,"Benzene, trichloro-, polymer with 1,4-dichlorobenzene and sodium sulfide (Na2S)",null,"72276-00-7","○","○","○","○","○","Ⅲ",1]
[1159,null,3,"１，４－ジヨードベンゼン・硫黄共重合体",null,"Benzene, 1,4-diiodo-, polymer with sulfur",null,"25212-74-2","○","○","○","○","○","Ⅲ",1]
[]
[null,null,"５０．ポリカーボネート（PC)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1087,null,1,"２，２－ビス（４－ヒドロキシフェニル）プロパン・塩化カルボニル共重合体",null,"Carbonic dichloride, polymer with 4,4'-(1-methylethylidene)bis[phenol]",null,"25971-63-5\n103598-77-2\n111211-39-3 \n24936-68-3","○","○","○","○","○","Ⅲ",1]
[1090,null,2,"２，２－ビス（４－ヒドロキシフェニル）プロパン・ジフェニルカーボネート共重合体",null,"Carbonic acid, diphenyl ester, polymer with 4,4'-(1-methylethylidene)bisphenol",null,"25929-04-8\n24936-68-3","○","○","○","○","○","Ⅲ",1]
[1085,null,3,"２，２－ビス（４－ヒドロキシフェニル）プロパン・塩化カルボニル・セバシン酸共重合体",null,"Sebacic acid , polymers with bisphenol A, carbonic dichloride and 4-(1-methyl-1-phenylethyl)phenol",null,"137397-37-6","○","○","○","○","○","Ⅲ",1]
[1088,null,4,"２，２－ビス（４－ヒドロキシフェニル）プロパン・塩化カルボニル・４，４’－シクロヘキサン－１，１－ジイルビス（２－メチルフェノール）共重合体",null,"Carbonic dichloride, polymer with 4,4'-cyclohexylidenebis[2-methylphenol] and 4,4'-(1- methylethylidene)bis[phenol], bis[4-(1-methyl-1-phenylethyl)phenyl] ester",null,"411234-34-9","○","○","○","○","○","Ⅱ",1]
[1089,null,5,"２，２－ビス（４－ヒドロキシフェニル）プロパン・塩化カルボニル・３，３－ビス（４－ヒドロキシフェニル）－２－フェニルイソインドリン－１－オン共重合体",null,"Carbonic dichloride, polymer with 2,3-dihydro-3,3-bis(4-hydroxyphenyl)-2-phenyl-1-H-isoindol-1-one and 4,4’-(1-methylethylidene)bis[phenol], bis[4-(1-methyl-1-phenylethyl)phenyl] ester",null,"503834-43-3","○","○","○","○","○","Ⅲ",1]
[1091,null,6,"２，２－ビス（４－ヒドロキシフェニル）プロパン・塩化カルボニル・α－ジメチル－３－（４’－ヒドロキシ－３’－メトキシフェニル）プロピルシリルオキシ－ω－３－ジメチル－３－（４’－ヒドロキシ－３’－メトキシフェニル）プロピルシリルポリジメチルシロキサン共重合体",null,"Siloxanes and silicones, di-methyl, 3-(4-hydroxy-3-methoxy-3-methoxyphenyl)propyl group-terminated, polymers with bisphenol A, carbonic dichloride and 4-(1-methyl-1-phenylethyl)phenol",null,"202483-49-6","○","○","○","○","○","Ⅱ",1,"シロキサン変成部分はポリマー構成成分に対して22重量%以下。\nα－ジメチル－３－（４’－ヒドロキシ－３’－メトキシフェニル）プロピルシリルオキシ－ω－３－ジメチル－３－（４’－ヒドロキシ－３’－メトキシフェニル）プロピルシリルポリジメチルシロキサン（CAS登録番号156065-00-8）C24H38Si2O5(SiOC2H6)n は 26≦ n ＜50。"]
[1086,null,7,"２，２－ビス（４－ヒドロキシフェニル）プロパン・塩化カルボニル・４，４’，４’’－エチリジントリスフェノール共重合体","塩化カルボニル・1,1,1-トリス(4-ヒドロキシフェニル)エタン・ビスフェノール A共重合体","Carbonic dichloride, polymer with 4,4',4''-ethylidynetris phenol and 4,4'-(1-methyl-ethylidene)bis[phenol]",null,"0131600-85-6\n0156042-30-7","○","○","ー","○","○","III",1]
[]
[null,null,"５１．ポリエステルカーボネート（PPC)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[977,null,1,"２，２－ビス（４－ヒドロキシフェニル）プロパン・塩化カルボニル・テレフタル酸クロライド・イソフタル酸クロライド共重合体",null,"1,3-Benzenedicarbonyl dichloride, polymer with 1,4-benzenedicarbonyl dichloride, carbonic dichloride and 4,4-(1-methylethylidene)bisphenol",null,"71519-80-7\n114096-64-9","○","○","○","○","○","Ⅲ",1,"ｐ－クミルフェノール（CAS登録番号599-64-4）により末端封止されたものを含む。\n\n２，２－ビス（４－ヒドロキシフェニル）プロパン（CAS登録番号80-05-7）及びテレフタル酸クロライド（CAS登録番号100-20-9）又はイソフタル酸クロライド（CAS登録番号99-63-8）のエステル（以下、エステル）はポリマー構成成分全体に対して45～85mol%、エステルを構成する酸成分に対して、テレフタル酸クロライドは55mol%以上。"]
[976,null,2,"２，２－ビス（４－ヒドロキシフェニル）プロパン・塩化カルボニル・テレフタル酸クロライド・イソフタル酸クロライド・レソルシノール共重合体",null,"1,3-Benzenedicarbonyl dichloride, polymer with 1,4-benzenedicarbonyl dichloride, 1,3-benzenediol, carbonic dichloride and 4,4'-(1-methylethylidene)bisphenol, 4-(1-methyl-1-phenylethyl)phenyl ester",null,"235420-85-6","○","○","○","○","○","Ⅱ",1,"ｐ－クミルフェノール（CAS登録番号599-64-4）により末端封止されたものを含む。"]
[]
[null,null,"５２．ポリアリレート（PAR)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[939,null,1,"２，２－ビス（４－ヒドロキシフェニル）プロパン・テレフタル酸クロライド・イソフタル酸クロライド共重合体",null,"1,3-Benzenedicarbonyl dichloride, polymer with 1,4-benzenedicarbonyl dichloride and 4,4'-(1-methylethylidene)bis[phenol]",null,"26590-50-1\n25639-68-3","○","○","○","○","○","Ⅲ",1]
[940,null,2,"4-tert-ブチルフェノールで末端封止された２，２－ビス（４－ヒドロキシフェニル）プロパン・テレフタル酸クロライド・イソフタル酸クロライド共重合体","4-t-ブチルフェノールで末端処理されたイソフタル酸クロライド・テレフタル酸クロライド・ビスフェノール A共重合体","1,3-Benzenedicarbonyl dichloride, polymer with 1,4-benzenedicarbonyl dichloride and 4,4'-(1-methylethylidene)bis[phenol],4-tert-butylphenol-terminated",null,"－","○","○","○","○","○","Ⅲ",1]
[]
[null,null,"５３．ポリエーテルイミド（PEI)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[953,null,1,"２，２－ビス（４－ヒドロキシフェニル）プロパン・無水フタル酸・１，３－ベンゼンジアミン共重合体",null,"1,3-Isobenzofurandione, 5,5'-[(1-methylethylidene)bis(4,1-phenyleneoxy)]bis-, polymer with 1,3-benzenediamine",null,"61128-46-9","○","○","○","○","○","Ⅲ",1]
[952,null,2,"２，２－ビス（４－ヒドロキシフェニル）プロパン・４－クロロ無水フタル酸・３－クロロ無水フタル酸・１，３－ベンゼンジアミン共重合体",null,"1,3-Isobenzofurandione, 5,5'-[(1-methylethylidene)bis(4,1-phenyleneoxy)]bis-, polymer with 1,3-benzenediamine",null,"536741-00-1","○","○","○","○","○","Ⅲ",1]
[951,null,3,"２，２－ビス（４－ヒドロキシフェニル）プロパン・無水フタル酸・４，４’－スルホニルビスベンゼンアミン共重合体",null,"1,3-Isobenzofurandione, 5,5 -[(1-Methylethylidene)Bis(4,1-Phenyleneoxy)]Bis-, polymer with 4,4 –Sulfonyldianiline",null,"77699-82-2","○","○","○","○","○","Ⅲ",1]
[]
[null,null,"５４．ポリイミド（PI)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[945,null,1,"4,4’-ジアミノジフェニルエーテル・無水ピロメリット酸共重合体",null,"4,4'-Diaminodiphenyl ether-Pyromellitic anhydride polycondensate",null,"25038-81-7","○","○","○","○","○","Ⅲ",1," "]
[946,null,2,"ビス[4-(アリルビシクロ[2,2,1]ヘプト-5-エン-2,3-ジカルボキシイミ ド)フェニル]メタン","ビス[4-(アリルビシクロ[2,2,1]-5-ヘプテン-2,3-ジカルボキシイミド)フェニル]メタン単独共重合体","Bis{4-(arylbicyclo[2.2.1]hepto-5-ene-2,3-dicarboxyimide)phenyl} metane",null,"0091865-54-2","○","○","○","○","○","Ⅲ",1]
[]
[null,null,"５５．ポリサルホン（PSU)",null,"ポリスルホン（PSU）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1132,null,1,"４，４’－ジクロロジフェニルサルホン・２，２－ビス（４－ヒドロキシフェニルプロパン）共重合体","4,4'-ジクロロジフェニルスルホン・ビスフェノール A共重合体","Phenol, 4,4'-(1-methylethylidene)bis-, polymer with 1,1'-sulfonylbis[4-chlorobenzene]",null,"25154-01-2","○","○","○","○","○","Ⅲ",1]
[]
[null,null,"５６．ポリエーテルサルホン（PESU)",null,"ポリエーテルスルホン（PESU）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[968,null,1,"４，４’－ジクロロジフェニルサルホン・４，４’－ジヒドロキシジフェニルサルホン共重合体","4,4'-ジクロロジフェニルスルホン・4,4'-ジヒドロキシジフェニルスルホン共重合体","Phenol, 4,4'-sulfonylbis-, polymer with 1,1'-sulfonylbis[4-chlorobenzene]",null,"25608-63-3\n25667-42-9","○","○","○","○","○","Ⅲ",1]
[971,null,2,"ヒドロキノン・4,4’－ジクロルジフェニルスルホン・4,4’－ジヒドロキシジフェニルスルホン重縮合物のスルホン化ナトリウム塩化物","スルホン化処理された4,4'-ジクロロジフェニルスルホン・4,4'-ジヒドロキシジフェニルスルホン・ヒドロキノン共重合体のナトリウム塩","A sodium salt of sulfonated polycondensate of Bisphenol-S with 4,4'-dichlorodiphenyl sulphone and 1,4-dihydroxybenzene.",null,"1310712-40-3","○","○","○","○","○","Ⅲ",1,"　"]
[969,null,3,"4,4’－ジクロロジフェニルスルホン・4,4’－ジヒドロキシジフェニルスルホン重縮合物のスルホン化物","スルホン化処理された4,4'-ジクロロジフェニルスルホン・4,4'-ジヒドロキシジフェニルスルホン共重合体","A sulfonated polycondensate of Bisphenol-S with 4,4'-dichlorodiphenyl sulphone.",null,"2024597-27-9","○","○","○","○","○","Ⅲ",1,"　"]
[970,null,4,"4,4’－ジクロロジフェニルスルホン・4,4’－ジヒドロキシジフェニルスルホン重縮合物のスルホン酸ナトリウム塩","スルホン化処理された4,4'-ジクロロジフェニルスルホン・4,4'-ジヒドロキシジフェニルスルホン共重合体のナトリウム塩","A sodium salt of sulfonated polycondensate of Bisphenol-S with 4,4'-dichlorodiphenyl sulphone.",null,"2306446-18-2","○","○","○","○","○","Ⅲ",1,"　"]
[]
[null,null,"５７．ポリフェニルサルホン（PPSU)",null,"ポリフェニルスルホン（PPSU）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1166,null,1,"４，４’－ジクロロジフェニルサルホン・４，４’－ジヒドロキシビフェニル共重合体","4,4'-ジクロロジフェニルスルホン・4,4'-ジヒドロキシビフェニル共重合体","[1,1'-Biphenyl]-4,4'-diol, polymer with 1,1'-sulfonylbis[4-chlorobenzene]",null,"25608-64-4\n25839-81-0","○","○","○","○","○","Ⅲ",1]
[]
[null,null,"５８．熱可塑性ポリウレタン（TPU)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS No","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[null,null,1,"下記のジイソシアネート及び下記のモノマーからなるポリエステルポリオールの共重合体",null,null,null,null,"〇","〇","〇","〇","〇","Ⅱ",3]
[null,null,null,"（ａ）ジイソシアネート",null,"diisocyanate"]
["削除2",null,null,"　１）ジフェニルメタンジイソシアネート",null,"Benzene, 1,1'-methylenebis(isocyanato-",null,"26447-40-5"]
[583,null,null,"　１－１）４，４’－ジフェニルメタンジイソシアネート",null,"4,4'-Diphenyl methane diisocyanate",null,"101-68-8"]
[584,null,null,"　１－２）２，４’－ジフェニルメタンジイソシアネート",null,"2,4'-Diphenyl methane diisocyanate",null,"5873-54-1"]
[585,null,null,"　１－３）２，２’－ジフェニルメタンジイソシアネート",null,"2,2'-Diphenyl methane diisocyanate",null,"2536-05-2"]
["削除3",null,null,"　２）トルエンジイソシアネート",null,"Toluene Diisocyanate",null,"26471-62-5"]
[587,null,null,"　２－１）２，４－トルエンジイソシアネート",null,"2,4-Toluene diisocyanate",null,"584-84-9"]
[588,null,null,"　２－２）２，６－トルエンジイソシアネート",null,"2,６-Toluene diisocyanate",null,"91-08-7"]
[582,null,null,"　３）ジシクロヘキシルメタンジイソシアネート",null,"Bis(4-isocyanatocyclohexan-1-yl)methane",null,"5124-30-1"]
[589,null,null,"　４）ヘキサメチレンジイソシアネート",null,"1,6-Diisocyanatohexane",null,"822-06-0"]
[586,null,null,"　５）4,4'-ジイソシアナト-3,3'-ジメチルビフェニル ","3,3'-ジメチル-4,4'-ビフェニレン ジイソシアネート","3,3'-Dimethylbiphenyl-4,4'-diyl Diisocyanate",null,"0000091-97-4"]
[590,null,null,"（ｂ）下記のモノマーから成るポリエステルポリオール"]
[591,null,null,"　１）アジピン酸",null,"Adipic acid",null,"124-04-9"]
[603,null,null,"　２）無水フタル酸",null,"Phthalic acid anhydride",null,"85-44-9"]
[602,null,null,"　３）無水コハク酸",null,"Succinic anhydride",null,"108-30-5"]
[594,null,null,"　４）セバシン酸",null,"Sebacic acid",null,"111-20-6"]
[592,null,null,"　５）エチレングリコール",null,"Ethylene glycol",null,"107-21-1"]
[597,null,null,"　６）１，４－ブタンジオール",null,"1,4-Butanediol",null,"110-63-4"]
[593,null,null,"　７）ジエチレングリコール",null,"2,2'-Dihydroxyethyl ether",null,"111-46-6"]
[601,null,null,"　８）１，５－ペンタンジオール",null,"Pentane-1,5-diol",null,"111-29-5"]
[595,null,null,"　９）１，９－ノナンジオール",null,"Nonane-1,9-diol",null,"3937-56-2"]
[598,null,null,"　１０）１，３－プロパンジオール",null,"Propane-1,3-diol",null,"504-63-2"]
[599,null,null,"　１１）１，２－プロパンジオール",null,"Propane-1,2-diol",null,"57-55-6"]
[600,null,null,"　１２）１，６－ヘキサンジオール\n　　　（アルカン（Ｃ＝５～２２）ジオール）",null,"1,6-Hexanediol",null,"629-11-8"]
[604,null,null,"　１３）２－メチル－１，３－プロパンジオール",null,"2-methyl-1,3-Propanediol",null,"2163-42-0"]
[605,null,null,"　１４）３－メチル－１，５－ペンタンジオール",null,"3-methyl-1,5-pentanediol",null,"4457-71-0"]
[596,null,null,"　１５）ビス（ヒドロキシエトキシ）ベンゼン（ＢＨＥＢ）\n　　　　ハイドロキノンジエタノールエーテル（ＨＱＥＥ）",null,"1,4-Di(2-hydroxyethoxy)benzene",null,"104-38-1"]
[null,null,2,"下記のジイソシアネート及び下記のモノマーからなるポリエーテルポリオールの共重合体",null,null,null,null,"〇","〇","〇","〇","〇","Ⅱ",3]
[null,null,null,"（a）ジイソシアネート",null,"diisocyanate"]
["削除4",null,null,"　１）ジフェニルメタンジイソシアネート",null,"Benzene, 1,1'-methylenebis(isocyanato-",null,"26447-40-5"]
[609,null,null,"　１－１）４，４’－ジフェニルメタンジイソシアネート",null,"4,4'-Diphenyl methane diisocyanate",null,"101-68-8"]
[610,null,null,"　１－２）２，４’－ジフェニルメタンジイソシアネート",null,"2,4'-Diphenyl methane diisocyanate",null,"5873-54-1"]
[611,null,null,"　１－３）２，２’－ジフェニルメタンジイソシアネート",null,"2,2'-Diphenyl methane diisocyanate",null,"2536-05-2"]
["削除5",null,null,"　２）トルエンジイソシアネート",null,"Toluene Diisocyanate",null,"26471-62-5"]
[613,null,null,"　２－１）２，４－トルエンジイソシアネート",null,"2,4-Toluene diisocyanate",null,"584-84-9"]
[614,null,null,"　２－２）２，６－トルエンジイソシアネート",null,"2,６-Toluene diisocyanate",null,"91-08-7"]
[608,null,null,"　３）ジシクロヘキシルメタンジイソシアネート",null,"Bis(4-isocyanatocyclohexan-1-yl)methane",null,"5124-30-1"]
[615,null,null,"　４）ヘキサメチレンジイソシアネート",null,"1,6-Diisocyanatohexane",null,"822-06-0"]
[612,null,null,"　５）4,4'-ジイソシアナト-3,3'-ジメチルビフェニル ","3,3'-ジメチル-4,4'-ビフェニレン ジイソシアネート","3,3'-Dimethylbiphenyl-4,4'-diyl Diisocyanate",null,"0000091-97-4"]
[null,null,null,"（ｂ）下記のモノマーから成るポリエーテルポリオール"]
[620,null,null,"　１）テトラヒドロフラン",null,"Tetrahydrofuran",null,"109-99-9"]
[618,null,null,"　２）オキシラン（エチレンオキシド）",null,"Oxirane",null,"75-21-8"]
[628,null,null,"　３）２－メチルオキシラン（プロピレンオキシド）",null,"2-Methyloxirane",null,"75-56-9"]
[617,null,null,"　４）エチレングリコール",null,"Ethylene glycol",null,"107-21-1"]
[625,null,null,"　５）１，２－プロパンジオール",null,"Propane-1,2-diol",null,"57-55-6"]
[623,null,null,"　６）１，４－ブタンジオール",null,"1,4-Butanediol",null,"110-63-4"]
[627,null,null,"　７）１，５－ペンタンジオール",null,"Pentane-1,5-diol",null,"111-29-5"]
[619,null,null,"　８）ジエチレングリコール",null,"2,2'-Dihydroxyethyl ether",null,"111-46-6"]
[624,null,null,"　９）１，３－プロパンジオール",null,"Propane-1,3-diol",null,"504-63-2"]
[626,null,null,"　１０）１，６－ヘキサンジオール\n      （アルカン（Ｃ＝５～２２）ジオール）",null,"1,6-Hexanediol",null,"629-11-8"]
[629,null,null,"　１１）２－メチル－１，３－プロパンジオール",null,"2-methyl-1,3-Propanediol",null,"2163-42-0"]
[630,null,null,"　１２）３－メチル－１，５－ペンタンジオール",null,"3-methyl-1,5-pentanediol",null,"4457-71-0"]
[621,null,null,"　１３）１，９－ノナンジオール",null,"Nonane-1,9-diol",null,"3937-56-2"]
[622,null,null,"　１４）ビス（ヒドロキシエトキシ）ベンゼン（ＢＨＥＢ）\n　　　　ハイドロキノンジエタノールエーテル（ＨＱＥＥ）",null,"1,4-Di(2-hydroxyethoxy)benzene",null,"104-38-1"]
[null,null,3,"下記のジイソシアネート及び下記のモノマーからなるポリカプロラクトンジオールの共重合体",null,null,null,null,"〇","〇","〇","〇","〇","Ⅱ",3]
[null,null,null,"（a）ジイソシアネート",null,"diisocyanate"]
["削除6",null,null,"　１）ジフェニルメタンジイソシアネート",null,"Benzene, 1,1'-methylenebis(isocyanato-",null,"26447-40-5"]
[634,null,null,"　１－１）４，４’－ジフェニルメタンジイソシアネート",null,"4,4'-Diphenyl methane diisocyanate",null,"101-68-8"]
[635,null,null,"　１－２）２，４’－ジフェニルメタンジイソシアネート",null,"2,4'-Diphenyl methane diisocyanate",null,"5873-54-1"]
[636,null,null,"　１－３）２，２’－ジフェニルメタンジイソシアネート",null,"2,2'-Diphenyl methane diisocyanate",null,"2536-05-2"]
["削除7",null,null,"　２）トルエンジイソシアネート",null,"Toluene Diisocyanate",null,"26471-62-5"]
[638,null,null,"　２－１）２，４－トルエンジイソシアネート",null,"2,4-Toluene diisocyanate",null,"584-84-9"]
[639,null,null,"　２－２）２，６－トルエンジイソシアネート",null,"2,６-Toluene diisocyanate",null,"91-08-7"]
[633,null,null,"　３）ジシクロヘキシルメタンジイソシアネート",null,"Bis(4-isocyanatocyclohexan-1-yl)methane",null,"5124-30-1"]
[640,null,null,"　４）ヘキサメチレンジイソシアネート",null,"1,6-Diisocyanatohexane",null,"822-06-0"]
[637,null,null,"　５）4,4'-ジイソシアナト-3,3'-ジメチルビフェニル ","3,3'-ジメチル-4,4'-ビフェニレン ジイソシアネート","3,3'-Dimethylbiphenyl-4,4'-diyl Diisocyanate",null,"0000091-97-4"]
[641,null,null,"（ｂ）下記のモノマーから成るポリカプロラクトンジオール"]
[643,null,null,"　１）ε－カプロラクトン",null,"ε-Caprolactone",null,"502-44-3"]
[642,null,null,"　２）エチレングリコール",null,"Ethylene glycol",null,"107-21-1"]
[648,null,null,"　３）１，４－ブタンジオール",null,"1,4-Butanediol",null,"110-63-4"]
[651,null,null,"　４）１，５－ペンタンジオール　",null,"Pentane-1,5-diol",null,"111-29-5"]
[644,null,null,"　５）ジエチレングリコール",null,"2,2'-Dihydroxyethyl ether",null,"111-46-6"]
[645,null,null,"　６）２，２－ジメチル－１，３－プロパンジオール",null,"2,2-Dimethyl-1,3-propanediol",null,"126-30-7"]
[649,null,null,"　７）１，３－プロパンジオール",null,"Propane-1,3-diol",null,"504-63-2"]
[650,null,null,"　８）１，６－ヘキサンジオール\n          （アルカン（Ｃ＝５～２２）ジオール）",null,"1,6-Hexanediol",null,"629-11-8"]
[652,null,null,"　９）２－メチル－１，３－プロパンジオール",null,"2-methyl-1,3-Propanediol",null,"2163-42-0"]
[653,null,null,"　１０）３－メチル－１，５－ペンタンジオール",null,"3-methyl-1,5-pentanediol",null,"4457-71-0"]
[646,null,null,"　１１）１，９－ノナンジオール",null,"Nonane-1,9-diol",null,"3937-56-2"]
[647,null,null,"　１２）ビス（ヒドロキシエトキシ）ベンゼン（ＢＨＥＢ）\n　　　　ハイドロキノンジエタノールエーテル（ＨＱＥＥ）",null,"1,4-Di(2-hydroxyethoxy)benzene",null,"104-38-1"]
[null,null,4,"下記のジイソシアネート及び下記のモノマーからなるポリカーボネートジオールとの共重合体",null,null,null,null,"〇","〇","〇","〇","〇","Ⅱ",3]
[null,null,null,"（a）ジイソシアネート",null,"diisocyanate"]
["削除8",null,null,"　１）ジフェニルメタンジイソシアネート",null,"Benzene, 1,1'-methylenebis(isocyanato-",null,"26447-40-5"]
[659,null,null,"　１－１）４，４’－ジフェニルメタンジイソシアネート",null,"4,4'-Diphenyl methane diisocyanate",null,"101-68-8"]
[660,null,null,"　１－２）２，４’－ジフェニルメタンジイソシアネート",null,"2,4'-Diphenyl methane diisocyanate",null,"5873-54-1"]
[661,null,null,"　１－３）２，２’－ジフェニルメタンジイソシアネート",null,"2,2'-Diphenyl methane diisocyanate",null,"2536-05-2"]
["削除9",null,null,"　２）トルエンジイソシアネート",null,"Toluene Diisocyanate",null,"26471-62-5"]
[663,null,null,"　２－１）２，４－トルエンジイソシアネート",null,"2,4-Toluene diisocyanate",null,"584-84-9"]
[664,null,null,"　２－２）２，６－トルエンジイソシアネート",null,"2,６-Toluene diisocyanate",null,"91-08-7"]
[658,null,null,"　３）ジシクロヘキシルメタンジイソシアネート",null,"Bis(4-isocyanatocyclohexan-1-yl)methane",null,"5124-30-1"]
[665,null,null,"　４）ヘキサメチレンジイソシアネート",null,"1,6-Diisocyanatohexane",null,"822-06-0"]
[662,null,null,"　５）4,4'-ジイソシアナト-3,3'-ジメチルビフェニル ","3,3'-ジメチル-4,4'-ビフェニレン ジイソシアネート","3,3'-Dimethylbiphenyl-4,4'-diyl Diisocyanate",null,"0000091-97-4"]
[657,null,null,"　６）キシリレンジイソシアネート\n　　   m-キシリレンジイソシアネート","1,3-キシレン ジイソシアネート\n1,2-キシレン ジイソシアネート","Xylylene diisocyanate\nm-Xylylene diisocyanate",null,"0025854-16-4\n0003634-83-1"]
[666,null,null,"（ｂ）下記のモノマーから成るポリカーボネートジオール"]
[671,null,null,"　１）炭酸ジフェニル",null,"Diphenyl carbonate",null,"102-09-0"]
[667,null,null,"　２）エチレングリコール",null,"Ethylene glycol",null,"107-21-1"]
[675,null,null,"　３）１，３－ブタンジオール",null,"1,3-Butanediol",null,"107-88-0"]
[676,null,null,"　４）１，４－ブタンジオール",null,"1,4-Butanediol",null,"110-63-4"]
[668,null,null,"　５）ジエチレングリコール",null,"2,2'-Dihydroxyethyl ether",null,"111-46-6"]
[677,null,null,"　６）１，３－プロパンジオール",null,"Propane-1,3-diol",null,"504-63-2"]
[678,null,null,"　７）１，６－ヘキサンジオール\n         （アルカン（Ｃ＝５～２２）ジオール）",null,"1,6-Hexanediol",null,"629-11-8"]
[679,null,null,"　８）１，５－ペンタンジオール",null,"Pentane-1,5-diol",null,"111-29-5"]
[672,null,null,"　９）炭酸ジメチル",null,"Dimethyl carbonate",null,"616-38-6"]
[670,null,null,"　１０）炭酸ジエチル",null,"Diethyl carbonate",null,"105-58-8"]
[669,null,null,"　１１）炭酸エチレン（エチレンカーボネート）",null,"Ethylene carbonate",null,"96-49-1"]
[682,null,null,"　１２）プロピレンカーボネート",null,"propylene carbonate",null,"108-32-7"]
[673,null,null,"　１３）二酸化炭素",null,"Carbon dioxide",null,"124-38-9"]
[683,null,null,"　１４）２－メチル－１，３－プロパンジオール",null,"2-methyl-1,3-Propanediol",null,"2163-42-0"]
[684,null,null,"　１５）３－メチル－１，５－ペンタンジオール",null,"3-methyl-1,5-pentanediol",null,"4457-71-0"]
[681,null,null,"　１６）２－メチル－１，８－オクタンジオール",null,"2-Methyloctane-1,8-diol",null,"109359-36-6"]
[674,null,null,"　１７）ビス（ヒドロキシエトキシ）ベンゼン（ＢＨＥＢ）\n　　　　ハイドロキノンジエタノールエーテル（ＨＱＥＥ）",null,"1,4-Di(2-hydroxyethoxy)benzene",null," 104-38-1"]
[680,null,null,"　１８）水","水","Water",null,"0007732-18-5"]
[null,null,5,"下記のジイソシアネート及び下記のモノマーの混合からなるジオールの共重合体"]
[null,null,null,"（ａ）ジイソシアネート",null,"diisocyanate"]
["削除10",null,null,"　１）ジフェニルメタンジイソシアネート",null,"Benzene, 1,1'-methylenebis(isocyanato-",null,"26447-40-5","〇","〇","〇","〇","〇","Ⅱ",3]
[688,null,null,"　１－１）４，４’－ジフェニルメタンジイソシアネート",null,"4,4'-Diphenyl methane diisocyanate",null,"101-68-8","〇","〇","〇","〇","〇","Ⅱ",3]
[689,null,null,"　１－２）２，４’－ジフェニルメタンジイソシアネート",null,"2,4'-Diphenyl methane diisocyanate",null,"5873-54-1","〇","〇","〇","〇","〇","Ⅱ",3]
[690,null,null,"　１－３）２，２’－ジフェニルメタンジイソシアネート",null,"2,2'-Diphenyl methane diisocyanate",null,"2536-05-2","〇","〇","〇","〇","〇","Ⅱ",3]
["削除11",null,null,"　２）トルエンジイソシアネート",null,"Toluene Diisocyanate",null,"26471-62-5","〇","〇","〇","〇","〇","Ⅱ",3]
[692,null,null,"　２－１）２，４－トルエンジイソシアネート",null,"2,4-Toluene diisocyanate",null,"584-84-9","〇","〇","〇","〇","〇","Ⅱ",3]
[693,null,null,"　２－２）２，６－トルエンジイソシアネート",null,"2,６-Toluene diisocyanate",null,"91-08-7","〇","〇","〇","〇","〇","Ⅱ",3]
[687,null,null,"　３）ジシクロヘキシルメタンジイソシアネート",null,"Bis(4-isocyanatocyclohexan-1-yl)methane",null,"5124-30-1","〇","〇","〇","〇","〇","Ⅱ",3]
[694,null,null,"　４）ヘキサメチレンジイソシアネート",null,"1,6-Diisocyanatohexane",null,"822-06-0","〇","〇","〇","〇","〇","Ⅱ",3]
[691,null,null,"　５）4,4'-ジイソシアナト-3,3'-ジメチルビフェニル ","3,3'-ジメチル-4,4'-ビフェニレン ジイソシアネート","3,3'-Dimethylbiphenyl-4,4'-diyl Diisocyanate",null,"0000091-97-4","〇","〇","〇","〇","〇","Ⅱ",3]
[null,null,null,"（ｂ）下記のモノマーの混合から成るジオール"]
[696,null,null,"　１）アジピン酸",null,"Adipic acid",null,"124-04-9","〇","〇","〇","〇","〇","Ⅱ",3]
[728,null,null,"　２）無水マレイン酸",null,"Maleic acid anhydride",null,"108-31-6","〇","〇","〇","〇","〇","Ⅱ",3]
[727,null,null,"　３）無水フタル酸",null,"Phthalic acid anhydride",null,"85-44-9","〇","〇","〇","〇","〇","Ⅱ",3]
[730,null,null,"　４）３－メチル－１，５－ペンタンジオール",null,"3-methyl-1,5-pentanediol",null,"4457-71-0","〇","〇","〇","〇","〇","Ⅱ",3]
[700,null,null,"　５）エチレンオキシド",null,"Oxirane",null,"75-21-8","〇","〇","〇","〇","〇","Ⅱ",3]
[729,null,null,"　６）プロピレンオキシド",null,"2-Methyloxirane",null,"75-56-9","〇","〇","〇","〇","〇","Ⅱ",3]
[713,null,null,"　７）テトラヒドロフラン",null,"Tetrahydrofuran",null,"109-99-9","〇","〇","〇","〇","〇","Ⅱ",3]
[701,null,null,"　８）ε－カプロラクトン",null,"ε-Caprolactone",null,"502-44-3","〇","〇","〇","〇","〇","Ⅱ",3]
[716,null,null,"　９）ネオペンチルグリコール",null,"2,2-Dimethyl-1,3-propanediol",null,"126-30-7","〇","〇","〇","〇","〇","Ⅱ",3]
[704,null,null,"　１０）ジエチレングリコール",null,"2,2'-Dihydroxyethyl ether",null,"111-46-6","〇","〇","〇","〇","〇","Ⅱ",3]
[710,null,null,"　１１）炭酸ジフェニル　",null,"Diphenyl carbonate",null," 102-09-0","〇","〇","〇","〇","〇","Ⅱ",3]
[711,null,null,"　１２）炭酸ジメチル",null,"Dimethyl carbonate",null,"16-38-6","〇","〇","〇","〇","〇","Ⅱ",3]
[709,null,null,"　１３）炭酸ジエチル",null,"Diethyl carbonate",null,"105-58-5","〇","〇","〇","〇","〇","Ⅱ",3]
[705,null,null,"　１４）炭酸エチレン（エチレンカーボネート）",null,"Ethylene carbonate",null,"95-49-1","〇","〇","〇","〇","〇","Ⅱ",3]
[697,null,null,"　１５）エチレングリコール",null,"Ethylene glycol",null,"107-21-1","〇","〇","〇","〇","〇","Ⅱ",3]
[721,null,null,"　１６）１，４－ブタンジオール　",null,"1,4-Butanediol",null,"110-63-4","〇","〇","〇","〇","〇","Ⅱ",3]
[726,null,null,"　１７）１，５－ペンタンジオール",null,"Pentane-1,5-diol",null,"111-29-5","〇","〇","〇","〇","〇","Ⅱ",3]
[725,null,null,"　１８）１，６－ヘキサンジオール　",null,"1,6-Hexanediol",null,"629-11-8","〇","〇","〇","〇","〇","Ⅱ",3]
[718,null,null,"　１９）１，４－ビス（２’－ヒドロキシエトキシ）ベンゼン",null,"1,4-Di(2-hydroxyethoxy)benzene",null,"104-38-1","〇","〇","〇","〇","〇","Ⅱ",3]
[717,null,null,"　２０）１，９－ノナンジオール",null,"Nonane-1,9-diol",null,"3937-56-2","〇","〇","〇","〇","〇","Ⅱ",3]
[715,null,null,"　２１）二酸化炭素",null,"Carbon dioxide",null,"124-38-9","〇","〇","〇","〇","〇","Ⅱ",3]
[722,null,null,"　２２）１，２－プロパンジオール",null,"Propane-1,2-diol",null,"57-55-6","〇","〇","〇","〇","〇","Ⅱ",3]
[720,null,null,"　２３）ビス（ヒドロキシエトキシプロピル）ジメチコン",null,"Bis-Hydroxyethoxypropyl Dimethicone",null,"222416-17-3","〇","〇","〇","〇","〇","Ⅱ",3]
[708,null,null,"　２４）水酸基末端ポリオレフィン","水素化処理及び水酸基末端処理されたイソプレン単独重合体","1,3-Butadiene, 2-methyl-, homopolymer, hydrogenated, hydroxy-terminated",null,"0146177-82-4","〇","〇","〇","〇","〇","III",3]
[724,null,null,"　２５）α，α’－［（イソプロピリデン）ジ－４，１－フェニレン］ビス｛ω－ヒドロキシ－ポリ［オキシ（メチルエチレン）］｝","プロポキシル化処理されたビスフェノールA","alpha,alpha'-[(Isopropylidene)di-4,1-phenylene]bis{omega-hydroxy-poly[oxy(methylethylene)]}",null,"0037353-75-6","〇","〇","〇","〇","〇","III",3]
[723,null,null,"　２６）トリメチロールプロパンプロポキシラート","プロポキシル化処理されたトリメチロールプロパン","Trimethylol propane propoxylated",null,"0025723-16-4","〇","〇","〇","〇","〇","III",3]
[702,null,null,"　２７）重合ひまし油","和名と英名が異なる（CASは英名）","Castor oil, oxidized",null,"0068187-84-8","〇","〇","〇","〇","〇","III",3]
[707,null,null,"　２８）ポリブタジエン（末端ヒドロキシ基，カルボキシ基，エポキシ基を含む）の水素化物","水素化処理及び水酸基またはカルボキシ基またはエポキシ基末端処理された1,3-ブタジエン単独重合体","1,3-Butadiene, homopolymer, hydrogenated, hydroxy-terminated",null,"0068954-10-9","〇","〇","〇","〇","〇","III",3]
[703,null,null,"　２９）２，４－ジエチルペンタン－１，５－ジオール","2,4-ジエチル-1,5-ペンタンジオール","2,4-Diethylpentane-1,5-diol",null,"0057987-55-0","〇","〇","〇","〇","〇","III",3]
[698,null,null,"　３０）２－プロポキシエタノール","エチレングリコールのモノプロピルエーテル","2-Propoxyethanol",null,"0002807-30-9","〇","〇","〇","〇","〇","III",3]
[714,null,null,"　３１）テトラヒドロフルフリルアルコール","テトラヒドロフルフリルアルコール","Tetrahydrofurfuryl alcohol",null,"0000097-99-4","〇","〇","〇","〇","〇","III",3]
[699,null,null,"　３２）２－エチル－２－（ヒドロキシメチル）プロパン－１，３－ジオール・エポキシ化脂肪酸（Ｃ＝１６～１８及び不飽和Ｃ＝１８）のメチルエステル重合物","エポキシ化処理された不飽和脂肪酸（C16-18）のメチルエステル・トリメチロールプロパン共重合体","Polymer of 2-ethyl-2-(hydroxymethyl)propane-1,3-diol / methyl ester of epoxidized fatty acids(C=16-18 and C=18 unsaturated)",null,"0188831-96-1","〇","〇","〇","〇","〇","III",3]
[706,null,null,"　３３）水酸基末端ポリブタジエン","水酸基末端処理された1,3-ブタジエン単独重合体","Hydroxy terminated polybutadiene",null,"0069102-90-5","〇","〇","〇","〇","〇","III",3]
[719,null,null,"　３４）N,N-ビス（2-ヒドロキシプロピル）アニリン","N,N-ビス(2-ヒドロキシプロピル)-アニリン","N,N-Bis (2-hydroxypropyl)aniline",null,"0003077-13-2","〇","〇","〇","〇","〇","III",3]
[712,null,null,"　３５）N,N,N',N'-テトラキス（2-ヒドロキシプロピル)エチレンジアミン","N,N,N',N'-テトラキス(2-ヒドロキシプロピル)-エチレンジアミン","N,N,N',N'-Tetrakis(2-hydroxypropyl)ethylenediamine",null,"0000102-60-3","〇","〇","〇","〇","〇","III",3]
[]
[null,null,"５９．熱可塑性ポリエステルエラストマー（TPC）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[739,null,1,"テレフタル酸ジメチル・１，４－ブタンジオール・α－ヒドロ－ω－ヒドロキシポリ（オキシブタン－１，４－ジイル）ブロック共重合体／\nテレフタル酸・１，４－ブタンジオール・α－ヒドロ－ω－ヒドロキシポリ（オキシブタン－１，４－ジイル）ブロック共重合体",null,"1,4-Benzenedicarboxylic acid, dimethyl ester, polymer with 1,4-butanediol and .alpha.-hydro-.omega.-hydroxypoly(oxy-1,4-butanediyl), block / \n1,4-Benzenedicarboxylic acid, polymer with 1,4-butanediol and .alpha.-hydro-.omega.-hydroxypoly(oxy-1,4-butanediyl), block",null,"9078-71-1\n37282-12-5\n106159-00-6\n106465-17-2","○","○","○","○","○","Ⅲ",3]
[740,null,2,"テレフタル酸ジメチル・１，４－ブタンジオール・α－ヒドロ－ω－ヒドロキシポリ（オキシブタン－１，４－ジイル）ブロック共重合体・無水マレイン酸付加物／\nテレフタル酸・１，４－ブタンジオール・α－ヒドロ－ω－ヒドロキシポリ（オキシブタン－１，４－ジイル）ブロック共重合体・無水マレイン酸付加物",null,"1,4-Benzenedicarboxylic acid, 1,4-dimethyl ester, polymer with 1,4-butanediol and α-hydro-ω-hydroxypoly(oxy-1,4-butanediyl), block, maleated /\n1,4-Benzenedicarboxylic acid, polymer with 1,4-butanediol and α-hydro-ω-hydroxypoly(oxy-1,4-butanediyl), block, maleated",null,"1224447-95-3\n1686129-33-8\n1686129-34-9","○","○","○","○","○","Ⅲ",3]
[737,null,3,"テレフタル酸ジメチル・イソフタル酸ジメチル・１，４－ブタンジオール・α－ヒドロ－ω－ヒドロキシポリ（オキシブタン－１，４－ジイル）ブロック共重合体／\nテレフタル酸・イソフタル酸・１，４－ブタンジオール・α－ヒドロ－ω－ヒドロキシポリ（オキシブタン－１，４－ジイル）ブロック共重合体","イソフタル酸またはイソフタル酸ジメチル・テレフタル酸またはテレフタル酸ジメチル・1,4-ブタンジオール共重合体と1,4-ブタンジオール単独重合体のブロック共重合体","1,3-Benzenedicarboxylic acid, 1,3-dimethyl ester polymer with 1,4-Benzenedicarboxylic acid, 1,4-dimethyl ester, 1,4-butanediol and .alpha.-hydro-.omega.-hydroxypoly(oxy-1,4-butanediyl), block／\n1,3-Benzenedicarboxylic acid polymer with 1,4-Benzenedicarboxylic acid,  1,4-butanediol and .alpha.-hydro-.omega.-hydroxypoly(oxy-1,4-butanediyl), block",null,"0107811-95-0\n0009086-55-9\n0037282-15-8","○","○","○","○","○","Ⅱ",3,"乳・乳製品の容器包装では、食品非接触層に限る。"]
[738,null,4,"テレフタル酸ジメチル・１，４－ブタンジオール・2-メチルオキシラン・オキシランブロック共重合体","テレフタル酸ジメチル・1,4-ブタンジオール共重合体とオキシラン・2-メチルオキシラン共重合体のブロック共重合体","1,4-Benzenedicarboxylic acid, 1,4-dimethyl ester polymer with 1,4-butanediol , 2-methyloxirane and oxirane, block",null,"0064811-37-6","○","○","○","○","○","Ⅲ",3]
[735,null,5,"テレフタル酸ジメチル・イソフタル酸ジメチル・１，４－ブタンジオール・2-メチルオキシラン・オキシランブロック共重合体","イソフタル酸ジメチル・テレフタル酸ジメチル・1,4-ブタンジオール共重合体とオキシラン・2-メチルオキシラン共重合体のブロック共重合体","1,3-Benzenedicarboxylic acid, 1,3-dimethyl ester polymer with 1,4-butanediol, 1,4-Benzenedicarboxylic acid, 1,4-dimethyl ester, 2-methyloxirane and oxirane, block",null,"0064811-38-7","○","○","○","○","○","Ⅱ",3]
[736,null,6,"テレフタル酸ジメチル・イソフタル酸ジメチル・１，４－ブタンジオール・α－ヒドロ－ω－ヒドロキシポリ（オキシエタン－１，２－ジイル）ブロック共重合体","イソフタル酸ジメチル・テレフタル酸ジメチル・1,4-ブタンジオール共重合体とポリエチレングリコールのブロック共重合体","1,3-benzenedicarboxylic acid, 1,3-dimethyl ester, polymer with 1,4-butanediol,\n1,4-dimethyl benzenedicarboxylate and alpha.-hydro-.omega.-hydroxypoly\n(oxy-1,2-ethanediyl), block",null,"0107087-28-5","○","○","○","○","○","Ⅲ",3]
[]
[null,null,"６０．メラミン樹脂（MF)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[1254,null,1,"メラミン・ホルムアルデヒド共重合体",null,"1,3,5-Triazine-2,4,6-Triamine, Polymer with Formaldehyde",null,"9003-08-1","○","○","○","○","○","Ⅲ",1,"メラミン（CAS登録番号108-78-1）1molに対して反応させるホルムアルデヒド（CAS登録番号50-00-0）は3mol以下。"]
[1252,null,2,"メラミン・ベンゾグアナミン・ホルムアルデヒド共重合体",null,"1,3,5-Triazine-2,4,6-Triamine / 2,4-Diamino-6-phenyl-1,3,5-triazine, Polymer with Formaldehyde",null,"25035-72-7","○","○","○","○","○","Ⅲ",1,"メラミン（CAS登録番号108-78-1）1molに対して反応させるベンゾグアナミン（CAS登録番号91-76-9）は0.75mol以下、ホルムアルデヒド（CAS登録番号50-00-0）は4mol以下。"]
[1251,null,3,"メラミン・尿素・ホルムアルデヒド共重合体",null,"1,3,5-Triazine-2,4,6-Triamine / Urea, Polymer with Formaldehyde",null,"25036-13-9","○","○","○","○","○","Ⅲ",1,"メラミン（CAS登録番号108-78-1）1molに対して反応させる尿素（CAS登録番号57-13-6）は0.75mol以下、ホルムアルデヒド（CAS登録番号50-00-0）は4mol以下。"]
[1253,null,4,"メラミン・ｐートルエンスルホンアミド・ホルムアルデヒド共重合体",null,"1,3,5-Triazine-2,4,6-Triamine /  p-Toluene sulfonamide , Polymer with Formaldehyde",null,"25067-00-9","○","○","○","○","○","Ⅲ",1,"メラミン（CAS登録番号108-78-1）1molに対して反応させるｐートルエンスルホンアミド（CAS登録番号70-55-3）は0.75mol以下、ホルムアルデヒド（CAS登録番号50-00-0）は4mol以下。"]
[]
[null,null,"６１．フェノール樹脂（PF)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[844,null,1,"フェノール・ホルムアルデヒド共重合体",null,"Phenol, polymer with formaldehyde",null,"9003-35-4","○","○","○","○","○","Ⅱ",1,"食品接触時間は30分未満。"]
[]
[null,null,"６２．メラミン・フェノール樹脂（MP)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[849,null,1,"メラミン・フェノール・ホルムアルデヒド共重合体",null,"1,3,5-Triazine-2,4,6-Triamine / Phenol, Polymer with Formaldehyde",null,"25917-04-8","○","○","○","○","○","Ⅱ",1,"メラミン（CAS登録番号108-78-1）1molに対して反応させるフェノール（CAS登録番号108-95-2）は1.4mol以下、ホルムアルデヒド（CAS登録番号50-00-0）は4mol以下。"]
[]
[null,null,"６３．ユリア樹脂（UF)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[575,null,1,"尿素・ホルムアルデヒド共重合体",null,"Urea, polymer with formaldehyde",null,"9011-05-6","ー","ー","ー","ー","ー","Ⅱ",1,"尿素1molに対して反応させるホルムアルデヒド（CAS登録番号50-00-0）2mol以下。\n食品非接触層に限る。"]
[]
[null,null,"６４．熱硬化性ポリウレタン樹脂（TSU)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・\n乳製品","酒類","その他"]
[745,null,1,"\nイソシアネート基を2個以上有する以下のイソシアネート類及びヒドロキシル基を2個以上有する以下のポリオール原料からなる重合体。\n",null,null,null,"9009-54-5"]
[746,null,null,"＜イソシアネート類＞",null,"＜Isocyanates＞"]
["削除12",null,null,"1) メチル-1,3-フェニレン=ジイソシアナート/トリレンジイソシアネート/トルエンジイソシアネート",null,"1)     Toluene diisocyanate",null,"26471-62-5","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[752,null,null,"1-1) ２－メチル－１，３－フェニレン＝ジイソシアナート/2,6-トリレンジイソシアネート/2,6-トルエンジイソシアネート",null,"1-1)     Toluene-2,6-diisocyanate",null,"91-08-7","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[751,null,null,"1-2) ４－メチル－１，３－フェニレン＝ジイソシアナート/2,4-トリレンジイソシアネート/2,4-トルエンジイソシアネート",null,"1-2)     Toluene-2,4-diisocyanate",null,"584-84-9","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[754,null,null,"2) ポリメチレンポリフェニルポリイソシアネート/ポリメリックMDI/クルードMDI",null,"2)     Polymeric diphenylmethane diisocyanate,Polymethylene polyphenylene isocyanate/Polymeric MDI/Diphenylmethane-2,4'-diisocyanate/1-Isocyanato-2-[(4-isocyanatophenyl)methyl] benzene",null,"9016-87-9","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
["削除13",null,null,"3) ジフェニルメタンジイソシアネート(MDI)",null,"3)     Diphenylmethane diisocyanate",null,"26447-40-5","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[750,null,null,"3-1) メチレンビス（４，１－フェニレン）＝ジイソシアナート/4,4'-ジフェニルメタンジイソシアネート",null,"3-1)     4,4'-Methylenedi(phenyl isocyanate)",null,"101-68-8","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[749,null,null,"3-2) 2,4'-ジフェニルメタンジイソシアネート",null,"3-2)     Diphenylmethane-2,4'-diisocyanate",null,"5873-54-1","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[748,null,null,"3-3) 2,2'-ジフェニルメタンジイソシアネート",null,"3-3)     Diphenylmethane-2,2'-diisocyanate",null,"2536-05-2","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[753,null,null,"4)     １，６－ジイソシアナトヘキサン",null,"4) 1,6-Diisocyanatohexane",null,"822-06-0","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[747,null,null,"5）ジフェニルメタンジイソシアネート(MDI)カルボジイミド変性物","カルボジイミド修飾されたジフェニルメタン ジイソシアネート","5）Diphenylmethane diisocyanate, modified carbodiimide.",null,"0025686-28-6","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[755,null,null,"＜ポリオール原料＞",null,"＜Polyol raw materials＞"]
[797,null,null,"1)     テレフタル酸",null,"1)     Terephthalic acid",null,"10021-0","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[773,null,null,"2)     オレイン酸",null,"2)     Oleic acid",null,"112-80-1","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[763,null,null,"3)     イソフタル酸",null,"3)     Isophthalic acid",null,"121-91-5","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[759,null,null,"4)     アジピン酸",null,"4)     Adipic acid",null,"124-04-9","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[812,null,null,"5)     オルソフタル酸",null,"5)     Orthophthalic acid",null,"88-99-3","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[765,null,null,"6)     ２－エチルヘキサン酸",null,"6)     2-Ethylhexanoic acid",null,"149-57-5","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[789,null,null,"7)     スチレン",null,"7)     Styrene",null,"10042-5","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[793,null,null,"8)     炭酸ジフェニル",null,"8)     Carbonic acid, diphenyl ester",null,"102-09-0","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[758,null,null,"9)     アクリロニトリル",null,"9)     Acrylonitrile",null,"107-13-1","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[829,null,null,"10)     2,4,6-トリアミノ-1,3,5-トリアジン（メラミン）",null,"10)   Melamine",null,"108-78-1","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[772,null,null,"11)     オキシラン （エチレンオキシド）",null,"11)   Ethylene oxide",null,"75-21-8","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[827,null,null,"12)     2-メチルオキシラン （プロピレンオキシド ）",null,"12)   Propylene oxide",null,"75-56-9","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[756,null,null,"13)   アクリル酸",null,"13)   Acrylic acid",null,"79-10-7","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[825,null,null,"14)   メタクリル酸",null,"14)   Methacrylic acid",null,"79-41-4","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[826,null,null,"15)   メタクリル酸－２－ヒドロキシエチル",null,"15)   2-Hydroxyethyl methacrylate",null,"868-77-9","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[757,null,null,"16)     アクリル酸－２－ヒドロキシエチル",null,"16)   2-Hydroxyethyl acrylate",null,"818-61-1","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[810,null,null,"17)     ブタジエン",null,"17)   1,3-Butadiene",null,"106-9-0","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[766,null,null,"18)     エチレングリコール",null,"18)   Ethylene glycol",null,"107-21-1","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[813,null,null,"19)     1,3-ブタンジオール",null,"19)     1,3-Butylene glycol",null,"107-88-0","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[814,null,null,"20)     1,4-ブタンジオール",null,"20)     1,4-Butanediol／Butylen glycol",null,"110-63-4","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[781,null,null,"21)     ジエチレングリコール",null,"21)     Diethylene glycol",null,"111-46-6","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[799,null,null,"22)     トリエチレングリコール",null,"22)     Triethylene glycol",null,"112-27-6","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[822,null,null,"23)     ペンタエリスリトール",null,"23)     Pentaerythritol",null,"115-77-5","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[800,null,null,"24)     トリプロピレングリコール",null,"24)     Tripropylene glycol",null,"2480044-0","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[783,null,null,"25)     ジプロピレングリコール",null,"25)     Dipropylene glycol",null,"25265-71-8","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[817,null,null,"26)     プロパン-1,3-ジオール　1,3-プロパンジオール",null,"26)     1,3-Propanediol",null,"504-63-2","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[774,null,null,"27)     グリセリン   ",null,"27)     Glycerine",null,"56-81-5","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[784,null,null,"28)     ショ糖（スクロース）","ショ糖","28)   Sucrose",null,"0000057-50-1","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[818,null,null,"29)     プロパン-1,2-ジオール　1,2-プロパンジオール",null,"29)   Propylene glycol",null,"57-55-6","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[801,null,null,"30)   2-エチル-2-ヒドロキシメチル-1,3-プロパンジオール（トリメチロールプロパン）",null,"30)   Trimethylolpropane",null,"77-99-6","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[791,null,null,"31)   大豆油",null,"31)   soybean oil",null,"8001-22-7","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[788,null,null,"32)   水素化ひまし油（水添動植物油脂）",null,"32)   Hydrogenated castor oil",null,"8001-78-3","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[808,null,null,"33)   ひまし油",null,"33)   Castor oil",null,"8001-79-4","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[815,null,null,"34)   プロパン-2-オール",null,"34)   Isopropanol",null,"67-63-0","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[761,null,null,"35)   アルキルアルコール（Ｃ＝５～３８）",null,"35)   C16-18 Alcohols　/　alcohol, aliphatic C4-C22, monohydric, saturated, linear, primary",null,"67762-27-0","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[816,null,null,"36)     プロピルアルコール",null,"36)   Propanol",null,"71-23-8","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[811,null,null,"37)     1-ブタノール（ブチルアルコール）",null,"37)   Butanol",null,"71-36-3","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[798,null,null,"38)     トリエタノールアミン",null,"38)   Triethanolamine",null,"102-71-6","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[830,null,null,"39)   リン酸",null,"39) Phosphoric acid",null,"7664-38-2","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[768,null,null,"40)     エチレンジアミン",null,"40）Ethylenediamine",null,"107-15-3","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[792,null,null,"41)     部分脱水ヒマシ油",null,"41）Castor oil　dehydrated",null,"64147-40-6","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[782,null,null,"42)     ジエチレントリアミン",null,"42）2,2'-Diaminodiethylamine",null,"111-40-0","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[790,null,null,"43)     D-ソルビトール",null,"43）D-Glucitol",null,"50-70-4","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[770,null,null,"44）エピクロルヒドリン","エピクロルヒドリン","44）epichlorohydrin",null,"0000106-89-8","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
["削除14",null,null,"45）2,2－ビス（4－ヒドロキシフェニル）プロパン\n　(ビスフェノールA)","ビスフェノールA","45）2,2-bis(4-hydroxyphenyl)propane",null,"0000080-05-7","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[795,null,null,"46）テトラヒドロフラン","テトラヒドロフラン","46）Tetrahydrofuran",null,"0000109-99-9","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[809,null,null,"47)  ヒマシ油脂肪酸メチルエステル","ヒマシ油脂肪酸のメチルエステル","47）Fatty acids, castor-oil, Me esters",null,"0000141-24-2","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[807,null,null,"48)  ポリオキシアルキレン(C=2～3)ビスフェノールAエーテル ","ビスフェノールAとプロピレングリコールのジエーテル","48）bis-(4-β-Hydroxypropoxyphenyl) dimethylmethane",null,"0000116-37-0","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[802,null,null,"49)  ナタネ油","ナタネ油","49）rapeseed oil",null,"0008002-13-9","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[828,null,null,"50) ３－メチル－１，５－ペンタンジオール","3-メチル-1,5-ペンタンジオール","50）3-methylpentane-1,5-diol",null,"0004457-71-0","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[775,null,null,"51)     酢酸ビニル","酢酸 ビニル","51）Vinyl acetate",null,"0000108-05-4","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[779,null,null,"52)     ジエタノールアミン","ジエタノールアミン","52）Diethanolamine",null,"0000111-42-2","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[760,null,null,"53)     アミノエチルピペラジン","N-(2-アミノエチル)ピペラジン","53）N-(2-Aminoethyl)piperazine",null,"0000140-31-8","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[764,null,null,"54)     モノエタノールアミン","エタノールアミン","54）Ethanolamine",null,"0000141-43-5","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[804,null,null,"55)     ノニルフェノール","ノニルフェノール","55）Nonylphenol",null,"0025154-52-3","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[777,null,null,"56)     ジシアンジアミド","N-シアノ-グアニジン","56）Dicyandiamide",null,"0000461-58-5","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[823,null,null,"57）　 ホルムアルデヒド","ホルムアルデヒド","57）Formaldehyde",null,"0000050-00-0","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[769,null,null,"58)     エトキシ化プロポキシ化アルコール（Ｃ＝１２～１４）","エトキシル化またはプロポキシル化処理された脂肪族アルコール（C12-14）","58）Ethoxylated propoxylated alcohols(C=12-14)",null,"0068439-51-0","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[806,null,null,"59)     ビスフェノールA","45と同じ","59）4,4'-Isopropylidenediphenol",null,"0000080-05-7","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[821,null,null,"60)  1, 6 - ヘキサンジオール","1,6-ヘキサンジオール","60)1,6-Hexanediol",null,"0000629-11-8","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[803,null,null,"61）２，２－ジメチル－１，３－プロパンジオール","ネオペンチルグリコール","61）2,2-Dimethyl-1,3-propanediol",null,"0000126-30-7","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[762,null,null,"62）安息香酸","安息香酸","62）benzoic acid",null,"0000065-85-0","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[824,null,null,"63）マニトール","マニトール","63）Mannitol ",null,"0000069-65-8","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[778,null,null,"64）ジアミノトルエン","ジアミノトルエン","64）Diaminotoluene",null,"0000095-80-7\n0000496-72-0","〇","〇","〇","〇","〇","Ⅰ",1,"食品非接触での使用可能温度はⅢ"]
[787,null,null,"65）水酸基末端ポリオレフィン","水素化処理及び水酸基末端処理されたイソプレン単独重合体","65）1,3-Butadiene, 2-methyl-, homopolymer, hydrogenated, hydroxy-terminated",null,"0146177-82-4","〇","〇","〇","〇","〇","III",3]
[820,null,null,"66）α，α’－［（イソプロピリデン）ジ－４，１－フェニレン］ビス｛ω－ヒドロキシ－ポリ［オキシ（メチルエチレン）］｝","プロポキシル化処理されたビスフェノールA","66）alpha,alpha'-[(Isopropylidene)di-4,1-phenylene]bis{omega-hydroxy-poly[oxy(methylethylene)]}",null,"0037353-75-6","〇","〇","〇","〇","〇","III",3]
[819,null,null,"67）トリメチロールプロパンプロポキシラート","プロポキシル化処理されたトリメチロールプロパン","67）Trimethylol propane propoxylated",null,"0025723-16-4","〇","〇","〇","〇","〇","III",3]
[776,null,null,"68）重合ひまし油","和名と英名が異なる（CASは英名）","68）Castor oil, oxidized",null,"0068187-84-8","〇","〇","〇","〇","〇","III",3]
[786,null,null,"69）ポリブタジエン（末端ヒドロキシ基，カルボキシ基，エポキシ基を含む）の水素化物","水素化処理及び水酸基またはカルボキシ基またはエポキシ基末端処理された1,3-ブタジエン単独重合体","69）1,3-Butadiene, homopolymer, hydrogenated, hydroxy-terminated",null,"0068954-10-9","〇","〇","〇","〇","〇","III",3]
[780,null,null,"70）２，４－ジエチルペンタン－１，５－ジオール","2,4-ジエチル-1,5-ペンタンジオール","70）2,4-Diethylpentane-1,5-diol",null,"0057987-55-0","〇","〇","〇","〇","〇","III",3]
[767,null,null,"71）２－プロポキシエタノール","エチレングリコールのモノプロピルエーテル","71）2-Propoxyethanol",null,"0002807-30-9","〇","〇","〇","〇","〇","III",3]
[796,null,null,"72）テトラヒドロフルフリルアルコール","テトラヒドロフルフリルアルコール","72）Tetrahydrofurfuryl alcohol",null,"0000097-99-4","〇","〇","〇","〇","〇","III",3]
[771,null,null,"73）２－エチル－２－（ヒドロキシメチル）プロパン－１，３－ジオール・エポキシ化脂肪酸（Ｃ＝１６～１８及び不飽和Ｃ＝１８）のメチルエステル重合物","エポキシ化処理された不飽和脂肪酸（C16-18）のメチルエステル・トリメチロールプロパン共重合体","73）Polymer of 2-ethyl-2-(hydroxymethyl)propane-1,3-diol / methyl ester of epoxidized fatty acids(C=16-18 and C=18 unsaturated)",null,"0188831-96-1","〇","〇","〇","〇","〇","III",3]
[785,null,null,"74）水酸基末端ポリブタジエン","水酸基末端処理された1,3-ブタジエン単独重合体","74）Hydroxy terminated polybutadiene",null,"0069102-90-5","〇","〇","〇","〇","〇","III",3]
[805,null,null,"75）N,N-ビス（2-ヒドロキシプロピル）アニリン","N,N-ビス(2-ヒドロキシプロピル)-アニリン","75）N,N-Bis (2-hydroxypropyl)aniline",null,"0003077-13-2","〇","〇","〇","〇","〇","III",3]
[794,null,null,"76）N,N,N',N'-テトラキス（2-ヒドロキシプロピル)エチレンジアミン","N,N,N',N'-テトラキス(2-ヒドロキシプロピル)-エチレンジアミン","76）N,N,N',N'-Tetrakis(2-hydroxypropyl)ethylenediamine",null,"0000102-60-3","〇","〇","〇","〇","〇","III",3]
[]
[null,null,"６５．シリコ－ン樹脂（SI)"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[null,null,1,"以下のモノマーから合成される直鎖または分岐状の有機ポリシロキサン。",null,null,null,"ー","＊以下の各構成モノマーの制限に従う",null,null,null,null,null,null,"区分４との混合（５％以下）では使用可能食品は全食品"]
[536,null,null,"メチルトリメトキシシラン","メチルトリメトキシシラン","Methyltrimethoxysilane",null,"1185-55-3","ー","○","○","ー","○","Ⅲ",1,"他の基ポリマーと混合する場合は、その制限に従う"]
[531,null,null,"メチルトリエトキシシラン","トリエトキメチルシシラン","Methyltriethoxysilane",null,"2031-67-6","ー","○","○","ー","○","Ⅲ",1,"他の基ポリマーと混合する場合は、その制限に従う"]
[529,null,null,"ジメチルジメトキシシラン","ジメチルジメトキシシラン","Dimethyldimethoxysilane",null,"1112-39-6","ー","○","○","ー","○","Ⅲ",1]
[522,null,null,"ジメチルジエトキシシラン","ジエトキシジメチルシラン","Dimethyldiethoxysilane",null,"78-62-6","ー","○","○","ー","○","Ⅲ",1]
[533,null,null,"メチルトリクロロシラン","トリクロロメチルシラン","Methytrichlorosilane",null,"75-79-6","ー","○","○","ー","○","Ⅲ",1,"他の基ポリマーと混合する場合は、その制限に従う"]
[524,null,null,"ジメチルジクロロシラン","ジクロロジメチルシラン","Dimethyldichlorosilane",null,"75-78-5","ー","○","○","ー","○","Ⅲ",1]
[532,null,null,"フェニルトリクロロシラン","トリクロロフェニルシラン","Phenyltrichlorosilane",null,"98-13-5","ー","○","○","ー","○","Ⅲ",1]
[527,null,null,"ジフェニルジメトキシシラン","ジフェニルジメトキシシラン","Diphenyldimethoxysilane",null,"6843-66-9","ー","○","○","ー","○","Ⅲ",1]
[535,null,null,"フェニルトリメトキシシラン","フェニルトリメトキシシラン","Phenyltrimethoxysilane",null,"2996-92-1","ー","○","○","ー","○","Ⅲ",1]
[530,null,null,"フェニルトリエトキシシラン","トリエトキシフェニルシラン","Phenyltriethoxysilane",null,"780-69-8","ー","○","○","ー","○","Ⅲ",1]
[521,null,null,"ジフェニルジエトキシシラン","ジエトキシジフェニルシラン","Diphenyldiethoxysilane",null,"2553-19-7","ー","○","○","ー","○","Ⅲ",1]
[534,null,null,"ビニルトリメトキシシラン","ビニルトリメトキシシラン","Vinyltrimethoxysilane",null,"2768-02-7","ー","○","○","ー","○","Ⅲ",1]
[528,null,null,"ジメチルクロロシラン","クロロジメチルシラン","Dimethylchlorosilane",null,"1066-35-9","ー","○","○","ー","○","Ⅲ",1]
[523,null,null,"ジフェニルジクロロシラン","ジクロロジフェニルシラン","Diphenyldichlorosilane",null,"0000080-10-4","ー","○","○","ー","○","Ⅲ",1]
[520,null,null,"クロロジメチルビニルシラン","クロロビニルジメチルシラン"," Chlorodimethylvinylsilane",null,"0001719-58-0","ー","○","○","ー","○","Ⅲ",1]
[526,null,null,"ジクロロメチルシラン","ジクロロメチルシラン","Dichloro(methyl)silane",null,"0000075-54-7","ー","○","○","ー","○","Ⅲ",1]
[519,null,null,"クロロトリメチルシラン","クロロトリメチルシラン","Chloro(trimethyl)silane",null,"0000075-77-4","ー","○","○","ー","○","Ⅲ",1]
[525,null,null,"ジクロロメチルビニルシラン","ジクロロビニルメチルシラン","Dichloro(methyl)(vinyl)silane",null,"0000124-70-9","ー","○","○","ー","○","Ⅲ",1]
[null,null,2,"以下のモノマーから合成される分岐状の有機変成ポリシロキサン。",null,null,null,"ー","＊以下の各構成モノマーの制限に従う"]
[538,null,null,"イソフタル酸",null,"Isophthalic acid",null,"121-91-5","ー","○","○","ー","○","Ⅲ",1]
[543,null,null,"テレフタル酸",null,"Terephthalic acid",null,"100-21-0","ー","○","○","ー","○","Ⅲ",1]
[544,null,null,"トリメチロールエタン",null,"Trimethylolethane",null,"77-85-0","ー","○","○","ー","○","Ⅲ",1]
[545,null,null,"トリメチロールプロパン",null,"Trimethylolpropane",null,"77-99-6","ー","○","○","ー","○","Ⅲ",1]
[539,null,null,"エチレングリコール",null,"1, 2-Ethanediol",null,"107-21-1","ー","○","○","ー","○","Ⅲ",1]
[548,null,null,"メチルトリメトキシシラン",null,"Methyltrimethoxysilane",null,"1185-55-3","ー","○","○","ー","○","Ⅲ",1]
[542,null,null,"ジメチルジメトキシシラン",null,"Dimethyldimethoxysilane",null,"1112-39-6","ー","○","○","ー","○","Ⅲ",1]
[547,null,null,"フェニルトリメトキシシラン",null,"Phenyltrimethoxysilane",null,"2996-92-1","ー","○","○","ー","○","Ⅲ",1]
[546,null,null,"ビニルトリメトキシシラン",null,"Vinyltrimethoxysilane",null,"2768-02-7","ー","○","○","ー","○","Ⅲ",1]
[541,null,null,"ジメチルクロロシラン",null,"Dimethylchlorosilane",null,"1066-35-9","ー","○","○","ー","○","Ⅲ",1]
[540,null,null,"1,2-エポキシ-4-ビニルシクロヘキサン","1,2-エポキシ-4-ビニルシクロヘキサン","1,2-Epoxy-4-vinylcyclohexane",null,"0000106-86-5","ー","○","○","ー","○","III",1]
[]
[null,null,"６６．合成吸着剤及びイオン交換樹脂"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[465,null,1,"ジビニルベンゼン単独重合体",null,"Divinylbenzene polymer, ",null,"9003-69-4","〇","〇","〇","〇","〇","Ⅱ",1]
[462,null,2,"スチレン・ジビニルベンゼン共重合体",null,"Styrene-divinylbenzene copolymer, ",null,"ー","〇","〇","〇","〇","〇","Ⅱ",1]
[425,null,3,"スチレン・ジビニルベンゼン・エチルスチレン共重合体",null,"Benzene,diethenyl-, polymer with ethenylbenzene and ethenylethylbenzene",null,"9052-95-3","〇","〇","〇","〇","〇","Ⅲ",3]
[466,null,4,"スチレン・ジビニルベンゼン・エチルスチレン共重合体臭素化物　",null,"Benzene, diethenyl-, polymer with ethenylbenzene and ethenylethylbenzene, brominated",null,"905310-11-4","〇","〇","〇","〇","〇","Ⅲ",3]
[424,null,5,"ジビニルベンゼン・エチルスチレン共重合体",null,"Benzene, diethenyl-, polymer with ethenylethylbenzene",null,"9043-77-0","〇","〇","〇","〇","〇","Ⅲ",3]
[479,null,6,"メタクリル酸メチル、エチレングリコールビスメタクリレートの共重合体",null,"2-Propenoic acid, 2-methyl-, 1,2-ethanediyl ester, polymer with methyl 2-methyl-2-propenoate",null,"25777-71-3","〇","〇","〇","〇","〇","Ⅲ",3]
[478,null,7,"エチレングリコールビスメタクリレート、グリシジルメタクリレートの共重合体",null,"2-Propenoic acid, 2-methyl-, 1,2-ethanediyl ester, polymer with oxiranylmethyl 2-methyl-2-propenoate",null,"31743-77-8","〇","〇","〇","〇","〇","Ⅰ",3]
[446,null,8,"エチレングリコールビスメタクリレート、グリシジルメタクリレートの共重合体の加水分解物",null,"2-Propenoic acid, 2-methyl-, 1,2-ethanediyl ester, polymer with oxiranylmethyl 2-methyl-2-propenoate, hydrolyzed",null,"116010-50-5","〇","〇","〇","〇","〇","Ⅰ",3]
[436,null,9,"エチレングリコールビスメタクリレート、グリシジルメタクリレートの共重合体の２－アクリロイルアミノ－２－メチル－１－プロパンスルホン酸、Ｎ－（２－ヒドロキシエチル）アクリルアミドの共重合体および水の付加物のナトリウム塩",null,"2-Propenoic acid, 2-methyl-, 1,1'-(1,2-ethanediyl) ester, polymer with N-(2-hydroxyethyl)-2-propenamide, 2-methyl-2-[(1-oxo-2-propen-1-yl)amino]-2-propanesulfonic acid and 2-oxiranylmethyl 2-methyl-2-propenoate, hydrolyzed, odium salts\n",null,"1569066-79-0","〇","〇","〇","〇","〇","Ⅰ",3]
[434,null,10,"エチレングリコールビスメタクリレート、グリシジルメタクリレートの共重合体のＮ－（２－ヒドロキシエチル）アクリルアミド重合体および水の付加物のトリメチル（オキシラン－２－イルメチル）アンモニウム＝クロリドと水酸化ナトリウムの反応生成物の塩酸反応物",null,"2-Oxiranemethanaminium, N,N,N-trimethyl-, chloride (1:1), reaction products with hydrolyzed ethylene dimethacrylate-glycidyl methacrylate-N-(2-hydroxyethyl)-2-propenamide polymer",null,"1569066-80-3","〇","〇","〇","〇","〇","Ⅰ",3]
[438,null,11,"エチレングリコールビスメタクリレート、グリシジルメタクリレートの共重合体のアクリル酸、Ｎ－（２－ヒドロキシエチル）アクリルアミドの共重合体および水の付加物のナトリウム塩",null,"2-Propenoic acid, 2-methyl-, 1,1'-(1,2-ethanediyl) ester, polymer with N-(2-hydroxyethyl)-2-propenamide, 2-oxiranylmethyl 2-methyl-2-propenoate and 2-propenoic acid, hydrolyzed, sodium salt",null,"1569066-76-7","〇","〇","〇","〇","〇","Ⅰ",3]
[444,null,12,"エチレングリコールビスメタクリレート、グリシジルメタクリレートの共重合体のＮ－［３－（Ｎ’，Ｎ’－ジメチルアミノ）プロピル］アクリルアミド、Ｎ－（２－ヒドロキシエチル）アクリルアミドの共重合体および水の付加物の硫酸塩及びリン酸塩",null,"2-Propenoic acid, 2-methyl-, 1,1'-(1,2-ethanediyl) ester, polymer with N-[3-(dimethylamino)propyl]-2-propenamide, \nN-(2-hydroxyethyl)-2-propenamide and 2-oxiranylmethyl 2-methyl-2-propenoate, hydrolyzed, phosphates (salts)  sulfates (salts)\n",null,"1569066-77-8","〇","〇","〇","〇","〇","Ⅰ",3]
[437,null,13,"［エチレングリコールビスメタクリレート、グリシジルメタクリレートの共重合体］と２－アクリロイルアミノ－２－メチル－１－プロパンスルホン酸のナトリウム塩の共重合体の水付加物のナトリウム塩",null,"2-Propenoic acid, 2-methyl-, 1,1'-(1,2-ethanediyl) ester, polymer with 2-methyl-2-[(1-oxo-2-propen-1-yl)amino]-2-propanesulfonic acid and 2-oxiranylmethyl 2-methyl-2-propenoate, \nhydrolyzed, sodium salts",null,"ー","〇","〇","〇","〇","〇","Ⅰ",3]
[445,null,14,"［エチレングリコールビスメタクリレート、グリシジルメタクリレートの共重合体］と３－（アクリロイルアミノ）プロピルトリメチルアンモニウム＝クロリド、Ｎ－（２－ヒドロキシエチル）アクリルアミドの共重合体の水付加物",null,"1-​Propanaminium, N,​N,​N-​trimethyl-​3-​[(1-​oxo-​2-​propen-​1-​yl)​amino]​-​, chloride (1:1), reaction products with hydrolyzed ethylene dimethacrylate-glycidyl methacrylate-N-(2-hydroxyethyl)-2-propenamide polymer",null,"ー","〇","〇","〇","〇","〇","Ⅰ",3]
[435,null,15,"［エチレングリコールビスメタクリレート、グリシジルメタクリレートの共重合体］とＮ－［３－（Ｎ’，Ｎ’－ジメチルアミノ）プロピル］アクリルアミド、Ｎ－（２－ヒドロキシエチル）アクリルアミドの共重合体の水付加物",null,"2-Propenoic acid, 2-methyl-, 1,1'-(1,2-ethanediyl) ester, polymer with N-[3-(dimethylamino)propyl]-2-propenamide, \nN-(2-hydroxyethyl)-2-propenamide and 2-oxiranylmethyl 2-methyl-2-propenoate, hydrolyzed",null,"ー","〇","〇","〇","〇","〇","Ⅰ",3]
[472,null,16,"スチレン・ジビニルベンゼン共重合体スルホン化物",null,"Benzene, diethenyl-, polymer with ethenylbenzene, sulfonated",null,"68037-26-3","〇","ー","〇","〇","〇","Ⅱ",1]
[459,null,17,"スチレン・ジビニルベンゼン共重合体クロロメチル化物とジメチルアミンの反応生成物",null,"Methanamine, N-methyl-, reaction products with chloromethylated divinylbenzene-styrene polymer",null,"68441-29ｰ2","〇","ー","〇","〇","〇","Ⅱ",1]
[474,null,18,"テトラフルオロエチレン・４－（トリフルオロビニルオキシ）ヘキサフルオロ酪酸共重合物",null,"Tetrafluoroethylene • 4- (trifluorovinyloxy) hexafluorobutyric acid copolymer",null,"83560-40-1","〇","ー","ー","ー","〇","Ⅱ",3]
[473,null,19,"テトラフルオロエチレン・２－［２－（トリフルオロビニルオキシ）－１－（トリフルオロメチル）トリフルオロエトキシ］テトラフルオロエタンスルホン酸共重合物",null,"Tetrafluoroethylene • 2- [2- (trifluorovinyloxy) -1- (trifluoromethyl) trifluoroethoxy] tetrafluoroethanesulfonic acid copolymer",null,"31175-20-9","〇","〇","〇","〇","〇","Ⅱ",3]
[431,null,20,"スチレン・ジビニルベンゼン・エチルジビニルベンゼン・トリメチル［４－（４－ビニルフェニル）ブチル］アンモニウムブロミドの共重合物",null,"Copolymer of styrene, divinylbenzene, ethylvinylbenzene, and trimethyl[4-(4-vinylphenyl)butyl]ammonium bromide",null,"ー","〇","〇","〇","〇","〇","Ⅱ",3]
[432,null,21,"スチレン・ジビニルベンゼン・エチルビニルベンゼン・ビニルベンジルトリメチルアンモニウムクロリド共重合体",null,"Copolymer of styrene, divinylbenzene, ethylvinylbenzene, and  vinylbenzyltrimethylammonium  chloride",null,"69011-19-4","〇","〇","〇","〇","〇","Ⅰ",3]
[475,null,22,"ビフェニル基上にトリメチルアンモニオメチル基を有し、ビフェニル基間が２，２，６，６－テトラメチル－２，６－ジアゾニアヘプタン－１，７－ジイル基で架橋されたポリフェニルサルホン樹脂","N,N,N,N',N',N'-ヘキサメチル-1,3-プロパンジアンモニウムでビフェニル基を架橋されたポリフェニルサルホン","Polyphenylsulfone  , trimethylammoniomethylated on biphenyl moiety, crosslinked between biphenyl moieties by 2,2,6,6-tetramethyl-2,6-diazoniaheptane-1,7-diyl group",null,"－","〇","〇","〇","〇","〇","Ⅰ",3]
[430,null,23,"スチレン・ジビニルベンゼン・エチルビニルベンゼン・Ｎ－ビニルベンジル－Ｎ，Ｎ，Ｎ－トリメチルアンモニウムクロライド・Ｎ，Ｎ－ジメチル－Ｎ－（６－ジメチルアミノヘキシル）アンモニオメチルスチレンクロリド・１，６－ビス（Ｎ－ビニルベンジル－Ｎ、Ｎ－ジメチルアンモニオ）ヘキサンジクロリド共重合体",null,"Copolymer of styrene, divinylbenzene, ethylvinylbenzene,  N-vinylbenzylN,N,N-trimethylammonium chloride, N,N-dimethyl-N-(6-dimethylaminohexyl)ammoniomethylstyrene chloride, and 1,6-bis(N-vinylbenzyl-N,N-dimethylammonio)hexane dichloride",null,"60177-39-1","〇","〇","〇","〇","〇","Ⅰ",3]
[429,null,24,"スチレン・ジビニルベンゼン・エチルビニルベンゼン・ビニルベンジルトリメチルアンモニウムクロライド・Ｎ，Ｎ－ジメチルアミノメチルスチレン・Ｎ，Ｎ－ジメチル－Ｎ，Ｎ－ビス（ビニルフェニルメチル）アンモニウムクロリド共重合体",null,"Copolymer of styrene, divinylbenzene, ethylvinylbenzene,  vinylbenzyltrimethylammonium chloride, N,N-dimethylaminomethylstyrene, and N,N-dimethyl-N,N-bis(vinylphenylmethyl)ammonium chloride",null,"60177-39-1","〇","〇","〇","〇","〇","Ⅰ",3]
[418,null,25,"スチレンスルホン酸・アクリル酸・ジビニルベンゼン・エチルビニルベンゼン共重合物",null,"Copolymer of styrene sulfonic acid, acrylic acid, divinylbenzene, and ethylbinylbenzene",null,"68441-33-8","〇","〇","〇","〇","〇","Ⅰ",3]
[433,null,26,"スチレンスルホン酸・アクリル酸・ジビニルベンゼン・エチルビニルベンゼン共重合物とエテン・３，３，４，４，５，５，６，６，６－ノナフルオロヘキサ－１－エン・ペルフルオロエテン共重合物の架橋物",null,"Crosslinked material of  Copolymer of styrene sulfonic acid, acrylic acid, divinylbenzene, and ethylbinylbenzene with copolymer of ethane, 3,3,4,4,5,5,6,6,6-nonafluorohexa-1-ene, and   1,1,2,2-tetrafluoroethene",null,"ー","〇","〇","〇","〇","〇","Ⅰ",3]
[423,null,27,"塩化ビニル・アクリロニトリル共重合体、メタクリル酸グリシジルエステル重合体、及びイミノジ酢酸の反応生成物のナトリウム塩","アクリロニトリル・塩化ビニル共重合体、メタクリル酸グリシジル単独重合体及びイミノジ酢酸の反応生成物のナトリウム塩","2-Propenenitrile, polymer with chloroethene and 2-Propenoic acid, 2-methyl-, 2-oxiranylmethyl ester, homopolymer, reaction products with iminodiacetic acid, sodium salts",null,"－","○","○","○","○","○","II",3]
[463,null,28,"スチレン・ジビニルベンゼン共重合体のアミノリン酸塩","ジビニルベンゼン・スチレン共重合体のアミノメチルホスホン酸塩","Styrene-divinylbenzene copolymer, amino methyl phosphonic acid",null,"－","○","○","○","○","○","Ⅰ",3]
[464,null,29,"スチレン・ジビニルベンゼン共重合体のイミノジ酢酸塩","ジビニルベンゼン・スチレン共重合体のイミノジ酢酸塩","Styrene-divinylbenzene copolymer, immodiacetic acid",null,"－","○","○","○","○","○","Ⅰ",3]
[467,null,30,"エチルスチレン・スチレン・ジビニルベンゼン共重合物のスルホン化物","スルホン化処理されたエチルスチレン・ジビニルベンゼン・スチレン共重合体","Benzene,diethenyl-, polymer with ethenylbenzene and ethenylethylbenzene, sulfonated",null,"0069011-20-7","○","○","○","○","○","II",3]
[471,null,31,"エチルスチレン・スチレン・ジビニルベンゼン共重合物のスルホン化物のナトリウム塩","スルホン化処理されたエチルスチレン・ジビニルベンゼン・スチレン共重合体のナトリウム塩","Benzene,diethenyl-, polymer with ethenylbenzene and ethenylethylbenzene, sulfonated, sodium salts",null,"0069011-22-9","○","○","○","○","○","II",3]
[469,null,32,"エチルスチレン・スチレン・ジビニルベンゼン共重合物のスルホン化物のカルシウム塩","スルホン化処理されたエチルスチレン・ジビニルベンゼン・スチレン共重合体のカルシウム塩","Benzene,diethenyl-, polymer with ethenylbenzene and ethenylethylbenzene, sulfonated, calcium salts",null,"0071786-43-1","○","○","○","○","○","II",3]
[468,null,33,"エチルスチレン・スチレン・ジビニルベンゼン共重合物のスルホン化物のカリウム塩","スルホン化処理されたエチルスチレン・ジビニルベンゼン・スチレン共重合体のカリウム塩","Benzene, diethenyl-, polymer with ethenylbenzene and ethenylethylbenzene, sulfonated, potassium salts",null,"0068584-07-6","○","○","○","○","○","II",3]
[470,null,34,"エチルスチレン・スチレン・ジビニルベンゼン共重合物の臭素化物のスルホン化物","スルホン化処理されたエチルスチレン・ジビニルベンゼン・スチレン共重合体の臭素化物","Benzene, diethenyl-, polymer with ethenylbenzene and ethenylethylbenzene, brominated,　sulfonated　",null,"0125935-37-7","○","○","○","○","○","II",3]
[455,null,35,"エチルスチレン・ジビニルベンゼン・スチレン共重合物のクロロメチル化物とトリメチルアミンの反応生成物（Ｃｌ型）","クロロメチル化処理されたエチルスチレン・ジビニルベンゼン・スチレン共重合体とトリメチルアミンの反応生成物の塩化物","Benzene, diethenyl-, polymer with ethenylbenzene and ethenylethylbenzene, chloromethylated, trimethylamine-quaternized ",null,"0069011-19-4","○","○","○","○","○","II",3]
[457,null,36,"エチルスチレン・スチレン・ジビニルベンゼン共重合物のクロロメチル化物とトリメチルアミンの反応生成物（ＯＨ形）","クロロメチル化処理されたエチルスチレン・ジビニルベンゼン・スチレン共重合体とトリメチルアミンの反応生成物の水酸化物","Benzene, diethenyl-, polymer with ethenylbenzene and ethenylethylbenzene, chloromethylated, trimethylamine-quaternized, hydroxide",null,"0069011-18-3","○","○","○","○","○","II",3]
[456,null,37,"エチルスチレン・スチレン・ジビニルベンゼン共重合物のクロロメチル化物とトリメチルアミンの反応生成物（ＨＣＯ３形）","クロロメチル化処理されたエチルスチレン・ジビニルベンゼン・スチレン共重合体とトリメチルアミンの反応生成物の炭酸塩","Benzenemethanaminium, ar-ethenyl-N,N,N-trimethyl-, polymer with diethenylbenzene and ethenylethylbenzene, carbonate ",null,"0121212-42-8","○","○","○","○","○","II",3]
[458,null,38,"エチルスチレン・スチレン・ジビニルベンゼン共重合物のクロロメチル化物とトリメチルアミンの反応生成物（ＳＯ４形）","クロロメチル化処理されたエチルスチレン・ジビニルベンゼン・スチレン共重合体とトリメチルアミンの反応生成物の硫酸塩","Benzene, diethenyl-, polymer with ethenylbenzene and ethenylethylbenzene, chloromethylated, trimethylamine-quaternized, sulphate",null,"－","○","○","○","○","○","II",3]
[448,null,39,"エチルスチレン・スチレン・ジビニルベンゼン共重合物のクロロメチル化物と２－（Ｎ，Ｎ－ジメチルアミノ）エタノールの反応生成物（Ｃｌ形）","クロロメチル化処理されたエチルスチレン・ジビニルベンゼン・スチレン共重合体と2-(ジメチルアミノ)エタノールの反応生成物","Benzene, diethenyl-, polymer with ethenylbenzene and ethenylethylbenzene, chloromethylated, 2-(dimethylamino) ethanol-quaternized ",null,"0069011-15-0","○","○","○","○","○","II",3]
[449,null,40,"エチルスチレン・スチレン・ジビニルベンゼン共重合物のクロロメチル化物と２－（Ｎ，Ｎ－ジメチルアミノ）エタノールの反応生成物（ＯＨ形）","クロロメチル化処理されたエチルスチレン・ジビニルベンゼン・スチレン共重合体と2-(ジメチルアミノ)エタノールの反応生成物の水酸化物","Benzene, diethenyl-, polymer with ethenylbenzene and ethenylethylbenzene, chloromethylated, 2-(dimethylamino) ethanol-quaternized, hydroxyde ",null,"0069011-16-1","○","○","○","○","○","II",3]
[452,null,41,"エチルスチレン・スチレン・ジビニルベンゼン共重合物のクロロメチル化物とジメチルアミンの反応生成物","クロロメチル化処理されたエチルスチレン・ジビニルベンゼン・スチレン共重合体とジメチルアミンの反応生成物","Methanamine, N-methyl-,reactionproducts with chloromethylated divinylbenzene-ethenylethylbenzene-styrene polymer ",null,"0069011-17-2","○","○","○","○","○","II",3]
[447,null,42,"エチルスチレン・スチレン・ジビニルベンゼン共重合物のクロロメチル化物とN-(2-アミノメチル)-1,2-ジアミンの反応生成物","クロロメチル化処理されたエチルスチレン・ジビニルベンゼン・スチレン共重合体とジエチレントリアミンの反応生成物","1,2-Ethanediamine, N-(2-aminoethyl)-,reaction products with chloromethylated divinylbenzene-ethenylethylbenzene-styrene-polymer",null,"0068584-04-3","○","○","○","○","○","II",3]
[451,null,43,"エチルスチレン・スチレン・ジビニルベンゼン共重合物のクロロメチル化物とトリメチルアミン及びジメチルアミンの反応生成物","クロロメチル化処理されたエチルスチレン・ジビニルベンゼン・スチレン共重合体とジメチルアミン及びトリメチルアミンの反応生成物の塩酸塩","Benzene, diethenyl-, polymer with ethenylbenzene and ethenylethylbenzene, chloromethylated, reaction products with dimethylamine and trimethylamine, hydrochlorides",null,"1835706-66-5","○","○","○","○","○","II",3]
[454,null,44,"エチルスチレン・スチレン・ジビニルベンゼン共重合物のクロロメチル化物のＮ，Ｎ－ビス（ソディウムカルボキシメチル）アミノ化物","クロロメチル化処理されたエチルスチレン・ジビニルベンゼン・スチレン共重合体とニトリロトリ酢酸トリエチルの反応生成物のナトリウム塩酸塩","Glycine, N-(2-ethoxy-2-oxoethyl)- ethyl ester, reaction products with chloromethylated divinylbenzene-ethenylethylbenzene-styrene polymer, hydrolyzed, sodium salt",null,"1167421-36-4","○","○","○","○","○","II",3]
[453,null,45,"エチルスチレン・スチレン・ジビニルベンゼン共重合物のクロロメチル化物と１－デオキシ－１－（メチルアミノ）－Ｄ－グルシトールの反応生成物","クロロメチル化処理されたエチルスチレン・ジビニルベンゼン・スチレン共重合体と1-デオキシ-1-メチルアミノソルビトールの反応生成物の加水分解物","Glycine, N,N-dimethyl-, ethyl ester, reaction products with chloromethylated divinylbenzene-ethenylethylbenzene-styrene polymer, hydrolyzed",null,"0071799-50-3","○","○","○","○","○","II",3]
[450,null,46,"エチルスチレン・スチレン・ジビニルベンゼン共重合物のクロロメチル化物と2-(ジメチルアミノ)酢酸エチルの反応生成物の加水分解物 ","クロロメチル化処理されたエチルスチレン・ジビニルベンゼン・スチレン共重合体と2-(ジメチルアミノ)酢酸エチルの反応生成物の加水分解物","Glycine, N,N-dimethyl-, ethyl ester, reaction products with chloromethylated divinylbenzene-ethenylethylbenzene-styrene polymer, hydrolyzed",null,"1167421-50-2","○","○","○","○","○","II",3]
[428,null,47,"エチルスチレン・メタクリル酸・メタクリル酸メチル・ジビニルベンゼン共重合物","エチルスチレン・ジビニルベンゼン・メタクリル酸・メタクリル酸 メチル共重合体","2-Propenoic acid, 2-methyl ,methyl ester, polymer with diethenylbenzene and ethenylethylbenzene, hydorolyzed",null,"0111559-80-9","○","○","○","○","○","II",3]
[422,null,48,"アクリロニトリル・エチルスチレン・スチレン・ジビニルベンゼン共重合物","アクリロニトリル・エチルスチレン・ジビニルベンゼン・スチレン共重合体","2-Propenenitrile, polymer with diethenylbenzene, ethenylbenzene and ethenylethylbenzene",null,"0072936-61-9","○","○","○","○","○","II",3]
[476,null,49,"２，３－エポキシプロピル＝メタクリラート・エチレン＝ジメタクリラート共重合物の水及びジエチルアミン付加物","メタクリル酸グリシジル・メタクリル酸とエチレングリコールのジエステル共重合体とジエチルアミンの反応生成物","2-Propenoic acid, 2-methyl-, 1,1'-(1,2-ethanediyl) ester, polymer with 2-oxiranylmethyl 2-methyl-2-propenoate, reaction products with diethylamine",null,"0125476-72-4","○","○","○","○","○","I",3]
[477,null,50,"２，３－エポキシプロピル＝メタクリラート・エチレン＝ジメタクリラート共重合物の水及びヘキサメチレンジアミン付加物","メタクリル酸グリシジル・メタクリル酸とエチレングリコールのジエステル共重合体とヘキサメチレンジアミンの反応生成物","2-Propenoic acid, 2-methyl-, 1,1'-(1,2-ethanediyl) ester, polymer with 2-oxiranylmethyl 2-methyl-2-propenoate, reaction products with  hexamethylenediamine, hydrolyzed",null,"－","○","○","○","○","○","I",3]
[426,null,51,"４－(４－ブロモブチル)スチレン・エチルスチレン・ジビニルベンゼン共重合物とトリメチルアミンの反応生成物（Br形→Cl形）","エチルスチレン・ジビニルベンゼン・4-(4-ブロモブチル)スチレン共重合物とトリメチルアミンの反応生成物の塩化物","Methanamine, N,N-dimethyl-, compd. with (4-bromobutyl) ethenylbenzene polymer with diethenylbenzene and ethenylethylbenzene",null,"0148601-45-0","○","○","○","○","○","III",3]
[427,null,52,"４－(４－ブロモブチル)スチレン・エチルスチレン・ジビニルベンゼン共重合物とトリメチルアミンの反応生成物（ＯＨ形）","エチルスチレン・ジビニルベンゼン・4-(4-ブロモブチル)スチレン共重合物とトリメチルアミンの反応生成物の水酸化物","Methanamine, N,N-dimethyl-, compd. with (4-bromobutyl) ethenylbenzene polymer with diethenylbenzene and ethenylethylbenzene, hydroxide",null,"－","○","○","○","○","○","III",3]
[480,null,53,"ベンジル＝２－メチルプロパ－２－エノアート・エタン－１，２－ジイル＝ビス（２－メチルプロパ－２－エノアート）共重合物","メタクリル酸ベンジル・メタクリル酸とエチレングリコールのジエステル共重合体","2-Propenoic acid, 2-methyl-, 1,1'-(1,2-ethanediyl) ester, polymer with phenylmethyl 2-methyl-2-propenoate",null,"0126969-53-7","○","○","○","○","○","II",3]
[442,null,54,"エチレン＝ジメタクリラート・オキシラン－２－イルメチル＝メタクリラート共重合物とポリエチレンイミンと水の反応生成物","加水分解処理されたアジリジン・ジエチレントリアミン・メタクリル酸グリシジル・メタクリル酸とエチレングリコールのジエステル共重合体","2-Propenoic acid, 2-methyl-, 1,1'-(1,2-ethanediyl) ester, polymer with N1-(2-aminoethyl) -1, 2-ethanediamine, aziridine and 2-oxiranylmethyl 2-methyl-2-propenoate, hydrolyzed",null,"－","○","○","○","○","○","I",3]
[419,null,55,"アクリル酸・ジビニルベンゼン共重合物","アクリル酸・ジビニルベンゼン共重合体","2-Propenoic acid, polymer with diethenylbenzene",null,"0009052-45-3","○","○","○","○","○","II",3]
[415,null,56,"トリメチルアミノプロピルアクリルアミドクロリド・ジビニルベンゼン・エチルスチレン・ジエチレングリコールジビニルエーテル共重合物","N-アクリルアミドプロピル-N,N,N-トリメチルアンモニウムの塩化物・ジエチレングリコールのジビニルエーテル・ジビニルベンゼン共重合体","1-Propanaminium, N,N,N-trimethyl-3-[(1-oxo-2-propen-1-yl)amino]-, chloride (1:1), polymer with diethenylbenzene and 1,1'-[oxybis(2,1-ethanediyloxy)]bis[ethene]",null,"0065997-24-2","○","○","○","○","○","II",3]
[440,null,57,"エチルスチレン・ジビニルベンゼン・N-ビニルホルムアミド・アクリロニトリル共重合物の加水分解物","加水分解処理されたアクリロニトリル・エチルスチレン・ジビニルベンゼン・スチレン・N-ビニル-ホルムアミド共重合体","2-Propenenitrile, polymer with diethenylbenzene, ethenylbenzene, ethenylethylbenzene, and formamide, -ethenyl-, hydrolyzed",null,"－","○","○","○","○","○","II",3]
[416,null,58,"アクリル酸エチル・エチルスチレン・ジビニルベンゼン・N-[3-（N’，N’-ジメチルアミノ)プロピル]アクリルアミド共重合物","アクリル酸エチル・エチルスチレン・ジビニルベンゼン共重合体とN, N-ジメチル-1, 3-プロパンジアミンの反応生成物","2-Propenoic acid, ethyl ester, polymer with diethenylbenzene and ethenylethylbenzene, reaction products with N1, N1-dimethyl-1, 3-propanediamine",null,"1987891-51-9","○","○","○","○","○","II",3]
[439,null,59,"アクリル酸メチル・アクリロニトリル・エチルスチレン・オクタ－１，７－ジエン・ジビニルベンゼン共重合物の加水分解物","加水分解処理されたアクリル酸メチル・アクリロニトリル・エチルスチレン・1,7-オクタジエン・ジビニルベンゼン共重合物","2-Propenoic acid, methyl ester, polymer with diethenylbenzene, ethenylethylbenzene, and 2-propenenitrile, hydrolyzed",null,"1026769-18-5","○","○","○","○","○","II",3]
[417,null,60,"アクリル酸・ジビニルベンゼン・エチルスチレン共重合物","アクリル酸・エチルスチレン・ジビニルベンゼン共重合体","2-Propenoic acid, polymer with diethenylbenzene, ethenylbenzene and ethenylethylbenzene",null,"0062612-13-9","○","○","○","○","○","II",3]
[420,null,61,"アクリル酸重合物　ナトリウム中和塩　（架橋物）","アクリル酸単独重合体のナトリウム塩","2-Propenoic acid, homopolymer, sodium salt, neutralized, cross-linked",null,"0009003-04-7","ー","○","ー","ー","○","Ⅰ",3]
[421,null,62,"アクリロニトリル・アクリル酸アルキルエステル・アクリル酸軽金属塩（Li,Na, K, Ca, Mg)の共重合体","アルキルの範囲不明","Acrylonitrile · acrylic acid alkyl ester · acrylic acid light metal salt copolymer (Li, Na, K, Ca, Mg, Al)",null,"－","○","○","○","○","○","Ⅰ",3]
[461,null,63,"レゾルシン・m-フェニレンジアミン・ホルムアルデヒド共重合体","1,3-ヒドロキシベンゼン・1,3-ベンゼンジアミン・ホルムアルデヒド共重合体","1,3-Benzenediol / 1,3-Benzenediamine, Polymer with Formaldehyde",null,"0029227-50-7","○","○","○","○","○","Ⅱ",1]
[460,null,64,"ピロガロール・レゾルシン・ホルムアルデヒド共重合体","1,3-ヒドロキシベンゼン・ピロガロール・ホルムアルデヒド共重合体","1,2,3-Benzenetriol / 1,3-Benzenediol, Polymer with Formaldehyde",null,"0027878-51-9","○","○","○","○","○","Ⅱ",1]
[441,null,65,"アクリロニトリル・ジビニルベンゼン共重合体のカルボン酸塩","カルボン酸の意味不明\nカルボン酸の詳細不明","Acrylonitrile-divinylbenzene copolymer, carboxylic acid",null,"－","○","○","○","○","○","Ⅱ",3]
[443,null,66,"メタクリル酸メチル・ジビニルベンゼン共重合体のカルボン酸塩","カルボン酸の意味不明\nカルボン酸の詳細不明","Methyl methacrylate-divinylbenzene copolymer, carboxylic acid",null,"－","○","○","○","○","○","Ⅱ",3]
[481,null,67,"上記１から６６以外の物質であって、下記の１種類以上の（a)と１種類以上の（ｃ）の反応によって得られる物質を必要に応じ１種類以上の（d）で処理した重合体に、又は１種類以上の（ｂ）を必要に応じ１種類以上の（d）で処理した重合体に、必要に応じ１種類以上の（e)を反応させたイオン交換樹脂","ー",null,null,null,"＊以下の各構成物質の制限に従う"]
[null,null,null,"(a)","ー"]
[487,null,null,"スチレン","スチレン","Styrene",null,"0000100-42-5","○","〇","○","○","○","Ⅱ",3]
[485,null,null,"クロロメチルスチレン（m-／p-混合）","クロロメチルスチレン","Vinylbenzyl chloride",null,"0030030-25-2","○","ー","○","○","○","Ⅰ",3,"m-体／p-体＝40/60～70/30"]
[486,null,null,"4-ビニルベンジルクロリド","4-(クロロメチル)スチレン","4-Vinylbenzyl chloride",null,"0001592-20-7","○","ー","○","○","○","Ⅰ",3]
[492,null,null,"メチルスチレン","メチルスチレン","Vinyltoluene",null,"0025013-15-4","○","ー","○","○","○","Ⅰ",3]
[491,null,null,"t-ブチルスチレン","t-ブチルスチレン","4-tert-Butylstyrene",null,"0001746-23-2","○","ー","○","○","○","Ⅰ",3]
[493,null,null,"α－メチルスチレン","α-メチルスチレン","alpha-Methyl styrene",null,"0000098-83-9","○","ー","○","○","○","Ⅰ",3]
[483,null,null,"アクリロニトリル","アクリロニトリル","Acrylonitrile",null,"0000107-13-1","○","ー","○","○","○","Ⅰ",3]
[484,null,null,"エチルビニルベンゼン","エチルビニルベンゼン","Ethylstyrene",null,"0028106-30-1","○","ー","○","○","○","Ⅰ",3]
[489,null,null,"４－ビニルピリジン","4-ビニルピリジン","4-vinylpyridine",null,"0000100-43-6","○","ー","○","○","○","Ⅰ",3]
[490,null,null,"２－ビニルピリジン","2-ビニルピリジン","2-Vinylpyridine",null,"0000100-69-6","○","ー","○","○","○","Ⅰ",3]
[488,null,null,"p-キシレンジクロライド","1,4-ビス(クロロメチル)ベンゼン","Alpha,alpha'-dichloro-p-xylene",null,"0000623-25-6","○","ー","○","○","○","Ⅰ",3]
[null,null,null,"（ｂ）","ー"]
[499,null,null,"SEPS（水添スチレン・イソプレンブロック共重合物）",null,"Benzene, ethenyl-, polymer with 2-methyl-1,3-butadiene, hydrogenated",null,"0068648-89-5","○","ー","○","○","○","Ⅰ",3,"スチレン単位含有量50～80質量%"]
[500,null,null,"SEBS（ｽﾁﾚﾝ・ﾌﾞﾀｼﾞｴﾝ共重合体の水素添加物）",null,"Hydrogenated styrene butadiene copolymer",null,"0113659-15-6","○","ー","○","○","○","Ⅰ",3,"スチレン単位含有量20～40質量%\n酸価20mg-CH3ONa／g以下"]
[502,null,null,"ポリフェニレンエーテル",null,"Polyphenyleneether",null,"0024938-67-8","○","ー","○","○","○","Ⅰ",3]
[501,null,null,"ポリスチレン","スチレン単独重合体","Polystyrene",null,"0009003-53-6","○","ー","○","○","○","Ⅰ",3,"揮発分5mg/g以下"]
[null,null,null,"（ｃ）","ー"]
[495,null,null,"ジビニルベンゼン","ジビニルベンゼン","Divinylbenzene ",null,"0001321-74-0","○","〇","○","○","○","Ⅱ",3,"エチルビニルベンゼン含有量45質量％以下"]
[497,null,null,"N,N,N',N'-ﾃﾄﾗメチル-1,6-ﾍｷｻﾝｼﾞｱﾐﾝ","N,N,N',N'-テトラメチル-1,6-ヘキサメチレンジアミン","N,N,N',N'-tetramethylhexamethylenediamine",null,"0000111-18-2","○","ー","○","○","○","Ⅰ",3]
[496,null,null,"1,6-ジブロモヘキサン","1,6-ジブロモヘキサン","1,6-dibromohexane",null,"0000629-03-8","○","ー","○","○","○","Ⅰ",3]
[null,null,null,"（ｄ）","ー"]
[506,null,null,"ホルマリン","ホルムアルデヒド","Formaldehyde",null,"0000050-00-0","○","ー","○","○","○","Ⅰ",3]
[504,null,null,"塩酸","塩酸","Hydrogen chloride",null,"0007647-01-0","○","ー","○","○","○","Ⅰ",3]
[505,null,null,"クロロメチルメチルエーテル","クロロメチル メチル エーテル","Chloro methyl methyl ether",null,"0000107-30-2","○","ー","○","○","○","Ⅱ",3]
[null,null,null,"（e）","ー"]
[510,null,null,"N,N,N',N'-ﾃﾄﾗメチル-1,6-ﾍｷｻﾝｼﾞｱﾐﾝ","N,N,N',N'-テトラメチル-1,6-ヘキサメチレンジアミン","N,N,N',N'-tetramethylhexamethylenediamine",null,"0000111-18-2","○","ー","○","○","○","Ⅰ",3]
[508,null,null,"クロロスルホン酸","クロロスルホン酸","Chlorosulphuric acid",null,"0007790-94-5","○","○","○","○","○","Ⅱ",3]
[513,null,null,"硫酸","硫酸","Sulphuric acid",null,"0007664-93-9","○","ー","○","○","○","Ⅰ",3]
[511,null,null,"トリメチルアミン","トリメチルアミン","Trimethylamine",null,"0000075-50-3","○","ー","○","○","○","Ⅰ",3]
[509,null,null,"ジメチルアミン","ジメチルアミン","Dimethylamine",null,"0000124-40-3","○","〇","○","○","○","Ⅱ",3]
[512,null,null,"ヨウ化メチル　","ヨウ化メチル　","Methyl iodide",null,"0000074-88-4","○","ー","○","○","○","Ⅰ",3]
[]
[null,null,"６７．不飽和ポリエステル樹脂（架橋ポリエステル樹脂）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,null,null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[null,null,1,"下記の１種類以上の不飽和酸及び必要に応じて加えた飽和酸並びに１種類以上のアルコール類及び／又はエポキシ化合物の共重合体を下記の１種類以上の架橋剤で架橋したポリマー。",null,null,null,"ー","＊以下の各構成モノマーの制限に従う",null,null,null,null,null,null,"酸類１当量に対してアルコール類及びエポキシ化合物等（架橋剤を除く）の合計は３当量以下。"]
[null,null,null,"１.    酸類（不飽和酸）"]
[330,null,null,"無水マレイン酸",null,"Maleic Anhydride",null,"108-31-6","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[322,null,null,"マレイン酸",null,"Maleic Acid",null,"110-16-7","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[320,null,null,"フマル酸",null,"Fumaric Acid",null,"110-17-8","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[305,null,null,"イタコン酸",null,"Itaconic Acid",null,"97-65-4","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[307,null,null,"クロトン酸",null,"Crotonic Acid",null,"107-93-7","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[300,null,null,"アクリル酸",null,"Acrylic Acid",null,"79-10-7","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[332,null,null,"メタクリル酸",null,"Methacrylic Acid",null,"79-41-4","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[null,null,null,"２.    酸類（飽和酸）"]
[329,null,null,"無水フタル酸",null,"Phthalic anhydride ",null,"85-44-9","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[319,null,null,"o-フタル酸",null,"Phthalic acid",null,"88-99-3","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[304,null,null,"イソフタル酸",null,"Isophthalic acid",null,"121-91-5","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[314,null,null,"テレフタル酸",null,"Terephthalic acid",null,"100-21-0","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[325,null,null,"テトラヒドロ無水フタル酸",null,"Tetrahydrophthalic anhydride ",null,"85-43-8","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[311,null,null,"テトラヒドロフタル酸",null,"Tetrahydrophthalic acid",null,"88-98-2","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[327,null,null,"エンドメチレンテトラヒドロ無水フタル酸",null,"endo-3,6-Methylene-1,2,3,6-tetrahydrophthalic anhydride",null,"129-64-6","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[301,null,null,"アジピン酸",null,"Adipic acid",null,"124-04-9","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[313,null,null,"セバシン酸",null,"Sebacic acid ",null,"111-20-6","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[326,null,null,"無水トリメリット酸",null,"Trimellitic anhydride",null,"552-30-7","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[317,null,null,"トリメリット酸",null,"Trimellitic acid",null,"528-44-9","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[328,null,null,"無水ピロメリット酸",null,"Pyromellitic dianhydride",null,"89-32-7","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[302,null,null,"アゼライン酸",null,"Azelaic acid",null,"123-99-9","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[321,null,null,"ペラルゴン酸",null,"Pelargonic Acid",null,"112-05-0","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[309,null,null,"コハク酸",null,"Succinic Acid",null,"110-15-6","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[324,null,null,"無水コハク酸",null,"Succinic Anhydride",null,"108-30-5","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[303,null,null,"安息香酸",null,"Benzoic Acid",null,"65-85-0","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[310,null,null,"酢酸",null,"Acetic Acid",null,"64-19-7","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[306,null,null,"カプリン酸",null,"Caprylic Acid",null,"124-07-2","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[318,null,null,"パルミチン酸",null,"Palmitic Acid",null,"57-10-3","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[312,null,null,"ステアリン酸",null,"Stearic Acid",null,"57-11-4","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[316,null,null,"動植物油脂肪酸およびその２量体",null,"Animal and vegetable oil fatty acid and its dimer",null,"57-10-3\n57-11-4\n60-33-3\n112-80-1\n61788-89-4\n 等","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[308,null,null,"ヘット酸",null,"Chlorendic Acid",null,"115-28-6","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[323,null,null,"ヘキサクロルエンドメチレンテトラヒドロ無水フタル酸",null,"Chlorendic anhydride",null,"115-27-5","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[null,null,null,"3.    酸類（その他）"]
[333,null,null,"ロジン",null,"Rosin",null,"8050-09-7","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[315,null,null,"ジメチルテレフタレート",null,"Dimethyl Terephthalate",null,"120-61-6","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[331,null,null,"ロジン－無水マレイン酸付加物",null,"Rosin, maleated",null,"8050-28-0","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[null,null,null,"4.    アルコール類"]
[338,null,null,"エチレングリコール",null,"Ethylene Glycol",null,"107-21-1","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[360,null,null,"プロピレングリコール",null,"Propylene Glycol ",null,"57-55-6","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[342,null,null,"ジエチレングリコール",null,"Diethylene Glycol",null,"111-46-6","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[345,null,null,"ジプロピレングリコール",null,"Dipropylene Glycol ",null,"110-98-5, 25265-71-8","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[355,null,null,"ネオペンチルグリコール",null,"Neopentylglycol",null,"126-30-7","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[358,null,null,"１，３ブタンジオール",null,"1,3-Butanediol",null,"107-88-0","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[359,null,null,"１，４ブタンジオール",null,"1,4-Butanediol",null,"110-63-4","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[362,null,null,"１，６ヘキサンジオール",null,"1,6-Hexanediol",null,"629-11-8","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[356,null,null,"水素化ビスフェノールA",null,"Hydrogenated Bisphenol -A",null,"80-04-6\n13804-54-1\n13804-57-4\n13804-58-5","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[339,null,null,"ビスフェノールA ＥＯ付加物",null,"Bisphenol A ethoxylate ",null,"32492-61-8","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[357,null,null,"ビスフェノールA ＰＯ付加物",null,"Bisphenol A bis(2-hydroxypropyl) ether",null,"116-37-0","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[364,null,null,"ポリエチレングリコール",null,"Polyethylene Glycol",null,"25322-68-3","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[365,null,null,"ポリプロピレングリコール",null,"Polypropylene glycol ",null,"25322-69-4","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[353,null,null,"トリメチロールプロパン",null,"Trimethylolpropane",null,"77-99-6","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[349,null,null,"トリエチレングリコール",null,"Triethylene Glycol",null,"112-27-6","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[341,null,null,"グリセリン",null,"Glycerol",null,"56-81-5","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[366,null,null,"マニトール",null,"Mannitol",null,"69-65-8,\n643-01-6,\n133-43-7","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[363,null,null,"ペンタエリスリトール",null,"Pentaerythritol",null,"115-77-5","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[351,null,null,"２，２，４－トリメチル－１，３－ペンタンジオール",null,"2,2,4-Trimethyl-1,3-pentanediol",null,"144-19-4","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[347,null,null,"ソルビトール",null,"Sorbitol",null,"50-70-4","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[352,null,null,"トリメチロールエタン",null,"Trimethylolethane",null,"77-85-0","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[350,null,null,"トリシクロデカンジメタノール",null,"Tricyclodecanedimethanol",null,"26896-48-0","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[346,null,null,"ネオペンチルアルコール",null,"2,2-Dimethyl-1-propanol ",null,"75-84-3","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[340,null,null,"オクチルアルコール",null,"1-Octanol",null,"111-87-5","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[348,null,null,"デシルアルコール",null,"1-Decanol",null,"112-30-1","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[335,null,null,"イソデシルアルコール",null,"Isodecyl Alcohol ",null,"25339-17-7","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[354,null,null,"トリメチロールプロパンジアリルエーテル",null,"Trimethylolpropanediallylether ",null,"682-09-7","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[337,null,null,"２－エチルヘキシルアルコール",null,"2-Ethyl-1-hexanol",null,"104-76-7","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[343,null,null,"ジエチレングリコールモノブチルエーテル",null,"Diethylene glycol monobutyl ether",null,"112-34-5","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[368,null,null,"α－メチルグリコシド",null,"Tetrabromobisphenol A bis(2-hydroxyethyl ether)",null,"4162-45-2","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[336,null,null,"２－エチル－２ーブチル－１,３－プロパンジオール","2-エチル-2-ブチル-1,3-プロパンジオール","2-Butyl-2-ethyl-1,3-propanediol",null,"0000115-84-4","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[367,null,null,"ヘキサヒドロ無水フタル酸","無水 1,2-シクロヘキサンジカルボン酸","Hexahydro phtalic acid anhydride",null,"0000085-42-7","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[344,null,null,"１，4ーシクロヘキサンジメタノール","1,4-シクロヘキサンジメタノール","1,4-cyclohexanedimethanol",null,"0000105-08-8","○","○","○","ー","○","Ⅲ",1]
[361,null,null,"１，２－プロパンジオール","CASと名称が異なる","1,​2-​propanediol ",null,"0000504-63-2","○","○","○","ー","○","Ⅲ",1]
[369,null,null,"２－メチル－１，３－プロパンジオール","2-メチル-1,3-プロパンジオール"," 2-​methyl-​1,​3-​propanediol",null,"0002163-42-0","○","○","○","ー","○","Ⅲ",1]
[null,null,null,"5.    エポキシ化合物"]
[376,null,null,"ビスフェノールA型エポキシ樹脂",null,"Bisphenol-A type Epoxy Resin",null,"1675-54-3","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[372,null,null,"フェノールノボラック型エポキシ樹脂（フェノールホルムアルデヒド縮合物-エピクロルヒドリン）",null,"Phenol Novolac type Epoxy Resin",null,"977103-59-5\n9003-36-5\n58421-55-9","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[378,null,null,"プロピレンオキサイド",null,"Propylene Oxide",null,"75-56-9","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[377,null,null,"グリシジルメタアクリレート",null,"Glycidyl Methacrylate",null,"106-91-2","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[371,null,null,"アリルグリシジルエーテル",null,"Allyl Glycidyl Ether",null,"106-92-3","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[null,null,null,"6.    その他"]
[375,null,null,"ビスフェノールA",null,"Bisphenol-A",null,"80-05-7","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[374,null,null,"ビスフェノールS",null,"Bisphenol-S",null,"80-09-1","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[373,null,null,"ジシクロペンタジエン",null,"Dicyclopentadiene",null,"77-73-6","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[null,null,null,"7.    架橋剤"]
[390,null,null,"スチレン",null,"Styrene",null,"100-42-5","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[408,null,null,"ビニルトルエン",null,"Vinyltoluene",null,"25013-15-4","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[409,null,null,"α－メチルスチレン",null,"α-Methylstyrene",null,"98-83-9","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[407,null,null,"メタクリル酸メチル",null,"Methyl Methacrylate",null,"80-62-6","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[387,null,null,"酢酸ビニル",null,"Vinyl Acetate ",null,"108-05-4","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[389,null,null,"ジビニルベンゼン",null,"Divinylbenzene",null,"1321-74-0","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[393,null,null,"Ｎ－ビニルピロリドン",null,"N-vinyl-2-pyrrolidone",null," 88-12-0","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[410,null,null,"パラメチルスチレン",null,"4-Methylstyrene",null,"622-97-9","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[394,null,null,"ジアリルフタレート",null,"Diallyl Phthalate",null,"131-17-9","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[386,null,null,"トリアリルイソシアヌレート",null,"Triallyl Isocyanurate",null,"1025-15-6","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[388,null,null,"トリアリルシアヌレート",null,"Triallyl Cyanurate",null,"101-37-1","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[395,null,null,"マレイン酸アリルエステル",null,"Diallyl Maleate",null,"999-21-3","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[396,null,null,"メタクリル酸アリルエステル",null,"Allyl Methacrylate",null,"96-05-9","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[382,null,null,"２－ヒドロキシエチルアクリレート",null,"2-Hydroxyethyl Acrylate",null,"818-61-1","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[385,null,null,"メチルアクリレート",null,"Methyl Acrylate",null,"96-33-3","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[380,null,null,"エチルアクリレート",null,"Ethyl Acrylate",null,"140-88-5","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[384,null,null,"プロピルアクリレート",null,"n-Propyl acrylate",null,"925-60-0","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[383,null,null,"ブチルアクリレート",null,"Butyl Acrylate",null,"141-32-2","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[398,null,null,"エチルメタクリレート",null,"Ethyl Methacrylate",null,"97-63-2","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[405,null,null,"プロピルメタクリレート",null,"Propyl methacrylate",null,"2210-28-8","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[404,null,null,"ブチルメタクリレート",null,"Butyl Methacrylate",null,"97-88-1","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[381,null,null,"２－エチルヘキシルアクリレート",null,"2-Ethylhexyl Acrylate ",null,"103-11-7","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[402,null,null,"２－ヒドロキシエチルメタクリレート",null,"2-Hydroxyethyl Methacrylate",null,"868-77-9","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[406,null,null,"ベンジルメタクリレート",null,"Benzyl Methacrylate ",null,"2495-37-6","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[403,null,null,"フェノキシエチルメタクリレート",null,"2-Phenoxyethyl Methacrylate",null,"10595-06-9","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[397,null,null,"イソボルニルメタクリレート",null,"Isobornyl methacrylate ",null,"7534-94-3","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[399,null,null,"ジシクロペンテニルオキシエチルメタクリレート",null,"Dicyclopentenyloxyethyl methacrylate ",null,"68586-19-6","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[392,null,null,"ネオペンチルグリコールジメタクリレート",null,"Neopentyl Glycol Dimethacrylate",null,"1985-51-9","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[400,null,null,"エチレングリコールジメタクリレート",null,"Etylene glycol dimethacrylate",null,"97-90-5","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[401,null,null,"ジエチレングリコールジメタクリレート",null,"Dietylene glycol dimethacrylate",null,"2538-84-1","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[391,null,null,"トリメチロールプロパントリメタクリレート",null,"Trimethylolpropane Trimethacrylate",null,"3290-92-4","○","○","○","○","○","Ⅲ",1,"乳・乳製品、酒類の使用可能温度はⅠ"]
[]
[null,null,"６８．エチレン・メタクリル酸グリシジル共重合体"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,"ー",null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[109,null,1,"エチレン・メタクリル酸グリシジル共重合","エチレン・メタクリル酸 グリシジル共重合体","Poly(ethylene-co-glycidyl methacrylate) \n（ethylene：50wt% or more）",null,"0026061-90-5","○","○","○","ー","○","Ⅱ",2,"エチレンはポリマー構成成分に対して50重量%以上"]
[]
[null,null,"６９．エポキシ樹脂の架橋体",null,"架橋エポキシポリマー"]
["整理番号","No.",null,"使用可能ポリマー","ー","英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,"ー",null,null,null,"酸性","油性及び脂肪性","乳・\n乳製品","酒類","その他"]
[null,1,null,"以下の1種類以上のエポキシ樹脂を以下のポリアミド樹脂及び／又は架橋反応剤で架橋したエポキシ樹脂の架橋体","ー","Epoxy resin crosslinked product obtained by crosslinking epoxy resin with any polyamide resin and/or crosslinking reaction agent.",null,null,"○","○","○","○","○","Ⅲ",1]
[null,"エポキシ樹脂"]
[null,"(i)",null,"次の1種又は２種以上のフェノール類とエピクロロヒドリン、又は（ⅱ）のエポキシ樹脂との反応により得られるエポキシ樹脂","ー","Epoxy resin by reaction of one or more of the following phenols with epichlorohydrin or (ii) epoxy resin　"]
[125,null,"①","ビスフェノールＡ","ビスフェノールＡ","Bisphenol A",null,"0000080-05-7"]
[126,null,"②","ビスフェノールＢ","ビスフェノールＢ","Bispenol B",null,"0000077-40-7"]
[127,null,"③","ビスフェノールＦ","ビスフェノールＦ","Bisphenol F",null,"0000620-92-8\n0001333-16-0"]
[122,null,"④","テトラメチルビスフェノールＦ","3,3',5,5'-テトラメチルビスフェノールＦ","Tetrametyl Bisphenol F",null,"0005384-21-4"]
[123,null,"⑤","フェノールノボラック樹脂","フェノール・ホルムアルデヒド共重合体（ノボラック）","Phenol novlac resin",null,"0009003-35-4"]
[124,null,"⑥","オルソクレゾールノボラック樹脂","ホルムアルデヒド・2-メチルフェノール共重合体（ノボラック）","o-cresol novolac resin",null,"0025053-96-7"]
[128,null,"⑦","フェノール","フェノール","phenol",null,"0000108-95-2"]
[129,null,"⑧","p-ターシャリーブチルフェノール","4-t-ブチルフェノール","P-tert-butylphenol",null,"0000098-54-4"]
[130,null,"⑨","p-セカンダリ-ブチルフェノール","4-sec-ブチルフェノール","P-sec-butylphenol",null,"0000099-71-8"]
[134,"(ii)","①","ビスフェノールＡ型エポキシ樹脂","エピクロルヒドリン・ビスフェノールＡ共重合体","Bisphenol A type epoxy resin",null,"0025068-38-6 0025036-25-3 0020232-24-0  0001675-54-3　0025068-38-6　0025085-99-8"]
[132,null,"②","ビスフェノールＢ型エポキシ樹脂","エピクロルヒドリン・ビスフェノールＢ共重合体","Bisphenol B type epoxy resin",null,"0009003-88-7"]
[133,null,"③","ビスフェノールＦ型エポキシ樹脂","エピクロルヒドリン・ビスフェノールＦ共重合体","Bisphenol F type epoxy resin",null,"0058421-55-9"]
[131,"　","④","テトラメチルビスフェノールＦ型エポキシ樹脂","エピクロルヒドリン・3,3',5,5'-テトラメチルビスフェノールＦ共重合体","Tetramethyl bisphenol F type epoxy resin",null,"0113693-69-9"]
[135,"　","⑤","フェノールノボラック型エポキシ樹脂","エピクロルヒドリン・フェノール・ホルムアルデヒド共重合体","Phenol novlac type epoxy resin",null,"0009003-36-5\n0028064-14-4"]
[139,"　","⑥","オルソクレゾールノボラック型エポキシ樹脂","エピクロルヒドリン・ホルムアルデヒド・2-メチルフェノール共重合体（ノボラック）","o-Cresol novolac type epoxy resin",null,"0029690-82-2"]
[136,null,"⑦","フェニルグリシジルエーテル","グリシジル フェニル エーテル","Phenyl glycidyl ether",null,"0000122-60-1"]
[137,null,"⑧","P-ターシャリーブチルフェニルグリシジルエーテル","グリシジル 4-t-ブチルフェニル エーテル","P-tert-butylphenyl 1-(2,3-epoxy)propyl ether",null,"0003101-60-8"]
[138,null,"⑨","p-セカンダリーブチルフェノールグリシジルエーテル","グリシジル 4-sec-ブチルフェニル エーテル","2-[(2-butylphenoxy)methyl]oxirane",null,"0029756-52-3"]
[null,"(iii)",null,"以下の1種又は2種以上のアルコール類とエピクロロヒドリンとの反応により得られるエポキシ樹脂","ー","Epoxy resin by reaction of one or more of the following alcohols （ｂ）with epichlorohydrin "]
[150,null,"①","ネオペンチルグリコール","ネオペンチルグリコール","Neopenthyl Glycol",null,"0000126-30-7"]
[153,null,"②","1，6ヘキサンジオール","1,6-ヘキサンジオール","1.6-Hexanediol",null,"0000629-11-8"]
[149,null,"③","トリメチロールプロパン","トリメチロールプロパン","Trimetylolpropane",null,"0000077-99-6"]
[141,null,"④","アルキル(C12-14)アルコール","アルキルアルコール（C12-14）","Alkil(C12-14)Alcohol",null,"0009002-92-0"]
[147,null,"⑤","水添ビスフェノールＡ","水素化処理されたビスフェノールＡ","Hydrogenated Bisphenol A",null,"0101320-77-8"]
[154,null,"⑥","ポリプロピレングリコール","プロピレングリコール単独重合体（PO≥4）","Polypropyleneglycol,",null,"0025322-69-4"]
[144,null,"⑦","ポリエチレングリコール","エチレングリコール単独重合体（EO≥4）","Polyetyleneglycol",null,"0025322-68-3"]
[143,null,"⑧","エチレングリコール","エチレングリコール","Ethyleneglycol",null,"?107-214-1"]
[145,null,"⓽","グリセロール","グリセロール","Glycerol",null,"0025618-55-7"]
[152,null,"⓾","1,4ブタンジオ-ル","1,4-ブタンジオール","1,4-Butanediol",null,"0000110-63-4"]
[151,null,"⑪","ブタノール","ブタノール","Butanol",null,"0000071-36-3"]
[146,null,"⑫","ジエチレングリコール","ジエチレングリコール","Dietylene glycol",null,"0000111-46-4"]
[142,null,"⑬","イソノナノール","アルキルアルコール（C9）","Isononanol",null,"0027458-94-2"]
[155,null,"⑭","ドデカノール","ドデカノール","Dodecanol",null,"0000112-30-1"]
[148,null,"⑮","トリデカノール","トリデカノール"," Toridecanol",null,"0000112-70-9"]
[null,"(iv)",null,"アルコールグリシジルエーテル型エポキシ樹脂",null,"Alcohol glycidyl ether type epoxy resin"]
[166,null,"①","ネオペンチルグリコールジグリシジルエーテル","ネオペンチルグリコールのジグリシジルエーテル","Neopenthyl glycol diglycidyl ether",null,"0017557-23-2\n0034629-78-2"]
[168,null,"②","1，6ヘキサンジオールジグリシジルエーテル","1,6-ヘキサンジオールのジグリシジルエーテル","1,6-hexanediol digltcidyl ether",null,"0016096-31-4"]
[165,null,"③","トリメチロ－ルプロパントリグリシジルエーテル","トリメチロ－ルプロパンのトリグリシジルエーテル","Trimetyilpropane triglycidyl ether",null,"0030499-70-8"]
[159,null,"④","アルキル(C12-14)アルコールグリシジルエーテル","アルキルアルコール（C12-14）のグリシジルエーテル","Alkyl(C12-14) glycidyl ether",null,"0068609-97-2"]
[164,null,"⑤","水添ビスフェノールＡジグリシジルエーテル","水素化処理されたビスフェノールＡのジグリシジルエーテル","Hydrogenated bisphenol A diglycidyl eter",null,"0030583-72-3"]
[170,null,"⑥","ポリプロピレングリコールジグリシジルエーテル","ポリプロピレングリコールのジグリシジルエーテル","Polypropireneglycol diglycidyl ether",null,"0026142-30-3"]
[169,null,"⑦","ポリエチレングリコールジグリシジルエーテル","ポリエチレングリコールのジグリシジルエーテル","Polyethyleneglycol diglycidyl ether",null,"0072207-80-8"]
[160,null,"⑧","エチレングリコールジグリシジルエーテル","エチレングリコールのジグリシジルエーテル","Ethyleneglycol diglycidyl ether",null,"0002224-15-9"]
[162,null,"⑨","ポリグリセロールポリグリシジルエーテル","ポリグリセロールのポリグリシジルエーテル","polyglycerol polyglycidyl ether",null,"0027043-36-3\n0118549-88-5",null,null,null,null,null,null,null,"最大使用量：100㎎/㎡\n\n"]
[167,null,"⓾","1,4-ブタンジオールジグリシジルエーテル","1,4-ブタンジオールのジグリシジルエーテル","1,4-Butanediol diglycidyl ether",null,"0002425-79-8"]
[161,null,"⑪","ブチルグリシジルエーテル","グリシジル ブチル エーテル","butyl glycidyl ether",null,"0002426-08-6"]
[163,null,"⑫","ジエチレングリコールジグリシジルエーテル","ジエチレングリコールのジグリシジルエーテル","Dietyleneglicol diglycidyl ether",null,"0004206-61-5"]
[157,null,"⑬","［（アルキル（Ｃ＝１０～１６）オキシ）メチル］オキシラン","アルキル グリシジル エーテル（C10-16）","[(C10-16-Alkyloxy)methyl]oxirane",null,"0068081-84-5"]
[158,null,"⑭","２－［（アルキル（Ｃ＝１２～１３）オキシ）メチル］オキシラン","アルキル グリシジル エーテル（C12、13）","2-[(Alkyl(C=12-13)oxy)methyl]oxirane",null,"0120547-52-6"]
[null,"(v)",null,"以下の酸類とエピクロロヒドリンとの反応により得られるエポキシ樹脂","ー","Epoxy resin by reaction of the following acids (c) with epichlorohydrin"]
[172,null,"①","ダイマー酸","二量化処理された脂肪酸 (不飽和 C18)","Dimer acid ",null,"0061788-89-4　"]
[173,null,"②","ネオデカン酸","ネオデカン酸","Neodecan acid",null,"0026896-20-8"]
[null,"(vi)",null,"グリシジルエステル型エポキシ樹脂",null,"Glycidyl ester type epoxy resin"]
[175,null,"①","ダイマー酸ジグリシジルエステル","エピクロロヒドリン・二量化処理された脂肪酸 (不飽和 C18）共重合体","Dimer acid diglycidyl ester",null,"0068475-94-5"]
[176,null,"②","ネオデカン酸グリシジルエステル","ネオデカン酸 グリシジル","Neodecanic acid　glycidyl ester",null,"0026761-45-5"]
[null,"(vii)",null,"以下のアミン類とエピクロロヒドリンとの反応により得られるエポキシ樹脂","ー","Glycidyl amine by reaction of the amines with epichlorohydrin "]
[180,null,"①","１,３-ビス（アミノメチル）シクロヘキサン","1,3-ビス(アミノメチル)シクロヘキサン","1.3-Bis(aminomethyl)cyclohexane",null,"0002579-20-6"]
[179,null,"②","メタキシリレンジアミン","1,3-キシレンジアミン","m-Xylylendiamine",null,"0001477-55-0"]
[178,null,"③","４メトキシアニリン","4-アミノアニソール","４-methoxyaniline",null,"0000104-94-9"]
[null,"(viii)",null,"グリシジルアミン型エポキシ樹脂",null,"Glycidyl amine type epoxy resin"]
[184,null,"①","１，３－ビス（Ｎ，Ｎ－ジグリシジルアミノメチル）シクロヘキサン","N,N,N',N-テトラグリシジル-1,3-ビス(アミノメチル)シクロヘキサン","1,3-bis(N,N-diglycidyl amino methyl) cyclohexane",null,"0065992-66-7"]
[183,null,"②","N,N,N',N'-テトラグリシジル,メタキシレンジアミン","N,N,N',N-テトラグリシジル-1,3-キシレンジアミン"," N,N,N',N'-tetraglycidyl,m-xylene diamine",null,"0063738-22-7"]
[182,null,"③","Ｎ，Ｎ－ビス（２，３－エポキシプロピル）－４－（２，３－エポキシプロポキシ）アニリン","グリシジル 4-(ジグリシジルアミノ)フェニル エーテル","N,N-Bis(2,3-epoxypropyl)-4-(2,3-epoxypropoxy)aniline",null,"0005026-74-4"]
[null,"(ix)",null,"過酸化法により得られるエポキシ樹脂",null,"Epoxy resin of peroxidation method"]
[186,null,"①","１，４－ビス［（オキシラン－２－イルメトキシ）メチル］シクロヘキサン","1,4-シクロヘキサンジメタノールのジグリシジルエーテル","1,4-Bis[(2,3-epoxypropoxy)ethyl]cyclohexane",null,"0014228-73-0"]
[null,"ポリアミド樹脂",null,null,"ー"]
[null,"(i)",null,"次の（ａ）（ｂ）（ｃ）の出発原料から得られるポリアミド（混合原料も含む）","ー","The polyamide (including the mixed raw material) obtained from the starting materials of the following (a), (b) and (c) "]
[189,null,"(a) ","酸","ー","Acids"]
[190,null,"(1)","アジピン酸","アジピン酸","Adipic.",null,"0000124-04-9"]
[191,null,"(2)","アゼライン酸","アゼライン酸","Azelaic.",null,"0000123-99-9"]
[192,null,"(3)","セバシン酸","セバシン酸","Sebacic.",null,"0000111-20-6"]
[193,null,"(4)","植物油から得られる脂肪酸","植物性油脂由来の脂肪酸","Vegetable oil acids",null,"0068955-98-6"]
[194,null,"(5)","植物油から得られる二量化脂肪酸","二量化処理された植物性油脂由来の脂肪酸","Vegetable oil acids with dimerization",null,"0061788-89-4"]
[195,null,"(b) ","アミン","ー"," Amines"]
[197,null,"(1)","ジエチレントリアミン","ジエチレントリアミン","Diethylenetriamine",null,"0000111-40-0"]
[198,null,"(2)","ジフェニルアミン","ジフェニルアミン","Diphenylamine",null,"0000122-39-4"]
[196,null,"(3)","エチレンジアミン","エチレンジアミン","Ethylenediamine",null,"0000107-15-3"]
[202,null,"(4)","ヘキサメチレンジアミン","ヘキサメチレンジアミン","Hexamethylenediamine",null,"0000124-09-4"]
[199,null,"(5)","テトラエチレンペンタミン","テトラエチレンペンタミン","Tetraethylene pentamine",null,"0000112-57-2"]
[200,null,"(6)","トリエチレンテトラミン","トリエチレンテトラミン","Triethylene tetramine",null,"0000112-24-3"]
[201,null,"(7)","ピペラジン","ピペラジン","piperazine",null,"0000110-85-0",null,null,null,null,null,null,null," "]
[203,null,"(c)","変性剤","ー","Denaturant"]
[204,null,"(1)","ε－カプロラクタム－（エチレン－エチルアクリレート）グラフトポリマー","アクリル酸エチル・エチレン・カプロラクタム共重合体","Epsilon-caprolactam-(ethylene-ethyl acrylate)graft polymer",null,"0025052-65-7"]
[205,null,"(2)","ジ（４－オクチルフェニル）アミン","4,4'-ジオクチルジフェニルアミンまたは4,4'-ビス(2,4,4-トリメチルペンチル)ジフェニルアミン","Bis(4-octylphenyl)amine",null,"0000101-67-7\n0068411-46-1",null,null,null,null,null,null,null," "]
[null,"(ii)",null,"その他のポリアミド樹脂","ー","Other polyamide resins"]
[null,null,"(１)","以下のアミンと二量化植物油から誘導されるポリアミド樹脂",null,"Polyamides derived from amines listed in following below with dimerized vegetable oils."]
[208,null,"①","シアノグアニジン (ジシアンジアミド）","シアノグアニジン","Cyanoguanidine　（Dicyandiamide)",null,"0000461-58-5"]
[207,null,"②","Ｎ－オレイル－１，３－プロパンジアミン","N-オレイル-1,3-ジアミノプロパン","N-Oleyl-1,3-propanediamine with not more　than 10 percent by weight of　diethylaminoethanol.",null,"0007173-62-8"]
["削除15",null,"③","脂肪酸変性テトラエチレンペンタミン","脂肪酸の範囲不明\n脂肪酸とテトラエチレンペンタミンの反応生成物","Tetraethylenepentamine reacted with\nequimolar quantities of fatty acids.",null,"0977181-68-2"]
[null,"架橋反応剤"]
[235,null,"(1)","シアノグアニジン (ジシアンジアミド）","シアノグアニジン","Cyanoguanidine　（Dicyandiamide)",null,"0000461-58-5"]
[238,null,"(2)","ジエチレントリアミン","ジエチレントリアミン","Diethylenetriamine.",null,"0000111-40-0"]
[239,null,"(3)","ジフェニルアミン","ジフェニルアミン","Diphenylamine",null,"0000122-39-4"]
[223,null,"(4)","エチレンジアミン","エチレンジアミン","Ethylenediamine",null,"0000107-15-3"]
[226,null,"(5)","Ｎ－オレイル－１，３－プロパンジアミン","N-オレイル-1,3-ジアミノプロパン","N-Oleyl-1,3-propanediamine",null,"0007173-62-8"]
[245,null,"(6)","テトラエチレンペンタミン","テトラエチレンペンタミン","Tetraethylene pentamine",null,"0000112-57-2"]
["削除16",null,"(7)","脂肪酸変性テトラエチレンペンタミン","脂肪酸の範囲不明\n脂肪酸とテトラエチレンペンタミンの反応生成物","Tetraethylenepentamine reacted with\nequimolar quantities of fatty acids.",null,"0977181-68-2"]
[250,null,"(8)","トリエチレンテトラミン","トリエチレンテトラミン","Triethylene tetramine",null,"0000112-24-3"]
[242,null,-9,"ジメチルアミン－２－メチル－１－プロパノール","要構造確認\nN,N-ジメチル-2-アミノ-2-メチル-1-プロパノール","Dimethylamine-2-methyl-1-propanol",null,"0977176-55-8"]
[278,null,-10,"メチルプロパノールアミン","N-メチル-3-アミノプロパノール","Methylpropanolamine",null,"0042055-15-2"]
[247,null,-11,"トリエタノールアミン","トリエタノールアミン","Triethanolamine",null,"0000102-71-6"]
[276,null,-12,"無水フタル酸","無水フタル酸","Phthalic anhydride",null,"0000085-44-9"]
[275,null,-13,"無水トリメリット酸","無水トリメリット酸","Trimellitic anhydride",null,"0000552-30-7"]
[216,null,-14,"2ーアミノー２－メチルプロパノール","2-アミノ-2-メチル-1-プロパノール","2-amino-2-methyipropanol",null,"0000124-68-5"]
[261,null,-15,"ジイソプロパノールアミン","ビス(2-プロパノール)アミン","Diisopropanolamine",null,"0000110-97-4"]
[222,null,-16,"２－エチル－４－メチルイミダゾール","2-エチル-4-メチルイミダゾール","2-Ethyl-4-methylimidazole",null,"0000931-36-2"]
[248,null,-17,"トリエチルアミン","トリエチルアミン","Triethylamine",null,"0000121-44-8"]
[243,null,-18,"ジメチルアミン","ジメチルアミン","Dimethylamine",null,"0000124-40-3"]
[262,null,-19,"２－フェニルイミダゾール","2-フェニルイミダゾール","2-Phenylimidazole",null,"0000670-96-2"]
[264,null,-20,"フェノール","フェノール","Phenol",null,"0000108-95-2"]
[220,null,-21,"イソホロンジアミン","イソホロンジアミン","Isophoronediamine",null,"0002855-13-2"]
[218,null,-22,"トリス（２，3-エポキシプロピル）イソシアヌレート","イソシアヌル酸 トリグリシジル","1,3,5-Triglycidyl isocyanurate",null,"0002451-62-9"]
[237,null,-23,"３－ジエチルアミノプロピルアミン","N,N-ジエチル-1,3-プロパンジアミン","3-Diethylaminopropylamine",null,"0000104-78-9"]
[280,null,-24,"４，４’－メチレンジアニリン","4,4'-メチレンジアニリン","4,4′-Methylenedianiline",null,"0000101-77-9"]
[272,null,-25,"3-ペンタデセニルフェノール混合物","名称とCASが異なる","3-Pentadecenyl phenol mixture",null,"0068413-28-5"]
[212,null,-26,"ポリエチレンポリアミン",null,"Polyethylenepolyamine",null,"0068131-73-7"]
[217,null,-27,"安息香酸","安息香酸","Benzoic acid",null,"0000065-85-0"]
[274,null,-28,"無水コハク酸","無水コハク酸","Succinic anhydride",null,"0000108-30-5"]
[252,null,-29,"２，４，６－トリジメチルアミノメチルフェノール","2,4,6-トリス[(ジメチルアミノ)メチル]フェノール","2,4,6-Tris[(dimethylamino)methyl]phenol",null,"0000090-72-2",null,null,null,null,null,null,null,"　"]
[258,null,-30,"ビス（ジメチルアミノメチル）フェノール","ビス[(ジメチルアミノ)メチル]フェノール","Bis[(dimethylamino)methyl]phenol",null,"0071074-89-0",null,null,null,null,null,null,null,"　"]
[211,"　",-31,"エチレンイミン","アジリジン","Ethyleneimine",null,"0000151-56-4"]
[246,null,-32,"Ｎ，Ｎ，Ｎ’，Ｎ’‐テトラキス（２‐ヒドロキシプロピル）アジポアミド","N,N,N',N'-テトラキス(2-ヒドロキシプロピル)アジピン酸アミド","N,N,N',N'-tetrakis(2-hydroxypropyl)adipamide",null,"0057843–53–5"]
[279,null,-33,"クレゾール","クレゾール","Cresol",null,"0001319-77-8"]
[254,null,-34,"ノニルフェノール","ノニルフェノール","Nonylphenol",null,"0025154-52-3"]
[266,null,-35,"p-ターシャリーブチルフェノール","4-t-ブチルフェノール","p-tert-ｂutylphenol",null,"0000098-54-4"]
[269,null,-36,"ヘキサメチレンテトラミンで変性されたフェノール樹脂",null,"Phenol resin modified with hexamethylenetetramine"]
[232,null,-37,"ホルムアルデヒド、ｍ－キシリレンジアミン、及びフェノールの重縮合物","1,3-キシレンジアミン・フェノール・ホルムアルデヒド共重合体","Formaldehyde, polymer with 1,3-benzenedimethanamine and phenol ",null,"0057214-10-5"]
[228,"　",-38,"メタキシリレンジアミン","1,3-キシレンジアミン","m-Xylylendiamine",null,"0001477-55-0"]
[265,null,-39,"ジアミノジフェニルメタン・フェノールホルムアルデヒド重縮合物","フェノール・ホルムアルデヒド・4,4'-メチレンジアニリン共重合体","Polycondensate of 4,4'diaminodiphenylmethane and phenolformaldehyde",null,"0051601-28-6"]
[283,null,-40,"4,4'－メチレンビス（2-メチルシクロヘキシルアミン）","4,4'-メチレンビス(2-メチルシクロヘキシルアミン)","4,4'-Methylenebis(2-methylcyclohexylamine)",null,"0006864-37-5"]
[267,null,-41,"フルフリルアルコール","フルフリルアルコール","Furfuryl Alcohol",null,"0000098-00-0"]
[213,null,-42,"アセチルサリチル酸","アセチルサリチル酸","Acetylsalicylic acid",null,"0000050-78-2"]
[253,null,-43,"トリメチルヘキサメチレンジアミン","トリメチル-1,6-ヘキサンジアミン","Trimethihexamethylenediamin",null,"0025513-64-8"]
[244,null,-44,"アニリン/ホルムアルデヒドポリマー水素化物","水素化処理されたアニリン・ホルムアルデヒド共重合体","Formaidehyde, polymaer with benzeneamine, hydrogenated",null,"0135108-88-2"]
[282,null,-45,"4,4'-メチレンビス（シクロヘキシルアミン）","4,4'-メチレンビス(シクロヘキサンアミン)","4,4'-Methylen bis(2-methylcyclohexylamine)",null,"0001761-71-3"]
[215,null,-46,"1-(2-アミノエチル）ピペラジン","N-(2-アミノエチル)ピペラジン","N-Aminoethylpiperajine",null,"0000140-31-8"]
[234,null,-47,"サリチル酸","サリチル酸","Salicylic acid",null,"0000069-72-7"]
[270,null,-48,"ベンジルアルコール","ベンジルアルコール","Benzyl alcohol",null,"0000100-51-6"]
[233,null,-49,"牛脂アルキルトリメチレンジアミン","N-牛脂アルキル-トリメチレンジアミン","Diamine RRT",null,"0061791-55-7"]
[273,null,-50,"α-[2-(アミノメチル）エチル]-ω-(２－アミノメチルエトキシ）ポリ[オキシ（メチルエチレン）]","ポリプロピレングリコールのビス(2-アミノプロピル)エーテル","Alpha-[2-(aminomethyl)ethyl]-omega-(2-aminomethyleoxy)poly[oxy(methylethylenme)]",null,"0009046-10-0"]
[227,null,-51,"カシューナッツオイル","カシューナッツ油","Cashew nut oil",null,"0008007-24-7"]
[255,null,-52,"１,３-ビス（アミノメチル）シクロヘキサン","1,3-ビス(アミノメチル)シクロヘキサン","1.3-Bis(aminomethyl)cyclohexane",null,"0002579-20-6"]
[268,null,-53,"エチルトリス[アミノポリプロピルオキシ（n=～3)メチル]メタン","プロポキシル化処理されたトリメチロールプロパンのトリス(2-アミノエチル)エーテル","Ethyl tris[amonopolypropyloxy(n=--3)methyl]methane",null,"0039423-51-3"]
[259,null,-54,"ビスフェノールＡ型エポキシ樹脂とエチルトリス[アミノポリプロピルオキシ（ｎ＝～３）メチル]メタンの反応物","ビスフェノールAのジグリシジルエーテル・プロポキシル化処理されたトリメチロールプロパンのトリス(2-アミノエチル)エーテル共重合体","Reaction of bisphenol A-epichlorohydrin and Ethyl tris[amonopolypropyloxy(n=--3)methyl]methane",null,"0070548-69-5"]
[214,null,-55,"ホルムアルデヒドとアニリンの重合物","アニリン・ホルムアルデヒド共重合体","Formaldehyde, polymer with benzenamine",null,"0025214-70-4"]
[281,null,-56,"メチレンジアニリンとビスフェノールA型エポキシ樹脂の反応物","4,4'-メチレンジアニリン・ビスフェノールAのジグリシジルエーテル共重合体","Methylenedianiline, bisphenol A, diglycidyl ether adduct",null,"0026376-58-9"]
[225,null,-57,"（Ｚ)-９-オクタデセン-１-アミン","オレイルアミン","9-Octadecen-1-amine, (9Z)-",null,"0000112-90-3"]
[210,null,-58,"キシリレンジアミン・アクリロニトリル反応物","アクリロニトリルとキシレンジアミンの反応生成物","Benzenedimethanamine, N-(2-cyanoethyl) derivs.",null,"0073050-11-0"]
[219,null,-59,"１－イソブチル－２－メチルイミダゾール","1-イソブチル-2-メチルイミダゾール","1-isobuthyl-2-methylimidazole",null,"0116680-33-2"]
[249,null,-60,"トリエチレンジアミン","トリエチレンジアミン","Triethylenediamine",null,"0000280-57-9"]
[277,null,-61,"メチルヘキサヒドロ無水フタル酸","無水メチルシクロヘキサン-1,2-ジカルボン酸","Methylhexahydrophthalic anhydride",null,"0025550-51-0"]
[236,null,-62,"ジエチルトルエンジアミン","ジエチルトルエンジアミン","Diethyltoluenediamine",null,"0068479-98-1"]
[271,null,-63,"Ｎ－ベンジルエチレンジアミン","N-ベンジル-エチレンジアミン","N-benzylethylenediamine",null,"0004152-09-4"]
[241,null,-64,"Ｎ，Ｎ－ジベンジルエチレンジアミン","N,N-ジベンジル-エチレンジアミン","1,2-Ethanediamine, N,N-bis(phenylmethyl)-",null,"0014165-27-6"]
[260,null,-65,"２,２-ビス(２-ヒドロキシ-３-メルカプトプロポキシフェニル)プロパン","ビスフェノールAのビス(2-ヒドロキシ-3-メルカプトプロピル)エーテル","1,1'-[isopropylidenebis(p-phenyleneoxy)]bis[3-mercaptopropan-2-ol]",null,"0029953-09-1"]
[251,null,-66,"液状ジエトキシメタンポリサルファイドポリマー","1,2,3-トリクロロプロパン・ジ(2-クロロエトキシ)メタン・多硫化ナトリウム共重合体","Propane, 1,2,3-trichloro-, polymer with 1,1'-[methylenebis(oxy)]bis[2-chloroethane] and sodium sulfide (Na2(Sx)), reduced",null,"0068611-50-7"]
[224,null,-67,"２－（クロロメチル）オキシラン・シクロヘキサン－１，３－ジイルビス（メタンアミン）・４，４’－（イソプロピリデン）ジフェノール重合物","エピクロルヒドリン・1,3-ビス(アミノメチル)シクロヘキサン・ビスフェノールA共重合体","Polymer of 2-(chloromethyl)oxirane / cyclohexane-1,3-diylbis(methanamine) / 4,4'-(isopropylidene)diphenol",null,"0060112-98-3"]
[221,null,-68,"３－（アミノメチル）－３，５，５－トリメチルシクロヘキサン－１－アミン・２－（クロロメチル）オキシラン・４，４’－プロパン－２，２－ジイルジフェノール重合物","イソホロンジアミン・エピクロルヒドリン・ビスフェノールA共重合体","Polymer of 3-(aminomethyl)-3,5,5-trimethylcyclohexan-1-amine / 2-(chloromethyl)oxirane / 4,4'-propane-2,2-diyldiphenol",null,"0038294-64-3"]
[231,null,-69,"メタキシリレンジアミンとスチレンの反応付加物","1,3-キシレンジアミンとスチレンの反応生成物","1,3-Benzenedimethanamine, N-(2-phenylethyl)derivs.",null,"0404362-22-7"]
[230,null,-70,"１，３－ビス（アミノメチル）ベンゼン・トリルグリシジルエーテル付加物","1,3-キシレンジアミンとグリシジル メチルフェニル エーテルの反応生成物","1,3-Benzenedimethanamine, reaction products with glycidyl tolyl ether",null,"0090194-04-0"]
[229,null,-71,"１，３－ビス（アミノメチル）ベンゼン・フェニルグリシジルエーテル付加物","1,3-キシレンジアミンとグリシジル フェニル エーテルの反応生成物","1,3-Benzenedimethanamine, reaction products with phenyl　glycidyl ether",null,"0090194-03-9"]
[256,null,-72,"１，３－ビス（アミノメチル）シクロヘキサン・フェニルグリシジルエーテル付加物","1,3-ビス(アミノメチル)シクロヘキサンとグリシジル フェニル エーテルの反応生成物","1,3-cyclohexanedimethanamine, reaction products with phenyl　glycidyl ether"]
[257,null,-73,"ビシクロ［２．２．１］ヘプタン－２，３－ジイルジメタンアミン","ビス(アミノメチル)ノルボルナン","Bicyclo[2.2.1]heptane-2,3-diyldimethanamine",null,"0056602-77-8"]
[263,null,-74,"フェニル尿素","N-フェニル尿素","Phenylurea",null,"0000064-10-8"]
[240,null,-75,"１，３－ジフェニル尿素","N,N-ジフェニル尿素","1,3-Diphenylurea",null,"0000102-07-8"]
[]
[null,null,"７０．ポリアクリルニトリル（PAN）"]
["整理番号",null,"No","使用可能ポリマー",null,"英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,"ー",null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[884,null,1,"アクリロニトリル・酢酸ビニル共重合物","アクリロニトリル・酢酸 ビニル共重合体","Poly(acrylonitrile-co-vinyl acetate)",null,"0024980-62-9","○","○","ー","○","○","Ⅱ",3]
[882,null,2,"アクリロニトリル・メタクリル酸・アクリル酸メチル共重合体","アクリル酸 メチル・アクリロニトリル・メタクリル酸共重合体","Polymer of acrylonitrile / methacrylic acid / methyl acrylate　copolymer",null,"0036905-44-9","○","○","○","○","○","I",3]
[883,null,3,"アクリロニトリル・アクリル酸メチル・メタリルスルホン酸ナトリウム共重合体","アクリル酸 メチル・アクリロニトリル・メタリルスルホン酸 ナトリウム共重合体","Polymer of acrylonitrile / Methyl acrylate /  Methallylsulfonic Acid Sodium Salt  copolymer",null,"0026658-88-8","○","○","○","○","○","Ⅱ",3]
[885,null,4,"アクリロニトリル単独重合体","アクリロニトリル単独重合体","Poly-acrylonitrile",null,"0025014-41-9","○","○","○","○","○","Ⅰ",1]
[]
[null,null,"７１．アクリル樹脂（ポリメタクリル酸メチルを除く）"]
["整理番号",null,"No","使用可能ポリマー","ー","英名",null,"CAS登録番号","使用可能食品",null,null,null,null,"使用可能温度\nⅠ. ～70℃  \nⅡ. ～100℃\nⅢ. 101℃～","区分","特記事項"]
[null,null,null,null,"ー",null,null,null,"酸性","油性及び脂肪性","乳・乳製品","酒類","その他"]
[50,null,1,"アクリル酸ブチル・スチレン共重合物","アクリル酸 ブチル・スチレン共重合体"," Butyl acrylate-styrene copolymer",null,"0025767-47-9","○","○","○","○","○","　II",3,"アクリル酸ブチルはポリマー構成成分に対して50重量%以上"]
[51,null,2,"アクリル酸ブチル・メタクリル酸メチル・スチレン共重合物","アクリル酸ブチル・メタクリル酸メチル・スチレン共重合体"," Butyl acrylate-methyl methacrylate-styrene copolymer",null,"0027136-15-8","○","○","○","○","○","II",3,"メタクリル酸メチルは、ポリマー構成成分に対して50重量％以下\nメタクリル酸メチルとアクリル酸ブチルの合計はポリマー構成成分に対して50重量％以上"]
[48,null,3,"メタクリル酸メチルとアクリル酸メチルとアクリル酸ブチルとスチレンのコポリマー","アクリル酸 ブチル・アクリル酸 メチル・スチレン・メタクリル酸 メチル共重合体","Copolymers of methyl methacrylate and methyl acrylate and butylacrylate with styrene.",null,"0051998-22-2","○","○","○","○","○","II",3,"メタクリル酸メチルは、ポリマー構成成分に対して50重量％以下\nメタクリル酸メチルとアクリル酸メチルとアクリル酸ブチルの合計は、ポリマー構成成分に対して50重量％以上"]
[52,null,4,"メタクリル酸メチル・メタクリル酸ブチル・アクリル酸ブチル共重合体","アクリル酸 ブチル・メタクリル酸 ブチル・メタクリル酸 メチル共重合体","2-Propenoic acid, 2-methyl-, butyl ester, polymer with butyl 2-propenoate and methyl 2-methyl-2-propenoate",null,"0025322-99-0","○","○","○","○","○","II",3,"メタクリル酸メチルは、ポリマー構成成分に対しての50重量％以上。"]
[49,null,5,"アクリロニトリル・アクリル酸ブチル・メタクリル酸メチル共重合体","アクリル酸 ブチル・アクリロニトリル・メタクリル酸 メチル共重合体","Acrylonitrile, butyl acrylate, methyl methacrylate polymer",null,"0027340-76-7","○","○","○","○","○","II",3,"アクリル酸ブチルは、ポリマー構成成分に対しての50重量％以上。"]
[47,null,6,"メタクリル酸メチル・アクリル酸ブチル・アクリル酸 2-エチルへキシル共重合体","アクリル酸 2-エチルへキシル・アクリル酸 ブチル・メタクリル酸 メチル共重合体","2-Propenoic acid, 2-methyl-, methyl ester, polymer with butyl 2-propenoate and 2-ethylhexyl 2-propenoate",null,"0031261-08-2","○","○","○","○","○","II",3,"アクリル酸ブチルは、ポリマー構成成分に対しての50重量％以上。"]
[53,null,7,"メタクリル酸メチル・アクリル酸ブチル共重合体","アクリル酸 ブチル・メタクリル酸 メチル共重合体","2-Propenoic acid, 2-methyl-, methyl ester, polymer with butyl 2-propenoate",null,"0025852-37-3","○","○","○","○","○","II",3,"アクリル酸ブチルは、ポリマー構成成分に対しての50重量％以上。"]